<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.37" y2="0" width="0" layer="20"/>
<wire x1="39.37" y1="0" x2="39.37" y2="6.985" width="0" layer="20"/>
<wire x1="39.37" y1="6.985" x2="30.48" y2="6.985" width="0" layer="20"/>
<wire x1="30.48" y1="6.985" x2="30.48" y2="29.845" width="0" layer="20"/>
<wire x1="30.48" y1="29.845" x2="39.37" y2="29.845" width="0" layer="20"/>
<wire x1="39.37" y1="29.845" x2="39.37" y2="36.83" width="0" layer="20"/>
<wire x1="39.37" y1="36.83" x2="0" y2="36.82" width="0" layer="20"/>
<wire x1="0" y1="36.82" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="2.54" drill="1.99898125" locked="yes"/>
<hole x="2.54" y="34.29" drill="1.99898125" locked="yes"/>
<hole x="36.83" y="4.445" drill="3.048"/>
<hole x="36.83" y="32.385" drill="3.048"/>
<text>RV-Project.Com
OLED Display Board
RevC     3/13/2019</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>Optional IIC Pullup Resistors</text>
<text>VCC</text>
<text>GND</text>
<text>A:VCC-GND-SCL-SDA
B:GND-VCC-SCL-SDA</text>
<text>VCC</text>
<text>GND</text>
<text>A:</text>
<text>B:</text>
<text>SCL</text>
<text>SDA</text>
<text>Display
Power</text>
</plain>
<libraries>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="ICSP_BOX">
</package>
</packages>
</library>
<library name="a-lib_Modules">
<packages>
<package name="096_OLED">
<description>128x64 and 128x32 displays
&lt;br&gt;SSD1306 Driver
&lt;br&gt;I2C</description>
</package>
</packages>
</library>
<library name="a-lib_SMD">
<description>All SMD Devices; Actives, Passives, Connectors</description>
<packages>
<package name="1206-RES">
</package>
<package name="SMD-JUMPER_3">
<description>Pad Size: 0.18"x0.06"&lt;br&gt;Resist remoted between pads for ease of solder bridge.</description>
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="USA_SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="a-lib_Modules" package="096_OLED" value="OLED_096_I2C_DISPLAY"/>
<element name="J1" library="a-lib_Connectors" package="ICSP_BOX" value=""/>
<element name="R1" library="a-lib_SMD" package="1206-RES" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a-lib_SMD" package="1206-RES" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="a-lib_SMD" package="SMD-JUMPER_3" value="M33PIN_JUMPER"/>
<element name="U$3" library="a-lib_SMD" package="SMD-JUMPER_3" value="M33PIN_JUMPER"/>
<element name="U$4" library="a-lib_Asthetics" package="USA_SMALL" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="J1" pad="VCC"/>
<contactref element="J1" pad="MOSI"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="SCL"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="SCK"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="SDA"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="MISO"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="RST"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="U$3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
