(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 46)
    (no_connects 0)
    (area 121.924999 92.924999 178.075001 111.075001)
    (thickness 1.6)
    (drawings 25)
    (tracks 121)
    (zones 0)
    (modules 26)
    (nets 14)
  )
  (page A4)
  (title_block
    (title "X-Y Endstop")
    (date 2017-11-09)
    (rev A)
    (comment 3 " CARLOS RUIZ")
    (comment 4 " MAKSIM ZOLIN")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.3 4.3)
    (pad_drill 4.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 +5V)
  (net 5 +3V3)
  (net 6 Y_SIG)
  (net 7 X_SIG)
  (net 8 "Net-(U1-Pad3)")
  (net 9 "Net-(U2-Pad3)")
  (net 10 "Net-(D1-Pad1)")
  (net 11 "Net-(D2-Pad1)")
  (net 12 "Net-(R1-Pad2)")
  (net 13 "Net-(R3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U2-Pad3)")
    (add_net X_SIG)
    (add_net Y_SIG)
  )
  (net_class power ""
    (clearance 0.2032)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module MZBOT:CT6EP103 (layer B.Cu) (tedit 5A4E788F)
    (at 155.4 107.6)
    (fp_text reference VR1 (at 0 -2.54) (layer B.SilkS))
    (fp_text value 10.0K (at 0 3.81) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 1.25) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(R1-Pad2)"))
    (pad 2 thru_hole circle (at -2.5 -1.25) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 2.5 -1.25) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 5 +3V3))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/CT6EP103.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_DIN965 locked (layer F.Cu) (tedit 5A050E53)
    (at 167 98.75)
    (descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
    (tags "mounting hole 4.3mm no annular m4 din965")
    (clearance 60)
    (attr virtual)
    (fp_text reference REF** (at 0 -4.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4_DIN965 (at 0 4.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask)
      (clearance 0.05))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_DIN965 locked (layer F.Cu) (tedit 5A050B87)
    (at 127.75 98.75)
    (descr "Mounting Hole 4.3mm, no annular, M4, DIN965")
    (tags "mounting hole 4.3mm no annular m4 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4_DIN965 (at 0 4.75) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module MZBOT:C_0603 (layer F.Cu) (tedit 5A04D107)
    (at 128.5722 105.9058)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -0.0722 -1.2058) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:1X4_CONN_L_RA (layer B.Cu) (tedit 5A4EEA55)
    (at 142.6 107.9 90)
    (fp_text reference J1 (at -0.3 6.35 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 6.858 7.62 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 3.81 90) (size 2.032 2.032) (drill 1.1684) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 1.27 90) (size 2.032 2.032) (drill 1.1684) (layers *.Cu *.Mask B.SilkS)
      (net 7 X_SIG))
    (pad 3 thru_hole circle (at 0 -1.27 90) (size 2.032 2.032) (drill 1.1684) (layers *.Cu *.Mask B.SilkS)
      (net 6 Y_SIG))
    (pad 4 thru_hole circle (at 0 -3.81 90) (size 2.032 2.032) (drill 1.1684) (layers *.Cu *.Mask B.SilkS)
      (net 4 +5V))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/1X4_CONN_L_RA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:R_0603 (layer F.Cu) (tedit 5A04D115)
    (at 128.508 108.0902)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -0.008 1.3098) (layer F.SilkS))
    (fp_text value 1.00K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 X_SIG))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:C_0603 (layer F.Cu) (tedit 5A4EEBE0)
    (at 149.2 107.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2 0.05 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:C_0603 (layer F.Cu) (tedit 5A4EEBF4)
    (at 149.1 100.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.2 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:C_0603 (layer F.Cu) (tedit 5A4EEC0A)
    (at 135.3 106.3 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.15 -0.05 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:C_0603 (layer F.Cu) (tedit 5A4EEC15)
    (at 135.3 98.4 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.1 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:R_0603 (layer F.Cu) (tedit 5A4EEBFA)
    (at 149.2 104.8 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 1.00K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:R_0603 (layer F.Cu) (tedit 5A4EEBDA)
    (at 150.7 107.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.05 0 270) (layer F.SilkS))
    (fp_text value 10.0k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:R_0603 (layer F.Cu) (tedit 5A04B8FA)
    (at 149.1 97.7 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.03 -1.17 90) (layer F.SilkS))
    (fp_text value 1.00K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad2)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:R_0603 (layer F.Cu) (tedit 5A4EEBF7)
    (at 150.7 100.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.85 0 270) (layer F.SilkS))
    (fp_text value 10.0k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:R_0603 (layer F.Cu) (tedit 5A4EEC3F)
    (at 173.6184 99.0224 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -0.0224 1.3684 270) (layer F.SilkS))
    (fp_text value 1.00K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 Y_SIG))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:SIP-3 locked (layer F.Cu) (tedit 5A04D0FD)
    (at 123.5 106.98 270)
    (fp_text reference U1 (at -2.88 -0.3 270) (layer F.SilkS))
    (fp_text value SS49E (at 0 -3.302 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 270) (size 0.9 0.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 0.9 0.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 0.9 0.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad3)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/SIP-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:SIP-3 (layer F.Cu) (tedit 5A04D15D)
    (at 174.5 94.5 180)
    (fp_text reference U2 (at 2.9 -0.3 180) (layer F.SilkS))
    (fp_text value SS49E (at 0 -3.302 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 180) (size 0.9 0.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 0.9 0.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 0.9 0.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U2-Pad3)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/SIP-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A04D0DF)
    (at 142.8 101.2 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 2.05 3.75 180) (layer F.SilkS))
    (fp_text value LM393 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 X_SIG))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad3)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U2-Pad3)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 Y_SIG))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/SOIC_8_3_9x4_9mm_Pitch1_27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:SOT-23 (layer F.Cu) (tedit 5A4EEC20)
    (at 135.5 101.2)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U4 (at -2.4 0) (layer F.SilkS))
    (fp_text value AP2210N (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/SOT_23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:C_0603 (layer F.Cu) (tedit 5A4EEC40)
    (at 175.6504 99.124 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -0.024 -1.2496 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:C_0603 (layer F.Cu) (tedit 5A04D06C)
    (at 139.1 98.9 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.25 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:C_0805 (layer F.Cu) (tedit 5A4EEC0E)
    (at 135.4 104.2 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 2.4 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at -0.05 0.05 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:LED_0805 (layer F.Cu) (tedit 5A04D0F4)
    (at 125.75 107 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.7 0.05 90) (layer F.SilkS))
    (fp_text value LED_0805 (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MZBOT:LED_0805 (layer F.Cu) (tedit 5A04D166)
    (at 174.5582 96.4316)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -2.8582 0.0684) (layer F.SilkS))
    (fp_text value LED_0805 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad1)"))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MZBOT:CT6EP103 (layer B.Cu) (tedit 5A4E788F)
    (at 155.4 99.5)
    (fp_text reference VR2 (at 0 -2.54) (layer B.SilkS))
    (fp_text value 10.0K (at 0 3.81) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 1.25) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(R3-Pad2)"))
    (pad 2 thru_hole circle (at -2.5 -1.25) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(R3-Pad2)"))
    (pad 3 thru_hole circle (at 2.5 -1.25) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 5 +3V3))
    (model ../../../../../../Users/cr185092/Documents/KiCAD_Projects/MZBOT_XY-Endstop/MZBOT.pretty/3D_Files/CT6EP103.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MZBOT:LOGO_small (layer B.Cu) (tedit 5A4EE900)
    (at 134.35 104 270)
    (fp_text reference G*** (at -0.9 3.5 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text V24-PCB-ES1 (at 124.1 97.45 270) (layer B.SilkS))
  (gr_text "REV B" (at 123.15 95.6 270) (layer B.SilkS))
  (gr_text "XY Endstop" (at 168.5 102.6) (layer F.SilkS))
  (gr_text BOT (at 134.35 98.9 270) (layer B.SilkS))
  (gr_text MZ (at 134.35 101.55 270) (layer B.SilkS))
  (gr_text X (at 160.2 103.4 270) (layer B.SilkS))
  (gr_text Y (at 160.2 95.1 270) (layer B.SilkS))
  (gr_line (start 160.65 109.5) (end 160.65 105.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178 102.75) (end 178 94.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.5 104.25) (end 162.15 104.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 176.5 102.75) (end 178 102.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.15 111) (end 123.5 111) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 159.15 109.5) (end 160.65 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.15 105.75) (end 160.65 105.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 94.5) (end 122 95.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.5 93) (end 123.5 93) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 176.5 94.5) (end 176.5 93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.5 93) (end 176.5 93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 109.5) (end 122 95.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.5 109.5) (end 123.5 111) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 123.5 94.5) (end 122 94.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178 105) (xy 161 105) (xy 161 111) (xy 122 111) (xy 122 93)
        (xy 178 93) (xy 178 105)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178 105) (xy 161 105) (xy 161 111) (xy 122 111) (xy 122 93)
        (xy 178 93) (xy 178 105)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.94962 99.53752) (xy 170.94962 97.9678) (xy 170.35018 96.51492) (xy 169.2402 95.4024) (xy 167.78986 94.80042)
        (xy 166.2176 94.80042) (xy 164.76472 95.39986) (xy 163.6522 96.50984) (xy 163.05022 97.96018) (xy 163.05022 99.53244)
        (xy 163.64966 100.98532) (xy 164.75964 102.09784) (xy 166.21252 102.69982) (xy 167.78478 102.69982) (xy 169.23512 102.10038)
        (xy 170.34764 100.9904) (xy 170.94962 99.54006)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.69962 99.53752) (xy 131.69962 97.9678) (xy 131.10018 96.51492) (xy 129.9902 95.4024) (xy 128.53986 94.80042)
        (xy 126.9676 94.80042) (xy 125.51472 95.39986) (xy 124.4022 96.50984) (xy 123.80022 97.96018) (xy 123.80022 99.53244)
        (xy 124.39966 100.98532) (xy 125.50964 102.09784) (xy 126.96252 102.69982) (xy 128.53478 102.69982) (xy 129.98512 102.10038)
        (xy 131.09764 100.9904) (xy 131.69962 99.54006)
      )
    )
  )
)
