(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-dev-493-gd776eac)")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 77)
    (zones 0)
    (modules 19)
    (nets 15)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.35 6.35)
    (pad_drill 5.08)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 105.41 90.17)
    (grid_origin 130.81 100.33)
    (visible_elements FFFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J2-Pad7)")
  (net 4 VDD)
  (net 5 "Net-(J2-Pad11)")
  (net 6 "Net-(CRNSOUT1-Pad1)")
  (net 7 "Net-(CRNSOUT1-Pad2)")
  (net 8 "Net-(CRNSOUT1-Pad3)")
  (net 9 "Net-(CRNSOUT1-Pad4)")
  (net 10 "Net-(CRNSOUT1-Pad5)")
  (net 11 "Net-(CRNSOUT1-Pad6)")
  (net 12 "Net-(CRNSOUT1-Pad7)")
  (net 13 "Net-(CRNSOUT1-Pad8)")
  (net 14 "Net-(CRNSOUT1-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(CRNSOUT1-Pad1)")
    (add_net "Net-(CRNSOUT1-Pad2)")
    (add_net "Net-(CRNSOUT1-Pad3)")
    (add_net "Net-(CRNSOUT1-Pad4)")
    (add_net "Net-(CRNSOUT1-Pad5)")
    (add_net "Net-(CRNSOUT1-Pad6)")
    (add_net "Net-(CRNSOUT1-Pad7)")
    (add_net "Net-(CRNSOUT1-Pad8)")
    (add_net "Net-(CRNSOUT1-Pad9)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad7)")
    (add_net VCC)
    (add_net VDD)
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ADA65D5)
    (at 103.505 132.715)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 5.08) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5ADA64F2)
    (at 103.505 90.805)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 5.08) (layers *.Cu *.Mask))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5AD907D3)
    (at 123.444 112.776 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J4 (at 0 -3.302 180) (layer F.SilkS))
    (fp_text value GS4 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad11)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CRNSOUT1-Pad4)"))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad7)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5AD907CD)
    (at 123.444 110.236 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J5 (at 0 -3.302 180) (layer F.SilkS))
    (fp_text value GS5 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad11)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CRNSOUT1-Pad5)"))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad7)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5AD907C5)
    (at 123.444 107.696 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at 0 -3.302 180) (layer F.SilkS))
    (fp_text value GS6 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad11)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CRNSOUT1-Pad6)"))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad7)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5AD907BC)
    (at 123.444 105.156 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at 0 -3.302 180) (layer F.SilkS))
    (fp_text value GS7 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad11)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CRNSOUT1-Pad7)"))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad7)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5AD907B3)
    (at 123.444 102.616 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J8 (at 0 -3.302 180) (layer F.SilkS))
    (fp_text value GS8 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad11)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CRNSOUT1-Pad8)"))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad7)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5AD907AA)
    (at 123.444 100.076 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J9 (at 0 -3.302 180) (layer F.SilkS))
    (fp_text value GS9 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad11)"))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CRNSOUT1-Pad9)"))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad7)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5AD907E1)
    (at 134.62 104.14 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP1 (at 0 3.302 270) (layer F.SilkS))
    (fp_text value DSD_EN_3V3 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad7)"))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 4 VDD))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5AD9081E)
    (at 108.458 124.46)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P4 (at -3.048 0) (layer F.SilkS))
    (fp_text value GND4 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5AD90816)
    (at 108.458 119.888)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P5 (at -3.048 0) (layer F.SilkS))
    (fp_text value GND5 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5AD9080D)
    (at 108.458 115.316)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P6 (at -3.048 0) (layer F.SilkS))
    (fp_text value GND6 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5AD90803)
    (at 108.458 110.744)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P7 (at -3.048 0) (layer F.SilkS))
    (fp_text value GND7 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5AD907F6)
    (at 108.458 106.172)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P8 (at -3.048 0) (layer F.SilkS))
    (fp_text value GND8 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5AD907EB)
    (at 108.458 101.6)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P9 (at -3.048 0) (layer F.SilkS))
    (fp_text value GND9 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Modules:Molex_KK-6410-02_02x2.54mm_Straight_Power (layer F.Cu) (tedit 5AD8F0C8)
    (at 116.84 90.678)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference PWR_3V31 (at 1 -4.5) (layer F.SilkS) hide)
    (fp_text value PWR_3V3 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad GND thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad VCC thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 VDD))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Modules:Molex_KK-6410-02_02x2.54mm_Straight_Power (layer F.Cu) (tedit 5AD8F0C3)
    (at 110.236 90.678)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference PWR_5V1 (at 0 -4.572) (layer F.SilkS) hide)
    (fp_text value PWR_5V (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad GND thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad VCC thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headers:Pin_Header_Straight_2x10_Top_To_Bottom_Pitch2.54mm (layer F.Cu) (tedit 5ADA683B)
    (at 115.57 121.92 180)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference CRNSOUT (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value CRNSOUT (at -2.54 11.43 270) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(CRNSOUT1-Pad1)"))
    (pad 11 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(CRNSOUT1-Pad2)"))
    (pad 12 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(CRNSOUT1-Pad3)"))
    (pad 13 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(CRNSOUT1-Pad4)"))
    (pad 14 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(CRNSOUT1-Pad5)"))
    (pad 15 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(CRNSOUT1-Pad6)"))
    (pad 16 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(CRNSOUT1-Pad7)"))
    (pad 17 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(CRNSOUT1-Pad8)"))
    (pad 18 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(CRNSOUT1-Pad9)"))
    (pad 19 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headers:Pin_Header_Straight_2x10_Top_To_Bottom_Pitch2.54mm (layer F.Cu) (tedit 5ADA6848)
    (at 130.81 123.19 180)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference DSCIN (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value DSC2IN (at -2.54 11.43 270) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad11)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(CRNSOUT1-Pad2)"))
    (pad 13 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(CRNSOUT1-Pad1)"))
    (pad 14 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(CRNSOUT1-Pad3)"))
    (pad 15 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad7)"))
    (pad 17 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VDD))
    (pad 19 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VDD))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MUTE PIN" (at 122.174 116.205 90) (layer F.SilkS))
  (gr_text "DSDEN PIN" (at 124.714 116.586 90) (layer F.SilkS))
  (gr_text DSDEN (at 134.366 107.95) (layer F.SilkS))
  (gr_text MUTE (at 125.222 123.19) (layer F.SilkS))
  (gr_text GND (at 116.586 95.504 90) (layer F.SilkS))
  (gr_text +3V3 (at 119.507 95.885 90) (layer F.SilkS))
  (gr_text +5V (at 113.03 95.504 90) (layer F.SilkS))
  (gr_text 1 (at 117.856 121.92 90) (layer F.SilkS))
  (gr_text 1 (at 133.35 123.19 90) (layer F.SilkS))
  (gr_text GND (at 109.982 95.504 90) (layer F.SilkS))
  (gr_line (start 121.92 86.36) (end 99.06 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 96.52) (end 121.92 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 96.52) (end 121.92 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 127) (end 137.16 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 127) (end 137.16 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 137.16) (end 121.92 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.06 137.16) (end 121.92 137.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.06 86.36) (end 99.06 137.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.762) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.06 86.36) (xy 99.06 137.16) (xy 121.92 137.16) (xy 121.92 127) (xy 137.16 127)
        (xy 137.16 96.52) (xy 121.92 96.52) (xy 121.92 86.36)
      )
    )
  )
  (zone (net 4) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 96.52) (xy 137.16 96.52) (xy 137.16 127) (xy 121.92 127) (xy 121.92 137.16)
        (xy 99.06 137.16) (xy 99.06 86.36) (xy 121.92 86.36)
      )
    )
  )
)
