(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 47)
    (no_connects 0)
    (area 29.615001 74.492 221.083 126.905591)
    (thickness 1.6)
    (drawings 22)
    (tracks 127)
    (zones 0)
    (modules 18)
    (nets 16)
  )
  (page A4)
  (title_block
    (title "ESP8266 Capacitive Soil Sensor")
    (date 2017-02-24)
    (rev 1.0)
    (company "Author: Alan Lord")
    (comment 1 "Contact: alanslists@gmail.com")
    (comment 3 "Creative Commons Attribution-NonCommercial-ShareAlike 4.0 International Public License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.65)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 249.555 95.25)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/alanlord/Personal/Projects/git/esp8266-cap-soil-sensor/pcb/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 /RXD)
  (net 5 /TXD)
  (net 6 "Net-(R1-Pad2)")
  (net 7 /SENS)
  (net 8 "Net-(R2-Pad2)")
  (net 9 "Net-(R3-Pad2)")
  (net 10 /FLASH)
  (net 11 /CHIP_EN)
  (net 12 "Net-(RV1-Pad2)")
  (net 13 "Net-(SW3-Pad3)")
  (net 14 "Net-(CS1-Pad1)")
  (net 15 "Net-(CS1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CHIP_EN)
    (add_net /FLASH)
    (add_net /RXD)
    (add_net /SENS)
    (add_net /TXD)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(CS1-Pad1)")
    (add_net "Net-(CS1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(SW3-Pad3)")
    (add_net VCC)
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58B07F0C)
    (at 161.925 95.758 180)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 2.54 -5.334 360) (layer F.SilkS))
    (fp_text value 74LCX14MX (at 0 5.375 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.7 -1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 0 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.7 1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -2.7 2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.7 3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 2.7 3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(RV1-Pad2)"))
    (pad 9 smd rect (at 2.7 2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CS1-Pad1)"))
    (pad 10 smd rect (at 2.7 1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CS1-Pad2)"))
    (pad 11 smd rect (at 2.7 0 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(RV1-Pad2)"))
    (pad 12 smd rect (at 2.7 -1.27 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (pad 13 smd rect (at 2.7 -2.54 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CS1-Pad2)"))
    (pad 14 smd rect (at 2.7 -3.81 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58A6F384)
    (at 191.643 102.87 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 4.445 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58A6F38A)
    (at 201.041 102.87 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.445 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 58B049A3)
    (at 205.867 89.916 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference P4 (at 6.096 -0.254 360) (layer F.SilkS))
    (fp_text value PWR (at 1.25 4.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58B0495D)
    (at 167.005 88.646)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 2.286 -1.778) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58B04946)
    (at 168.529 100.838 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -2.032 -1.778 90) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /SENS))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58A6F391)
    (at 191.643 94.996 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.445 0 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58B04981)
    (at 194.945 94.996 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -4.318 0 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /FLASH))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58B04953)
    (at 168.529 93.726 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -2.286 -1.778 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /CHIP_EN))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module manuf:BOURNS-3364-W (layer F.Cu) (tedit 58B04962)
    (at 160.655 87.884 180)
    (attr smd)
    (fp_text reference RV1 (at -4.064 2.286 360) (layer F.SilkS))
    (fp_text value POT-BOURNS-3364W (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 2.1 180) (size 1.4 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1.5 2.1 180) (size 1.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CS1-Pad1)"))
    (pad 2 smd rect (at 0 -1.8 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(RV1-Pad2)"))
    (model smd_resistors/trim_murata_pvz2a.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.6 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module switches:SKQGAFE010_Switch (layer F.Cu) (tedit 58B04926)
    (at 161.417 104.14)
    (descr "SKQGAFE010 SMD Mount Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value RESET (at 0 3.556 180) (layer F.SilkS))
    (pad 3 smd rect (at -2.4 1.6) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.4 -1.6) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.4 -1.6) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad2)"))
    (pad 4 smd rect (at 2.4 1.6) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad2)"))
  )
  (module switches:SKQGAFE010_Switch (layer F.Cu) (tedit 58B04345)
    (at 196.291 102.73 90)
    (descr "SKQGAFE010 SMD Mount Tactile Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text value FLASH (at -4.318 0 180) (layer F.SilkS))
    (pad 3 smd rect (at -2.4 1.6 90) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.4 -1.6 90) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.4 -1.6 90) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 /FLASH))
    (pad 4 smd rect (at 2.4 1.6 90) (size 1.8 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 /FLASH))
  )
  (module ESP8266:ESP-12E (layer F.Cu) (tedit 58B07FE4)
    (at 173.101 90.424)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U2 (at -2 -2) (layer F.SilkS) hide)
    (fp_text value ESP-12F (at 6.985 5.08) (layer F.SilkS))
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 4) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 11 /CHIP_EN))
    (pad 4 thru_hole oval (at 0 6) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(R1-Pad2)"))
    (pad 5 thru_hole oval (at 0 8) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 6 thru_hole oval (at 0 10) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SENS))
    (pad 7 thru_hole oval (at 0 12) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 14) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 9 smd oval (at 1.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd oval (at 3.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd oval (at 5.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd oval (at 7.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd oval (at 9.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd oval (at 11.99 15.75 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 15 thru_hole oval (at 14 14) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 16 thru_hole oval (at 14 12) (size 2.5 1.1) (drill 0.65 (offset 0.6 0)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 17 thru_hole oval (at 14 10) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(R3-Pad2)"))
    (pad 18 thru_hole oval (at 14 8) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 10 /FLASH))
    (pad 19 thru_hole oval (at 14 6) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole oval (at 14 4) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole oval (at 14 2) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /RXD))
    (pad 22 thru_hole oval (at 14 0) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 5 /TXD))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58B04986)
    (at 199.009 95.25 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value MCP1700T (at 0 2.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(SW3-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes\SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module switches:SW_SPDT_PCM12 (layer F.Cu) (tedit 58B04999)
    (at 205.613 102.108 90)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference SW3 (at -5.334 0 180) (layer F.SilkS))
    (fp_text value Switch_SPDT_x2 (at 0 4.25 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -1.5 0.325 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.5 0.325 90) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.25 -1.425 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 -1.425 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 2.25 -1.425 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(SW3-Pad3)"))
    (pad "" smd rect (at -3.65 1.425 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 1.425 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 -0.775 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.65 -0.775 90) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58B049B8)
    (at 207.137 83.566 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P3 (at 2.286 5.842 360) (layer F.SilkS))
    (fp_text value SERIAL (at 0 12.55 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RXD))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /TXD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58B16FA7)
    (at 168.275 106.172)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P5 (at 2.54 0.762) (layer F.SilkS))
    (fp_text value INSPECTION (at 0 2.39) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SENS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module cap-sensor:cap_sensor_probe (layer F.Cu) (tedit 58BAE750)
    (at 101.981 94.488)
    (descr "Imported from cap.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference CS1 (at 0 -10.493993) (layer F.SilkS) hide)
    (fp_text value CS (at 0 10.493993) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 54 4.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(CS1-Pad1)"))
    (pad 2 thru_hole rect (at 54 -0.05) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(CS1-Pad2)"))
    (pad 1 thru_hole rect (at 54 -4.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(CS1-Pad1)"))
  )
  (dimension 7.62 (width 0.3) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 155.829 75.692) (layer Dwgs.User))
    (feature1 (pts (xy 149.225 79.502) (xy 149.225 74.516)))
    (feature2 (pts (xy 156.845 79.502) (xy 156.845 74.516)))
    (crossbar (pts (xy 156.845 77.216) (xy 149.225 77.216)))
    (arrow1a (pts (xy 149.225 77.216) (xy 150.351504 76.629579)))
    (arrow1b (pts (xy 149.225 77.216) (xy 150.351504 77.802421)))
    (arrow2a (pts (xy 156.845 77.216) (xy 155.718496 76.629579)))
    (arrow2b (pts (xy 156.845 77.216) (xy 155.718496 77.802421)))
  )
  (gr_text "Max. Depth ->" (at 140.335 94.234 180) (layer B.SilkS))
  (gr_text "Max. Depth ->" (at 140.335 94.234) (layer F.SilkS))
  (gr_line (start 52.705 102.87) (end 156.845 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.451 86.36) (end 156.845 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 164.846196 (width 0.3) (layer Dwgs.User)
    (gr_text "164.846 mm" (at 126.734136 125.428591 359.9117169) (layer Dwgs.User))
    (feature1 (pts (xy 44.323 117.602) (xy 44.309056 126.65159)))
    (feature2 (pts (xy 209.169 117.856) (xy 209.155056 126.90559)))
    (crossbar (pts (xy 209.159216 124.205593) (xy 44.313216 123.951593)))
    (arrow1a (pts (xy 44.313216 123.951593) (xy 45.440622 123.366909)))
    (arrow1b (pts (xy 44.313216 123.951593) (xy 45.438815 124.539749)))
    (arrow2a (pts (xy 209.159216 124.205593) (xy 208.033617 123.617437)))
    (arrow2b (pts (xy 209.159216 124.205593) (xy 208.03181 124.790277)))
  )
  (dimension 16.764 (width 0.3) (layer Dwgs.User)
    (gr_text "16.764 mm" (at 36.115 94.742 270) (layer Dwgs.User))
    (feature1 (pts (xy 42.545 103.124) (xy 34.765 103.124)))
    (feature2 (pts (xy 42.545 86.36) (xy 34.765 86.36)))
    (crossbar (pts (xy 37.465 86.36) (xy 37.465 103.124)))
    (arrow1a (pts (xy 37.465 103.124) (xy 36.878579 101.997496)))
    (arrow1b (pts (xy 37.465 103.124) (xy 38.051421 101.997496)))
    (arrow2a (pts (xy 37.465 86.36) (xy 36.878579 87.486504)))
    (arrow2b (pts (xy 37.465 86.36) (xy 38.051421 87.486504)))
  )
  (dimension 105.918 (width 0.3) (layer Dwgs.User)
    (gr_text "105.918 mm" (at 97.282 110.316) (layer Dwgs.User))
    (feature1 (pts (xy 44.323 104.648) (xy 44.323 111.666)))
    (feature2 (pts (xy 150.241 104.648) (xy 150.241 111.666)))
    (crossbar (pts (xy 150.241 108.966) (xy 44.323 108.966)))
    (arrow1a (pts (xy 44.323 108.966) (xy 45.449504 108.379579)))
    (arrow1b (pts (xy 44.323 108.966) (xy 45.449504 109.552421)))
    (arrow2a (pts (xy 150.241 108.966) (xy 149.114496 108.379579)))
    (arrow2b (pts (xy 150.241 108.966) (xy 149.114496 109.552421)))
  )
  (gr_line (start 44.323 94.488) (end 52.705 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 52.451 86.36) (end 44.323 94.488) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 52.324 (width 0.3) (layer Dwgs.User)
    (gr_text "52.324 mm" (at 183.007 114.634) (layer Dwgs.User))
    (feature1 (pts (xy 209.169 109.982) (xy 209.169 115.984)))
    (feature2 (pts (xy 156.845 109.982) (xy 156.845 115.984)))
    (crossbar (pts (xy 156.845 113.284) (xy 209.169 113.284)))
    (arrow1a (pts (xy 209.169 113.284) (xy 208.042496 113.870421)))
    (arrow1b (pts (xy 209.169 113.284) (xy 208.042496 112.697579)))
    (arrow2a (pts (xy 156.845 113.284) (xy 157.971504 113.870421)))
    (arrow2b (pts (xy 156.845 113.284) (xy 157.971504 112.697579)))
  )
  (dimension 29.21 (width 0.3) (layer Dwgs.User)
    (gr_text "29.210 mm" (at 214.583 94.615 90) (layer Dwgs.User))
    (feature1 (pts (xy 210.185 80.01) (xy 215.933 80.01)))
    (feature2 (pts (xy 210.185 109.22) (xy 215.933 109.22)))
    (crossbar (pts (xy 213.233 109.22) (xy 213.233 80.01)))
    (arrow1a (pts (xy 213.233 80.01) (xy 213.819421 81.136504)))
    (arrow1b (pts (xy 213.233 80.01) (xy 212.646579 81.136504)))
    (arrow2a (pts (xy 213.233 109.22) (xy 213.819421 108.093496)))
    (arrow2b (pts (xy 213.233 109.22) (xy 212.646579 108.093496)))
  )
  (gr_text 3.7v (at 208.407 98.806 90) (layer F.SilkS))
  (gr_text 3.2v (at 208.407 105.41 90) (layer F.SilkS))
  (gr_line (start 209.169 80.01) (end 209.169 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.169 109.22) (end 156.845 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.169 80.01) (end 156.845 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Capacitive WiFi Soil Moisture Sensor\n(c) Alan Lord 2017" (at 183.007 94.488 180) (layer B.SilkS))
  (gr_line (start 156.845 80.01) (end 156.845 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.845 102.87) (end 156.845 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.357 88.392) (xy 170.815 88.392) (xy 170.815 80.01) (xy 189.357 80.01)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.357 88.392) (xy 170.815 88.392) (xy 170.815 80.01) (xy 189.357 80.01)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.169 109.22) (xy 156.845 109.22) (xy 156.845 102.87) (xy 150.241 102.87) (xy 150.241 86.36)
        (xy 156.845 86.36) (xy 156.845 80.01) (xy 209.169 80.01)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.169 109.22) (xy 156.845 109.22) (xy 156.845 102.87) (xy 150.241 102.87) (xy 150.241 86.36)
        (xy 156.845 86.36) (xy 156.845 80.01) (xy 209.169 80.01)
      )
    )
  )
)
