(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 137.033 76.073)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "IN1")
  (net 2 "IN2")
  (net 3 "IN3")
  (net 4 "GND")
  (net 5 "OUTA")
  (net 6 "OUTB")
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126.492 84.455)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at -3.302 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 129.54 93.726)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -1.524 -1.778 45) (layer "F.SilkS"))
    (fp_text value "Conn_02x04_Odd_Even" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "OUTA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.574 84.455)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "footprints:KPJX-3S" (layer "F.Cu")
    (tedit 0)
    (at 137.0076 80.004)
    (descr "Kycon KPJX-3S by Matthew Nielsen, 2024")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -11.256 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x05" (at 0 -9.756 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -8.256 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.5 0.26) (size 1.7 1.7) (drill 1.9) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.5 0.26) (size 1.7 1.7) (drill 1.8) (layers F&B.Cu *.Mask))
    (pad "1" thru_hole oval (at 2.54 7.41) (size 2.5 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_1") (pintype "passive") (zone_connect 2))
    (pad "2" thru_hole oval (at -2.54 7.41) (size 2.5 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_2") (pintype "passive") (zone_connect 2))
    (pad "3" thru_hole circle (at -6 4.26) (size 2.3 2.3) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "IN3") (pinfunction "Pin_3") (pintype "passive") (zone_connect 2))
    (pad "4" thru_hole oval (at 0 -1.74) (size 3.3 2) (drill oval 2.2 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at -7.8 0.26) (size 3.6 3.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "5" thru_hole oval (at -7.8 8.76) (size 2 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "5" thru_hole oval (at 7.8 8.76) (size 2 3.2) (drill oval 0.6 2.7) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "5" thru_hole circle (at 7.8 0.26) (size 3.6 3.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_5") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 133.35 102.997 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 2.032 -1.778 46) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "OUTA") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTB") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 142.24 93.726)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -1.524 -1.778 45) (layer "F.SilkS"))
    (fp_text value "Conn_02x04_Odd_Even" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "OUTA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "IN1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.574 102.997)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 3.937 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126.492 102.997)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at -3.556 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 135.89 93.726)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "kpjx-3s_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -1.524 -1.778 45) (layer "F.SilkS"))
    (fp_text value "Conn_02x04_Odd_Even" (at 1.27 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "OUTA") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "OUTB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "IN2") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 149.734609 102.876433) (mid 149.06693 104.488321) (end 147.455042 105.156) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 147.451825 76.835) (end 126.614175 76.835) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 124.334608 79.114567) (end 124.331392 102.876433) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 126.610959 105.156) (mid 124.999071 104.488321) (end 124.331392 102.876433) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 126.610959 105.156) (end 147.455042 105.156) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 124.334608 79.114567) (mid 125.002287 77.502679) (end 126.614175 76.835) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 147.451825 76.835) (mid 149.063734 77.502668) (end 149.731392 79.114567) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 149.734609 102.876433) (end 149.731392 79.114567) (layer "Edge.Cuts") (width 0.1))
  (gr_text "github.com/xunker/kycon_breakout" (at 137.16 100.457) (layer "B.SilkS"))
  (gr_text "KYCON© KPJX-3S BREAKOUT" (at 137.16 91.8972) (layer "B.SilkS"))
  (gr_text "3" (at 131.826 82.804) (layer "B.SilkS"))
  (gr_text "1" (at 139.446 84.836) (layer "B.SilkS"))
  (gr_text "2" (at 134.366 84.836) (layer "B.SilkS"))
  (gr_text "A" (at 128.016 93.853) (layer "F.SilkS"))
  (gr_text "B" (at 147.066 96.52) (layer "F.SilkS"))
  (gr_text "A" (at 147.066 93.98) (layer "F.SilkS"))
  (gr_text "A" (at 133.35 100.965) (layer "F.SilkS"))
  (gr_text "PIN 2" (at 137.16 91.44) (layer "F.SilkS"))
  (gr_text "PIN 3" (at 130.81 91.44) (layer "F.SilkS"))
  (gr_text "B" (at 140.843 96.52) (layer "F.SilkS"))
  (gr_text "GND" (at 140.97 101.219) (layer "F.SilkS"))
  (gr_text "A" (at 134.366 93.98) (layer "F.SilkS"))
  (gr_text "B" (at 138.43 100.965) (layer "F.SilkS"))
  (gr_text "GND" (at 133.985 99.06 90) (layer "F.SilkS"))
  (gr_text "BOARD\n©2024" (at 143.51 84.709 90) (layer "F.SilkS"))
  (gr_text "GND" (at 135.89 101.219) (layer "F.SilkS"))
  (gr_text "A" (at 140.843 93.98) (layer "F.SilkS"))
  (gr_text "GND" (at 146.685 99.06 90) (layer "F.SilkS"))
  (gr_text "GND" (at 127.635 98.933 90) (layer "F.SilkS"))
  (gr_text "B" (at 134.493 96.52) (layer "F.SilkS"))
  (gr_text "GND" (at 140.335 99.06 90) (layer "F.SilkS"))
  (gr_text "B" (at 128.143 96.393) (layer "F.SilkS"))
  (gr_text "PIN 1" (at 143.51 91.44) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 147.574 102.997) (xy 126.492 102.997))
    (height -6.604)
    (gr_text "21.0820 mm" (at 137.033 108.451) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 126.492 84.455) (xy 126.492 102.997))
    (height 5.715)
    (gr_text "18.5420 mm" (at 119.627 93.726 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 150.114 76.835) (xy 150.114 105.156))
    (height -1.905)
    (gr_text "28.3210 mm" (at 150.869 90.9955 90) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 124.206 104.902) (xy 150.114 104.902))
    (height 2.54)
    (gr_text "25.9080 mm" (at 137.16 106.292) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 4) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.94 114.3)
        (xy 116.84 114.3)
        (xy 116.84 71.12)
        (xy 154.94 71.12)
      )
    )
  )
)
