(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 23)
    (zones 0)
    (modules 9)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-PadA)")
  (net 2 "Net-(L1-Pad1)")
  (net 3 "Net-(L1-Pad2)")
  (net 4 "Net-(Q1-Pad2)")
  (net 5 "Net-(S1-Pad1)")
  (net 6 "Net-(B1-Pad1)")
  (net 7 "Net-(B1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B1-Pad2)")
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(S1-Pad1)")
  )
  (module alexglow-footprints:JTsf380-2 (layer F.Cu) (tedit 0)
    (at 143.637 95.631)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module 1206 (layer F.Cu) (tedit 6245EEB7)
    (at 144.01546 93.98 180)
    (descr "GENERIC 3216 (1206) PACKAGE")
    (tags "GENERIC 3216 (1206) PACKAGE")
    (attr smd)
    (fp_text reference R1 (at -0.00254 0 270) (layer F.SilkS))
    (fp_text value RESISTOR1206 (at 0 1.524 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad2)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(L1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:hlogoTiny (layer F.Cu) (tedit 600E2129)
    (at 151.13 83.185)
    (fp_text reference " " (at 0 0) (layer F.SilkS) hide)
    (fp_text value " " (at 0.75 0) (layer F.SilkS) hide)
  )
  (module LED:LED_5MM (layer F.Cu) (tedit 62450D70)
    (at 143.51 83.185)
    (descr "LED 5MM PTH")
    (tags "LED 5MM PTH")
    (attr virtual)
    (fp_text reference D1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value LED5MM (at 0 3.81) (layer F.SilkS) hide)
    (pad A thru_hole circle (at -1.27 0) (size 1.8796 1.8796) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-PadA)") (solder_mask_margin 0.1016))
    (pad K thru_hole circle (at 1.27 0) (size 1.8796 1.8796) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(B1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:jewel-silk (layer F.Cu) (tedit 62450CD7)
    (at 143.51 98.425)
    (fp_text reference G*** (at -0.635 24.13 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at -0.75 20.955 180) (layer B.SilkS) hide)
  )
  (module alexglow-footprints:maker-tape-batt (layer F.Cu) (tedit 6244A2D6)
    (at 143.51 111.125)
    (fp_text reference B1 (at 0 -6.35) (layer F.SilkS))
    (fp_text value maker-tape-batt (at 0 6.985) (layer F.Fab) hide)
    (fp_text user - (at -1.143 -5.08) (layer F.SilkS))
    (fp_text user + (at 1.143 -5.08) (layer F.SilkS))
    (pad 2 thru_hole circle (at -5.715 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(B1-Pad2)"))
    (pad 1 thru_hole circle (at 5.715 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(B1-Pad1)"))
  )
  (module alexglow-footprints:joule-thief-inductor (layer F.Cu) (tedit 6244A8B4)
    (at 141.605 93.345 90)
    (fp_text reference L1 (at 1.905 -5.08 90) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.81 90) (layer F.Fab))
    (fp_text user α1+β2 (at -5.715 -5.588 90) (layer F.SilkS))
    (fp_text user Col (at 4.318 -2.159 90) (layer F.SilkS))
    (fp_text user Base (at -0.635 -2.159 90) (layer F.SilkS))
    (fp_text user + (at -5.715 -2.286 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.715 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(L1-Pad1)"))
    (pad 2 thru_hole circle (at -0.635 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(L1-Pad2)"))
    (pad 3 thru_hole circle (at 4.445 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-PadA)"))
  )
  (module alexglow-footprints:pn2222a (layer F.Cu) (tedit 6221BC58)
    (at 145.415 88.9 180)
    (fp_text reference Q1 (at 0 -1.651) (layer F.SilkS))
    (fp_text value " " (at 0 3) (layer F.Fab))
    (fp_text user E (at -3 1.5) (layer F.SilkS))
    (fp_text user B (at 0 1.5) (layer F.SilkS))
    (fp_text user C (at 3 1.5) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(B1-Pad2)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 3 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-PadA)"))
  )
  (module Switches:SWITCH_SPST_SMD_A (layer F.Cu) (tedit 600F3B81)
    (at 153.51252 96.6343 270)
    (descr "SPDT SLIDE SWITCH - SMD")
    (tags "SPDT SLIDE SWITCH - SMD")
    (attr smd)
    (fp_text reference S1 (at -0.1143 -0.15748 270) (layer F.SilkS))
    (fp_text value " " (at 0 3.175 270) (layer B.SilkS))
    (pad 1 smd rect (at -2.2479 1.74752 90) (size 0.6985 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(S1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.7493 1.74752 90) (size 0.6985 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(B1-Pad1)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 2.2479 1.74752 90) (size 0.6985 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(L1-Pad1)") (solder_mask_margin 0.1016))
    (pad GND1 smd rect (at -3.64998 -0.99822 270) (size 0.99822 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad GND2 smd rect (at -3.64998 1.09982 270) (size 0.99822 0.79756) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad GND3 smd rect (at 3.64998 -0.99822 270) (size 0.99822 0.59944) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad GND4 smd rect (at 3.64998 1.09982 270) (size 0.99822 0.79756) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
  )
  (gr_text α2 (at 136.017 93.98 90) (layer F.SilkS))
  (gr_text β1 (at 136.017 88.9 90) (layer F.SilkS))
  (gr_text "thx to z. kaparnik & big clive" (at 132.969 103.378 90) (layer F.SilkS))
  (gr_text bit.ly/hackjoule (at 145.415 97.663) (layer F.SilkS))
  (gr_text "joule thief" (at 135.255 85.725 45) (layer F.SilkS))
  (gr_text "alex glow" (at 135.553807 81.945307 45) (layer F.SilkS))
  (gr_text @glowascii (at 135.255 83.82 45) (layer F.SilkS))
  (gr_text v1 (at 147.066 80.01) (layer F.SilkS))
  (gr_line (start 149.86 116.84) (end 137.16 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.08 83.82) (end 137.16 78.74) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.08 111.76) (end 132.08 83.82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.16 116.84) (end 132.08 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.94 111.76) (end 149.86 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.94 83.82) (end 154.94 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.86 78.74) (end 154.94 83.82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.16 78.74) (end 149.86 78.74) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 145.415 104.775) (end 145.415 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.035 104.775) (end 145.415 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.035 101.6) (end 153.035 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 145.415 101.6) (end 153.035 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.985 104.775) (end 133.985 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.605 104.775) (end 133.985 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.605 101.6) (end 141.605 104.775) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.985 101.6) (end 141.605 101.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 145.415 114.935) (end 145.415 107.315) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.605 107.315) (end 145.415 107.315) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.605 107.315) (end 141.605 114.935) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 145.415 114.935) (end 141.605 114.935) (layer Edge.Cuts) (width 0.05))
)
