(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 84)
    (tracks 110)
    (zones 0)
    (modules 5)
    (nets 31)
  )
  (page USLetter)
  (title_block
    (title "28C256 SOIC to 27C256 DIP")
    (date 2021-03-16)
    (rev 004)
    (company "Bran. K. White - b.kenyon.w@gmail.com")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (user_via 0.92 0.4)
    (uvia_size 0.5)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.3)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 2)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 0 0)
    (grid_origin 136.03 103.81)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_28C256_to_27C256_004"))
  )
  (net 0 "")
  (net 1 /VCC)
  (net 2 /GND)
  (net 3 /A14)
  (net 4 /D2)
  (net 5 /A13)
  (net 6 /D1)
  (net 7 /A8)
  (net 8 /D0)
  (net 9 /A9)
  (net 10 /A0)
  (net 11 /A11)
  (net 12 /A1)
  (net 13 /~OE)
  (net 14 /A2)
  (net 15 /A10)
  (net 16 /A3)
  (net 17 /~CE)
  (net 18 /A4)
  (net 19 /D7)
  (net 20 /A5)
  (net 21 /D6)
  (net 22 /A6)
  (net 23 /D5)
  (net 24 /A7)
  (net 25 /D4)
  (net 26 /A12)
  (net 27 /D3)
  (net 28 /~WE)
  (net 29 /A14_WE)
  (net 30 /NC_A14)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.3)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A14_WE)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /GND)
    (add_net /NC_A14)
    (add_net /VCC)
    (add_net /~CE)
    (add_net /~OE)
    (add_net /~WE)
  )
  (module 000_LOCAL:R_0805 (layer F.Cu) (tedit 5F9E65BE)
    (at 132.855 98.73)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.05 -0.02 -90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 28 /~WE))
    (pad 2 smd roundrect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 /VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:DIP28_0.6_pcb_sil_pins (layer F.Cu) (tedit 5FC98BE5)
    (at 136.03 103.81)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference J1 (at 0 0 -90) (layer F.SilkS))
    (fp_text value "27C256 DIP LEGS" (at -1.5 0 -90) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -7.62 -16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 30 /NC_A14))
    (pad 15 thru_hole circle (at 7.62 16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 27 /D3))
    (pad 2 thru_hole circle (at -7.62 -13.97) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 /A12))
    (pad 16 thru_hole circle (at 7.62 13.97) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 /D4))
    (pad 3 thru_hole circle (at -7.62 -11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 /A7))
    (pad 17 thru_hole circle (at 7.62 11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 23 /D5))
    (pad 4 thru_hole circle (at -7.62 -8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 22 /A6))
    (pad 18 thru_hole circle (at 7.62 8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 21 /D6))
    (pad 5 thru_hole circle (at -7.62 -6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 20 /A5))
    (pad 19 thru_hole circle (at 7.62 6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 /D7))
    (pad 6 thru_hole circle (at -7.62 -3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 /A4))
    (pad 20 thru_hole circle (at 7.62 3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 /~CE))
    (pad 7 thru_hole circle (at -7.62 -1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 /A3))
    (pad 21 thru_hole circle (at 7.62 1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 /A10))
    (pad 8 thru_hole circle (at -7.62 1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 /A2))
    (pad 22 thru_hole circle (at 7.62 -1.27) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 /~OE))
    (pad 9 thru_hole circle (at -7.62 3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 12 /A1))
    (pad 23 thru_hole circle (at 7.62 -3.81) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 /A11))
    (pad 10 thru_hole circle (at -7.62 6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 /A0))
    (pad 24 thru_hole circle (at 7.62 -6.35) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 /A9))
    (pad 11 thru_hole circle (at -7.62 8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 /D0))
    (pad 25 thru_hole circle (at 7.62 -8.89) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 /A8))
    (pad 12 thru_hole circle (at -7.62 11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 /D1))
    (pad 26 thru_hole circle (at 7.62 -11.43) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 /A13))
    (pad 13 thru_hole circle (at -7.62 13.97) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 /D2))
    (pad 27 thru_hole circle (at 7.62 -13.97) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 29 /A14_WE))
    (pad 14 thru_hole circle (at -7.62 16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 28 thru_hole circle (at 7.62 -16.51) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 /VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz -7.62 -16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 -1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 1.27 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 3.81 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 6.35 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 8.890000000000001 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 11.43 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 13.97 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/DIL_LEG.step
      (offset (xyz 7.62 16.51 0.18))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:NPTH_3mm (layer F.Cu) (tedit 5F9F8D8C)
    (at 136.03 86.665)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value NPTH_3mm (at 0 -2.54) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module 000_LOCAL:Pin_Header_Angled_1x04_Pitch2.54mm (layer F.Cu) (tedit 5E5EFA6B)
    (at 130.315 88.57)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference JP1 (at 4.385 -2.27) (layer F.SilkS) hide)
    (fp_text value Jumper_3_Bridged12 (at 4.385 9.89) (layer F.Fab))
    (fp_text user %R (at 2.77 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 30 /NC_A14))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 3 /A14))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 /A14_WE))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 /~WE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/PinHeader_1x04_P2.54mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:SOIC28W (layer F.Cu) (tedit 5E621887)
    (at 136.03 109.525)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -10.05) (layer F.SilkS) hide)
    (fp_text value 28C256 (at 0 0 -90) (layer F.SilkS))
    (fp_text user %R (at -0.01 1.61) (layer F.Fab))
    (pad 28 smd roundrect (at 4.7 -8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /VCC))
    (pad 27 smd roundrect (at 4.7 -6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /~WE))
    (pad 26 smd roundrect (at 4.7 -5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /A13))
    (pad 25 smd roundrect (at 4.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /A8))
    (pad 24 smd roundrect (at 4.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /A9))
    (pad 23 smd roundrect (at 4.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /A11))
    (pad 22 smd roundrect (at 4.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /~OE))
    (pad 21 smd roundrect (at 4.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /A10))
    (pad 20 smd roundrect (at 4.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /~CE))
    (pad 19 smd roundrect (at 4.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /D7))
    (pad 18 smd roundrect (at 4.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /D6))
    (pad 17 smd roundrect (at 4.7 5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /D5))
    (pad 16 smd roundrect (at 4.7 6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /D4))
    (pad 15 smd roundrect (at 4.7 8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /D3))
    (pad 14 smd roundrect (at -4.7 8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /GND))
    (pad 13 smd roundrect (at -4.7 6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /D2))
    (pad 12 smd roundrect (at -4.7 5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /D1))
    (pad 11 smd roundrect (at -4.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /D0))
    (pad 10 smd roundrect (at -4.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /A0))
    (pad 9 smd roundrect (at -4.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /A1))
    (pad 8 smd roundrect (at -4.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /A2))
    (pad 7 smd roundrect (at -4.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /A3))
    (pad 6 smd roundrect (at -4.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /A4))
    (pad 5 smd roundrect (at -4.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /A5))
    (pad 4 smd roundrect (at -4.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /A6))
    (pad 3 smd roundrect (at -4.7 -5.715) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /A7))
    (pad 2 smd roundrect (at -4.7 -6.985) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /A12))
    (pad 1 smd roundrect (at -4.7 -8.255) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /A14))
    (model ${KIPRJMOD}/000_LOCAL.pretty/packages3d/SOIC28W.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text github.com/bkw777/aDIPters (at 141.7574 98.9076 -270) (layer B.SilkS))
  (gr_text "28C256 pinout (PROGRAM)" (at 133.0325 97.79 -270) (layer B.SilkS))
  (gr_text "27C256 pinout (RUN)" (at 130.315 97.79 -270) (layer B.SilkS))
  (gr_text RUN (at 137.7445 92.4435) (layer F.SilkS))
  (gr_text "28C256 to 27C256" (at 136.03 119.685) (layer F.SilkS))
  (gr_line (start 127.775 120.955) (end 127.775 86.665) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144.285 86.665) (end 144.285 120.955) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.775 86.665) (end 144.285 86.665) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127.775 120.955) (end 144.285 120.955) (layer Edge.Cuts) (width 0.05))
  (gr_text "R1: 47k" (at 141.478 112.268 90) (layer B.SilkS))
  (gr_text "Legs: TE 1544210" (at 142.24 112.268 90) (layer B.SilkS))
)
