(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 40)
    (no_connects 1)
    (area 149.784999 104.064999 177.875001 157.555001)
    (thickness 1.6002)
    (drawings 23)
    (tracks 226)
    (zones 0)
    (modules 10)
    (nets 47)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 +12V)
  (net 17 GND)
  (net 18 "Net-(J2-Pad3)")
  (net 19 "Net-(J2-Pad4)")
  (net 20 "Net-(J2-Pad13)")
  (net 21 "Net-(J2-Pad6)")
  (net 22 "Net-(J2-Pad7)")
  (net 23 "Net-(J2-Pad8)")
  (net 24 "Net-(J2-Pad9)")
  (net 25 "Net-(J2-Pad10)")
  (net 26 "Net-(J2-Pad11)")
  (net 27 "Net-(J2-Pad12)")
  (net 28 "Net-(J2-Pad14)")
  (net 29 "Net-(J2-Pad15)")
  (net 30 "Net-(J4-Pad2)")
  (net 31 "Net-(J4-Pad3)")
  (net 32 "Net-(J4-Pad4)")
  (net 33 "Net-(J4-Pad5)")
  (net 34 "Net-(J4-Pad6)")
  (net 35 "Net-(J5-Pad2)")
  (net 36 "Net-(J5-Pad3)")
  (net 37 "Net-(J5-Pad4)")
  (net 38 "Net-(J5-Pad5)")
  (net 39 "Net-(J5-Pad6)")
  (net 40 "Net-(J7-Pad2)")
  (net 41 "Net-(U2-Pad5)")
  (net 42 "Net-(U2-Pad6)")
  (net 43 "Net-(U2-Pad7)")
  (net 44 "Net-(U2-Pad10)")
  (net 45 "Net-(U2-Pad11)")
  (net 46 "Net-(U2-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +12V)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 160.02 134.62 90)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 -3.55 90) (layer F.SilkS))
    (fp_text value ULN2003 (at 0 3.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at -2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 3 smd rect (at -2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 4 smd rect (at -2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 5 smd rect (at -2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 9 smd rect (at 2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 +12V))
    (pad 10 smd rect (at 2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at 2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J5-Pad6)"))
    (pad 14 smd rect (at 2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J5-Pad5)"))
    (pad 15 smd rect (at 2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J5-Pad4)"))
    (pad 16 smd rect (at 2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 152.4 109.22)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x15 (at 0 37.89) (layer F.Fab))
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 161.29 154.94 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +12V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad13)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad4)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 160.02 121.92 90)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -3.55 90) (layer F.SilkS))
    (fp_text value ULN2003 (at 0 3.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad7)"))
    (pad 2 smd rect (at -2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad8)"))
    (pad 3 smd rect (at -2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-Pad9)"))
    (pad 4 smd rect (at -2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J2-Pad10)"))
    (pad 5 smd rect (at -2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad11)"))
    (pad 6 smd rect (at -2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J2-Pad12)"))
    (pad 7 smd rect (at -2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 8 smd rect (at -2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 GND))
    (pad 9 smd rect (at 2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 +12V))
    (pad 10 smd rect (at 2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J5-Pad2)"))
    (pad 11 smd rect (at 2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J4-Pad6)"))
    (pad 12 smd rect (at 2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J4-Pad5)"))
    (pad 13 smd rect (at 2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J4-Pad4)"))
    (pad 14 smd rect (at 2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad3)"))
    (pad 15 smd rect (at 2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J4-Pad2)"))
    (pad 16 smd rect (at 2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 167.64 109.22)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x15 (at 0 37.89) (layer F.Fab))
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad13)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad15)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x15_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 175.26 106.68)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at -2.794 0) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 175.26 124.46)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at -2.794 0) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 175.26 142.24)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J6 (at -2.794 0) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 170.18 154.94 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 +12V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Graphics:laforge (layer B.Cu) (tedit 59F8A154)
    (at 161.036 138.557 180)
    (fp_text reference "" (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 149.86 154.94) (end 149.86 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 157.48) (end 152.4 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 106.68) (end 177.8 154.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 104.14) (end 175.26 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 154.94) (end 152.4 157.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.26 154.94) (end 177.8 154.94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 175.26 106.68) (end 175.26 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.4 106.68) (end 149.86 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text POT (at 158.75 151.13 90) (layer F.SilkS))
  (gr_text POT (at 156.21 151.13 90) (layer F.SilkS))
  (gr_text +12V (at 161.29 151.13 90) (layer F.SilkS))
  (gr_text GND (at 153.67 151.13 90) (layer F.SilkS))
  (gr_text "-If you havin core problems\nI feel bad for you son.\nI got 99 problems but\na breach ain't one!" (at 162.052 149.86) (layer B.SilkS))
  (gr_text "Arduino Nano Shield for\n3D Printed STTNG Warp Core\n\nwww.thingiverse.com/\nthing:1656741" (at 160.02 118.11 90) (layer B.SilkS))
  (gr_text 1 (at 154.94 108.585) (layer F.SilkS))
  (gr_text USB (at 160.02 144.78) (layer F.SilkS))
  (gr_text . (at 157.607 135.636) (layer F.SilkS))
  (gr_text . (at 157.607 122.936) (layer F.SilkS))
  (gr_text W3DRK (at 160.02 106.68 360) (layer F.Mask))
  (zone (net 16) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.86 104.14) (xy 177.8 104.14) (xy 177.8 157.48) (xy 149.86 157.48)
      )
    )
  )
  (zone (net 17) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.86 104.14) (xy 177.8 104.14) (xy 177.8 157.48) (xy 149.86 157.48)
      )
    )
  )
)
