(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(A1-RX{slash}D0-Pad14)")
	(net 2 "unconnected-(A1-DIO3-Pad31)")
	(net 3 "unconnected-(A1-A4-Pad9)")
	(net 4 "unconnected-(A1-D12-Pad24)")
	(net 5 "unconnected-(A1-ANT-Pad29)")
	(net 6 "GND")
	(net 7 "SCL")
	(net 8 "unconnected-(A1-DIO1-Pad16)")
	(net 9 "unconnected-(A1-AREF-Pad3)")
	(net 10 "unconnected-(A1-D10-Pad22)")
	(net 11 "unconnected-(A1-VBAT-Pad28)")
	(net 12 "unconnected-(A1-MOSI{slash}D23-Pad12)")
	(net 13 "unconnected-(A1-DIO5-Pad30)")
	(net 14 "unconnected-(A1-D13-Pad25)")
	(net 15 "unconnected-(A1-A3-Pad8)")
	(net 16 "unconnected-(A1-EN-Pad27)")
	(net 17 "unconnected-(A1-D9-Pad21)")
	(net 18 "unconnected-(A1-SCK{slash}D24-Pad11)")
	(net 19 "unconnected-(A1-DAC0{slash}A0-Pad5)")
	(net 20 "+3V3")
	(net 21 "unconnected-(A1-MISO{slash}D22-Pad13)")
	(net 22 "SDA")
	(net 23 "unconnected-(A1-A1-Pad6)")
	(net 24 "unconnected-(A1-D11-Pad23)")
	(net 25 "unconnected-(A1-D5-Pad19)")
	(net 26 "unconnected-(A1-TX{slash}D1-Pad15)")
	(net 27 "unconnected-(A1-DIO2-Pad32)")
	(net 28 "unconnected-(A1-A2-Pad7)")
	(net 29 "unconnected-(A1-D6-Pad20)")
	(net 30 "unconnected-(A1-USB-Pad26)")
	(net 31 "unconnected-(A1-A5-Pad10)")
	(net 32 "unconnected-(A1-~{RESET}-Pad1)")
	(net 33 "unconnected-(Artemis1-COPI-Pad6)")
	(net 34 "Net-(Artemis1-AD11)")
	(net 35 "Net-(Artemis1-AD12)")
	(net 36 "Net-(Artemis1-AD29)")
	(net 37 "unconnected-(Artemis1-CIPO-Pad7)")
	(net 38 "unconnected-(Artemis1-GND-Pad5)")
	(net 39 "unconnected-(Artemis1-RST-Pad20)")
	(net 40 "unconnected-(J1-GPIO27{slash}SDIO_DAT3-Pad13)")
	(net 41 "unconnected-(J1-~{CE1}_SPI0{slash}GPIO07-Pad26)")
	(net 42 "unconnected-(J1-MISO_SPI0{slash}GPIO09-Pad21)")
	(net 43 "unconnected-(J1-~{CE0}_SPI0{slash}GPIO08-Pad24)")
	(net 44 "unconnected-(J1-GPIO17{slash}SPI1_~{CE1}-Pad11)")
	(net 45 "unconnected-(J1-SCLK_SPI0{slash}GPIO11-Pad23)")
	(net 46 "unconnected-(J1-GPCLK2{slash}GPIO06-Pad31)")
	(net 47 "unconnected-(J1-GPIO13{slash}PWM1-Pad33)")
	(net 48 "unconnected-(J1-MOSI_SPI0{slash}GPIO10-Pad19)")
	(net 49 "unconnected-(J1-GPCLK0{slash}GPIO04-Pad7)")
	(net 50 "unconnected-(J1-3V3-Pad1)")
	(net 51 "+5V")
	(net 52 "unconnected-(J1-3V3-Pad1)_1")
	(net 53 "unconnected-(J1-GPIO23{slash}SDIO_CMD-Pad16)")
	(net 54 "unconnected-(J1-ID_SC_I2C0{slash}GPIO01-Pad28)")
	(net 55 "unconnected-(J1-GPIO19{slash}SPI1_MISO{slash}PCM_FS-Pad35)")
	(net 56 "unconnected-(J1-GPIO21{slash}SPI1_SCLK{slash}PCM_DOUT-Pad40)")
	(net 57 "unconnected-(J1-GPIO22{slash}SDIO_CLK-Pad15)")
	(net 58 "unconnected-(J1-GPIO15{slash}UART_RXD-Pad10)")
	(net 59 "unconnected-(J1-GPIO16{slash}SPI1_~{CE2}-Pad36)")
	(net 60 "unconnected-(J1-ID_SD_I2C0{slash}GPIO00-Pad27)")
	(net 61 "unconnected-(J1-GPIO25{slash}SDIO_DAT1-Pad22)")
	(net 62 "unconnected-(J1-GPCLK1{slash}GPIO05-Pad29)")
	(net 63 "unconnected-(J1-GPIO18{slash}SPI1_~{CE0}{slash}PCM_CLK{slash}PWM0-Pad12)")
	(net 64 "unconnected-(J1-GPIO20{slash}SPI1_MOSI{slash}PCM_DIN{slash}PWM1-Pad38)")
	(net 65 "unconnected-(J1-GPIO24{slash}SDIO_DAT0-Pad18)")
	(net 66 "unconnected-(J1-GPIO12{slash}PWM0-Pad32)")
	(net 67 "unconnected-(J1-GPIO14{slash}UART_TXD-Pad8)")
	(net 68 "unconnected-(J1-GPIO26{slash}SDIO_DAT2-Pad37)")
	(net 69 "unconnected-(PS1-CTRL{slash}UVLO-Pad2)")
	(net 70 "unconnected-(PS1-TRIM-Pad5)")
	(net 71 "Net-(J2-Pin_2)")
	(net 72 "Net-(J2-Pin_1)")
	(net 73 "unconnected-(PS1-+SENSE-Pad6)")
	(net 74 "unconnected-(Artemis1-AD15{slash}RX-Pad2)")
	(net 75 "unconnected-(Artemis1-D4-Pad10)")
	(net 76 "unconnected-(Artemis1-SCK-Pad8)")
	(net 77 "unconnected-(Artemis1-EN-Pad22)")
	(net 78 "unconnected-(U1D-RX2_J7-PadJ7_5)")
	(net 79 "unconnected-(U1D-RXI{slash}MOSI-PadJ7_3)")
	(net 80 "unconnected-(U1D-3.3V_J7-PadJ7_7)")
	(net 81 "unconnected-(U1D-TXO{slash}MISO-PadJ7_2)")
	(net 82 "unconnected-(U1D-TX2_J7-PadJ7_6)")
	(net 83 "Net-(Artemis1-AD31)")
	(net 84 "Net-(Artemis1-AD32)")
	(net 85 "unconnected-(Artemis1-3V3-Pad11)")
	(net 86 "unconnected-(Artemis1-VBUS-Pad24)")
	(net 87 "unconnected-(Artemis1-AD35-Pad9)")
	(net 88 "unconnected-(Artemis1-GND-Pad16)")
	(net 89 "unconnected-(Artemis1-AD42-Pad14)")
	(net 90 "unconnected-(Artemis1-AD43-Pad13)")
	(net 91 "unconnected-(Artemis1-AD37-Pad25)")
	(footprint "GPS-15136:GPS-15136"
		(layer "F.Cu")
		(at 50.97 66.75 -90)
		(property "Reference" "U1"
			(at 3.175 -44.635 90)
			(layer "F.SilkS")
		)
		(property "Value" "GPS-15136"
			(at 10.16 1.385 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "N/A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "SparkFun"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "N/A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 2.54 -40.64 270)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 -2.54 270)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 40.64 -40.64 270)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 40.64 -2.54 270)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "J1_1" thru_hole rect
			(at 1.27 -34.29 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J1_2" thru_hole circle
			(at 1.27 -31.75 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J1_3" thru_hole circle
			(at 1.27 -29.21 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J1_4" thru_hole circle
			(at 1.27 -26.67 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J1_5" thru_hole circle
			(at 1.27 -24.13 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J1_6" thru_hole circle
			(at 1.27 -21.59 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J3_1" thru_hole rect
			(at 13.97 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J3_2" thru_hole circle
			(at 16.51 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J3_3" thru_hole circle
			(at 19.05 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J3_4" thru_hole circle
			(at 21.59 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J6_1" thru_hole rect
			(at 24.13 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J6_2" thru_hole circle
			(at 26.67 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J6_3" thru_hole circle
			(at 29.21 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J6_4" thru_hole circle
			(at 31.75 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J6_5" thru_hole circle
			(at 34.29 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J6_6" thru_hole circle
			(at 36.83 -1.27 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "J7_1" thru_hole rect
			(at 34.29 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "SCL")
			(pinfunction "SCL/SCK_J7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "J7_2" thru_hole circle
			(at 31.75 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "unconnected-(U1D-TXO{slash}MISO-PadJ7_2)")
			(pinfunction "TXO/MISO")
			(pintype "output+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "J7_3" thru_hole circle
			(at 29.21 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "unconnected-(U1D-RXI{slash}MOSI-PadJ7_3)")
			(pinfunction "RXI/MOSI")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "J7_4" thru_hole circle
			(at 26.67 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "SDA")
			(pinfunction "SDA/~{CS}_J7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "J7_5" thru_hole circle
			(at 24.13 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "unconnected-(U1D-RX2_J7-PadJ7_5)")
			(pinfunction "RX2_J7")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "J7_6" thru_hole circle
			(at 21.59 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "unconnected-(U1D-TX2_J7-PadJ7_6)")
			(pinfunction "TX2_J7")
			(pintype "output+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "J7_7" thru_hole circle
			(at 19.05 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "unconnected-(U1D-3.3V_J7-PadJ7_7)")
			(pinfunction "3.3V_J7")
			(pintype "power_in+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "J7_8" thru_hole circle
			(at 16.51 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "5V_J7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "J7_9" thru_hole circle
			(at 13.97 -41.91 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND_J7")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/blchase1/Downloads/UBLOX_ZED_F9P_GPS_RTK_2.step"
			(offset
				(xyz 43.2 -0.1 5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom"
		(layer "F.Cu")
		(at 40.5 154)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 ISO7380")
		(property "Reference" "H2"
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "B.Cu" "B.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "KiCad:RPMGE5010"
		(layer "F.Cu")
		(at 51.94 33.76)
		(descr "RPMGE5.0-10-1")
		(tags "Power Supply")
		(property "Reference" "PS1"
			(at 25.4 7.62 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RPMGE5.0-10"
			(at 25.4 7.62 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://recom-power.com/pdf/Innoline/RPMGE-10.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "10A DC/DC-Converter 'INNOLINE' 1/8 Brick OF reg"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "10A DC/DC-Converter \\'INNOLINE\\' 1/8 Brick OF reg"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "919-RPMGE5.0-10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/RECOM-Power/RPMGE5.0-10?qs=i8QVZAFTkqRIqGb7iTFPig%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "RECOM Power"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "RPMGE5.0-10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 25.4 1.74 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.92 1.92)
			(drill 1.28)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(J2-Pin_1)")
			(pinfunction "+VIN")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 7.62)
			(size 1.92 1.92)
			(drill 1.28)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "unconnected-(PS1-CTRL{slash}UVLO-Pad2)")
			(pinfunction "CTRL/UVLO")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole circle
			(at 0 15.24)
			(size 1.92 1.92)
			(drill 1.28)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(J2-Pin_2)")
			(pinfunction "-VIN")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 50.8 15.24)
			(size 2.745 2.745)
			(drill 1.83)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "-VOUT")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 50.8 7.62)
			(size 1.92 1.92)
			(drill 1.28)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "unconnected-(PS1-TRIM-Pad5)")
			(pinfunction "TRIM")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole circle
			(at 50.8 3.81)
			(size 1.92 1.92)
			(drill 1.28)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "unconnected-(PS1-+SENSE-Pad6)")
			(pinfunction "+SENSE")
			(pintype "passive+no_connect")
		)
		(pad "7" thru_hole circle
			(at 50.8 0)
			(size 2.745 2.745)
			(drill 1.83)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+VOUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/Users/blchase1/Downloads/LIB_RPMGE5.0-10/RPMGE5.0-10/3D/RPMGE5.0-10.stp"
			(offset
				(xyz -3 -19 5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom"
		(layer "F.Cu")
		(at 169.5 29)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 ISO7380")
		(property "Reference" "H3"
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "B.Cu" "B.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 102.725 26 90)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J2"
			(at 2.5 -2.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "28V"
			(at 4.385 4.81 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 70.24 26 -90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Camera"
			(at 0 10 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "SCL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 94.78 26 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Servo1"
			(at 0 7.46 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(Artemis1-AD11)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 58.01 26.5 180)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 3.01 -2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "Net-(Artemis1-AD31)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.step"
			(offset
				(xyz 0 0 -3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 52.5 26.5 180)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 3 -2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "Net-(Artemis1-AD32)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.step"
			(offset
				(xyz 0 0 -3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "ToddToddsBattBatt:Battery"
		(layer "F.Cu")
		(at 161.04 21.77 -90)
		(property "Reference" "Battery1"
			(at 3.73 24 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 4 40.5)
			(end 5.5 40.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 99.5 40.5)
			(end 101 40.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 4 7.5)
			(end 5.5 7.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 99.5 7.5)
			(end 101 7.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 34.23 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "1" thru_hole circle
			(at 34.23 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 36.77 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 36.77 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 45.36 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 45.36 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 47.9 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 47.9 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 56.49 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 56.49 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 59.03 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 59.03 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 67.62 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 67.62 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 70.16 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 70.16 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at 78.75 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at 78.75 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+5")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at 81.29 1.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "10" thru_hole circle
			(at 81.29 46.2 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "21" thru_hole circle
			(at 108.5 8.73 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "+VCC")
			(pintype "input")
		)
		(pad "22" thru_hole circle
			(at 108.5 11.27 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom"
		(layer "F.Cu")
		(at 40.5 29)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 ISO7380")
		(property "Reference" "H1"
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "B.Cu" "B.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom"
		(layer "F.Cu")
		(at 169.5 154)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 ISO7380")
		(property "Reference" "H4"
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "F.Cu" "F.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.5 4.5)
			(layers "B.Cu" "B.Mask")
			(net 6 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 82.24 26 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Servo2"
			(at 0 7.46 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(Artemis1-AD12)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:Adafruit_Feather_M0_RFM"
		(layer "B.Cu")
		(at 154.28 50 90)
		(descr "Footprint for the Adafruit Feather M0 RFM series of boards, e.g. https://learn.adafruit.com/adafruit-feather-m0-radio-with-rfm69-packet-radio")
		(tags "Adafruit Feather M0 RFM")
		(property "Reference" "A1"
			(at 10.16 4.72 90)
			(layer "B.SilkS")
		)
		(property "Value" "Adafruit_Feather_M0_RFM9x_LoRa_Radio"
			(at 10.16 -45.72 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-radio-with-lora-radio-module.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU and RFM9x Radio"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Adafruit*Feather*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 -19.05 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 32 "unconnected-(A1-~{RESET}-Pad1)")
			(pinfunction "~{RESET}")
			(pintype "input+no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "+3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(A1-AREF-Pad3)")
			(pinfunction "AREF")
			(pintype "input+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 0 -10.16 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(A1-DAC0{slash}A0-Pad5)")
			(pinfunction "DAC0/A0")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 -12.7 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(A1-A1-Pad6)")
			(pinfunction "A1")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 -15.24 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(A1-A2-Pad7)")
			(pinfunction "A2")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 -17.78 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(A1-A3-Pad8)")
			(pinfunction "A3")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" thru_hole oval
			(at 0 -20.32 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(A1-A4-Pad9)")
			(pinfunction "A4")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" thru_hole oval
			(at 0 -22.86 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(A1-A5-Pad10)")
			(pinfunction "A5")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 -25.4 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-SCK{slash}D24-Pad11)")
			(pinfunction "SCK/D24")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" thru_hole oval
			(at 0 -27.94 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(A1-MOSI{slash}D23-Pad12)")
			(pinfunction "MOSI/D23")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole oval
			(at 0 -30.48 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(A1-MISO{slash}D22-Pad13)")
			(pinfunction "MISO/D22")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" thru_hole oval
			(at 0 -33.02 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(A1-RX{slash}D0-Pad14)")
			(pinfunction "RX/D0")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" thru_hole oval
			(at 0 -35.56 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(A1-TX{slash}D1-Pad15)")
			(pinfunction "TX/D1")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" thru_hole oval
			(at 0 -38.1 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(A1-DIO1-Pad16)")
			(pinfunction "DIO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" thru_hole oval
			(at 20.32 -38.1 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "SDA")
			(pinfunction "SDA/D20")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole oval
			(at 20.32 -35.56 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "SCL")
			(pinfunction "SCL/D21")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 20.32 -33.02 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(A1-D5-Pad19)")
			(pinfunction "D5")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" thru_hole oval
			(at 20.32 -30.48 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(A1-D6-Pad20)")
			(pinfunction "D6")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" thru_hole oval
			(at 20.32 -27.94 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(A1-D9-Pad21)")
			(pinfunction "D9")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" thru_hole oval
			(at 20.32 -25.4 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(A1-D10-Pad22)")
			(pinfunction "D10")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" thru_hole oval
			(at 20.32 -22.86 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-D11-Pad23)")
			(pinfunction "D11")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole oval
			(at 20.32 -20.32 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(A1-D12-Pad24)")
			(pinfunction "D12")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole oval
			(at 20.32 -17.78 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(A1-D13-Pad25)")
			(pinfunction "D13")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" thru_hole oval
			(at 20.32 -15.24 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(A1-USB-Pad26)")
			(pinfunction "USB")
			(pintype "power_in+no_connect")
		)
		(pad "27" thru_hole oval
			(at 20.32 -12.7 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-EN-Pad27)")
			(pinfunction "EN")
			(pintype "input+no_connect")
		)
		(pad "28" thru_hole oval
			(at 20.32 -10.16 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(A1-VBAT-Pad28)")
			(pinfunction "VBAT")
			(pintype "power_in+no_connect")
		)
		(pad "29" thru_hole oval
			(at 3.81 -43.18)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(A1-ANT-Pad29)")
			(pinfunction "ANT")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole oval
			(at 11.43 -43.18)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(A1-DIO5-Pad30)")
			(pinfunction "DIO5")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" thru_hole oval
			(at 13.97 -43.18)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(A1-DIO3-Pad31)")
			(pinfunction "DIO3")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" thru_hole oval
			(at 16.51 -43.18)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(A1-DIO2-Pad32)")
			(pinfunction "DIO2")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather_M0_RFM.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/blchase1/Downloads/LORA.step"
			(offset
				(xyz 28.75 5.6 8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:Raspberry Pi 2x20 Socket"
		(layer "B.Cu")
		(at 49.03 54.74 -90)
		(descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x20 2.54mm double row")
		(property "Reference" "J1"
			(at 0.5 5 90)
			(layer "B.SilkS")
		)
		(property "Value" "Raspberry_Pi_4"
			(at 0.5 1.5 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rpi4/raspberry-pi-4-datasheet.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Raspberry Pi 4 Model B"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 3.5 -3.5)
			(end 4.875 -3.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 61.5 -3.5)
			(end 62.875 -3.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 3.5 -52.5)
			(end 4.875 -52.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 61.5 -52.5)
			(end 62.875 -52.5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 3 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 8.4 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(J1-3V3-Pad1)_1")
			(pinfunction "3V3")
			(pintype "power_out+no_connect")
		)
		(pad "2" thru_hole circle
			(at 8.4 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "5V")
			(pintype "power_out")
		)
		(pad "3" thru_hole circle
			(at 10.94 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "SDA")
			(pinfunction "SDA_I2C1/GPIO02")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at 10.94 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "5V")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 13.48 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "SCL")
			(pinfunction "SCL_I2C1/GPIO03")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 13.48 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "7" thru_hole circle
			(at 16.02 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(J1-GPCLK0{slash}GPIO04-Pad7)")
			(pinfunction "GPCLK0/GPIO04")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole circle
			(at 16.02 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(J1-GPIO14{slash}UART_TXD-Pad8)")
			(pinfunction "GPIO14/UART_TXD")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" thru_hole circle
			(at 18.56 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 18.56 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(J1-GPIO15{slash}UART_RXD-Pad10)")
			(pinfunction "GPIO15/UART_RXD")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" thru_hole circle
			(at 21.1 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(J1-GPIO17{slash}SPI1_~{CE1}-Pad11)")
			(pinfunction "GPIO17/SPI1_~{CE1}")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" thru_hole circle
			(at 21.1 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "unconnected-(J1-GPIO18{slash}SPI1_~{CE0}{slash}PCM_CLK{slash}PWM0-Pad12)")
			(pinfunction "GPIO18/SPI1_~{CE0}/PCM_CLK/PWM0")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole circle
			(at 23.64 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(J1-GPIO27{slash}SDIO_DAT3-Pad13)")
			(pinfunction "GPIO27/SDIO_DAT3")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" thru_hole circle
			(at 23.64 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 26.18 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J1-GPIO22{slash}SDIO_CLK-Pad15)")
			(pinfunction "GPIO22/SDIO_CLK")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" thru_hole circle
			(at 26.18 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(J1-GPIO23{slash}SDIO_CMD-Pad16)")
			(pinfunction "GPIO23/SDIO_CMD")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" thru_hole circle
			(at 28.72 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(J1-3V3-Pad1)")
			(pinfunction "3V3")
			(pintype "passive+no_connect")
		)
		(pad "18" thru_hole circle
			(at 28.72 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "unconnected-(J1-GPIO24{slash}SDIO_DAT0-Pad18)")
			(pinfunction "GPIO24/SDIO_DAT0")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" thru_hole circle
			(at 31.26 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(J1-MOSI_SPI0{slash}GPIO10-Pad19)")
			(pinfunction "MOSI_SPI0/GPIO10")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" thru_hole circle
			(at 31.26 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 33.8 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(J1-MISO_SPI0{slash}GPIO09-Pad21)")
			(pinfunction "MISO_SPI0/GPIO09")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" thru_hole circle
			(at 33.8 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(J1-GPIO25{slash}SDIO_DAT1-Pad22)")
			(pinfunction "GPIO25/SDIO_DAT1")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" thru_hole circle
			(at 36.34 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(J1-SCLK_SPI0{slash}GPIO11-Pad23)")
			(pinfunction "SCLK_SPI0/GPIO11")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole circle
			(at 36.34 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(J1-~{CE0}_SPI0{slash}GPIO08-Pad24)")
			(pinfunction "~{CE0}_SPI0/GPIO08")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole circle
			(at 38.88 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at 38.88 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(J1-~{CE1}_SPI0{slash}GPIO07-Pad26)")
			(pinfunction "~{CE1}_SPI0/GPIO07")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" thru_hole circle
			(at 41.42 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(J1-ID_SD_I2C0{slash}GPIO00-Pad27)")
			(pinfunction "ID_SD_I2C0/GPIO00")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" thru_hole circle
			(at 41.42 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(J1-ID_SC_I2C0{slash}GPIO01-Pad28)")
			(pinfunction "ID_SC_I2C0/GPIO01")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" thru_hole circle
			(at 43.96 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "unconnected-(J1-GPCLK1{slash}GPIO05-Pad29)")
			(pinfunction "GPCLK1/GPIO05")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" thru_hole circle
			(at 43.96 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 46.5 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(J1-GPCLK2{slash}GPIO06-Pad31)")
			(pinfunction "GPCLK2/GPIO06")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" thru_hole circle
			(at 46.5 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "unconnected-(J1-GPIO12{slash}PWM0-Pad32)")
			(pinfunction "GPIO12/PWM0")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" thru_hole circle
			(at 49.04 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(J1-GPIO13{slash}PWM1-Pad33)")
			(pinfunction "GPIO13/PWM1")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" thru_hole circle
			(at 49.04 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "35" thru_hole circle
			(at 51.58 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J1-GPIO19{slash}SPI1_MISO{slash}PCM_FS-Pad35)")
			(pinfunction "GPIO19/SPI1_MISO/PCM_FS")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" thru_hole circle
			(at 51.58 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(J1-GPIO16{slash}SPI1_~{CE2}-Pad36)")
			(pinfunction "GPIO16/SPI1_~{CE2}")
			(pintype "bidirectional+no_connect")
		)
		(pad "37" thru_hole circle
			(at 54.12 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(J1-GPIO26{slash}SDIO_DAT2-Pad37)")
			(pinfunction "GPIO26/SDIO_DAT2")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" thru_hole circle
			(at 54.12 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "unconnected-(J1-GPIO20{slash}SPI1_MOSI{slash}PCM_DIN{slash}PWM1-Pad38)")
			(pinfunction "GPIO20/SPI1_MOSI/PCM_DIN/PWM1")
			(pintype "bidirectional+no_connect")
		)
		(pad "39" thru_hole circle
			(at 56.66 -51.21)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "40" thru_hole circle
			(at 56.66 -53.75)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(J1-GPIO21{slash}SPI1_SCLK{slash}PCM_DOUT-Pad40)")
			(pinfunction "GPIO21/SPI1_SCLK/PCM_DOUT")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.step"
			(offset
				(xyz 8.4 -51.2 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
		(model "C:/Users/blchase1/Downloads/RASPBERRY_PI_5_1.step"
			(offset
				(xyz 42 -28 21.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "Artemis_Awesome:Sparkfun Artemis Global Tracker"
		(layer "B.Cu")
		(at 106.8938 116.4146)
		(property "Reference" "Artemis1"
			(at 25.1062 -0.9146 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 25 1 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 26.5 3 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 2.6262 -60.9146)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.6262 -2.4946)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 48.3462 -60.9146)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 48.3462 -2.4946)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at 7.7062 -1.2246 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(Artemis1-AD12)")
			(pinfunction "AD12")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 10.2462 -1.2246 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "unconnected-(Artemis1-AD15{slash}RX-Pad2)")
			(pinfunction "AD15/RX")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 12.7862 -1.2246 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(Artemis1-AD11)")
			(pinfunction "AD11")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 15.3262 -1.2246 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(Artemis1-AD29)")
			(pinfunction "AD29")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 49.6162 -17.7346)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(Artemis1-GND-Pad5)")
			(pinfunction "GND")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 49.6162 -20.2746)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(Artemis1-COPI-Pad6)")
			(pinfunction "COPI")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 49.6162 -22.8146)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(Artemis1-CIPO-Pad7)")
			(pinfunction "CIPO")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 49.6162 -25.3546)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "unconnected-(Artemis1-SCK-Pad8)")
			(pinfunction "SCK")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at 49.6162 -27.8946)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "unconnected-(Artemis1-AD35-Pad9)")
			(pinfunction "AD35")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at 49.6162 -30.4346)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "unconnected-(Artemis1-D4-Pad10)")
			(pinfunction "D4")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at 49.6162 -32.9746)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "unconnected-(Artemis1-3V3-Pad11)")
			(pinfunction "3V3")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at 1.3562 -7.5746 180)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "Net-(Artemis1-AD32)")
			(pinfunction "AD32")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at 1.3562 -10.1146 180)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(Artemis1-AD43-Pad13)")
			(pinfunction "AD43")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at 1.3562 -12.6546 180)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "unconnected-(Artemis1-AD42-Pad14)")
			(pinfunction "AD42")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 1.3562 -15.1946 180)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "Net-(Artemis1-AD31)")
			(pinfunction "AD31")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 1.3562 -17.7346)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "unconnected-(Artemis1-GND-Pad16)")
			(pinfunction "GND")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 1.3562 -20.2746)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "+3V3")
			(pinfunction "3V3")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 1.3562 -22.8146)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "SDA")
			(pinfunction "SDA")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at 1.3562 -25.3546)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "SCL")
			(pinfunction "SCL")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at 1.3562 -43.1346 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(Artemis1-RST-Pad20)")
			(pinfunction "RST")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at 1.3562 -45.6746 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "GND")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at 1.3562 -48.2146 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "unconnected-(Artemis1-EN-Pad22)")
			(pinfunction "EN")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at 1.3562 -50.7546)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+5V")
			(pinfunction "VIN")
			(pintype "input")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 1.3562 -53.2946)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "unconnected-(Artemis1-VBUS-Pad24)")
			(pinfunction "VBUS")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at 1.3562 -55.8346 270)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(Artemis1-AD37-Pad25)")
			(pinfunction "AD37")
			(pintype "input+no_connect")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
		(model "C:/Users/blchase1/Downloads/Artemis_Global_Tracker.step"
			(offset
				(xyz 0.9 -50 8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Buzzer_Beeper:Buzzer_12x9.5RM7.6"
		(layer "B.Cu")
		(at 137.04 133 180)
		(descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
		(tags "buzzer")
		(property "Reference" "BZ1"
			(at 3.8 7.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "Buzzer"
			(at 3.8 -7.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Buzzer, polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Buzzer*")
		(sheetname "/")
		(sheetfile "WOMBAT.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at -0.01 3 0)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 3.8 4 0)
			(layer "B.Fab")
		)
		(fp_text user "+"
			(at -0.01 2.54 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(Artemis1-AD29)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.6 0 180)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 37.5 21.5)
		(end 172.5 161.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "LED2"
		(at 57.5 23 180)
		(layer "F.SilkS")
	)
	(gr_text "LED1"
		(at 50.5 23 180)
		(layer "F.SilkS")
	)
	(gr_text "RPM-GES5.0-10\nDC/DC Voltage Converter"
		(at 79 43.5 0)
		(layer "F.SilkS")
	)
	(gr_text "-+S"
		(at 96.5 27.5 180)
		(layer "F.SilkS")
	)
	(gr_text "18650 Batteries"
		(at 139.5 79 0)
		(layer "F.SilkS")
	)
	(gr_text "RTK2 GPS"
		(at 74 89 0)
		(layer "F.SilkS")
	)
	(gr_text "Servo2"
		(at 79.5 23 180)
		(layer "F.SilkS")
	)
	(gr_text "Camera"
		(at 66.5 23 180)
		(layer "F.SilkS")
	)
	(gr_text "Servo1"
		(at 92 23 180)
		(layer "F.SilkS")
	)
	(gr_text "28V"
		(at 109.5 25.5 180)
		(layer "F.SilkS")
	)
	(gr_text "WOMBAT PCB v1 | 07/10/2025\nWFF Balloon Program\nLogan Miller, Benjamin Chase, Sophia Reister, Jackson Thierfeldt"
		(at 50 140 0)
		(layer "F.SilkS")
	)
	(gr_text "-+"
		(at 67 27.5 180)
		(layer "F.SilkS")
	)
	(gr_text "-+S"
		(at 84 27.5 180)
		(layer "F.SilkS")
	)
	(gr_text "Raspberry Pi 5"
		(at 78.5 96.5 0)
		(layer "B.SilkS")
	)
	(gr_text "Buzzer :)"
		(at 120.5 133 0)
		(layer "B.SilkS")
	)
	(gr_text "Artemis Global Tracker"
		(at 139.5 86.5 0)
		(layer "B.SilkS")
	)
	(gr_text "Adafruit Feather LoRa"
		(at 136 39.5 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
