(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 12)
    (zones 0)
    (modules 4)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(SW1-Pad2)")
  (net 2 GND)
  (net 3 RST)
  (net 4 VCC)
  (net 5 SCK)
  (net 6 SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(SW1-Pad2)")
    (add_net RST)
    (add_net SCK)
    (add_net SDA)
    (add_net VCC)
  )
  (module crafting-labs:display_128x32_i2c (layer B.Cu) (tedit 605F0C4C)
    (at 167.64 81.915 270)
    (fp_text reference U1 (at 15.875 -5.08 270) (layer B.SilkS))
    (fp_text value display_128x32_i2c (at 11.43 6.985 270) (layer B.Fab))
    (fp_text user GND (at -15.875 -3.81 270) (layer B.SilkS))
    (fp_text user VCC (at -15.875 -1.27 270) (layer B.SilkS))
    (fp_text user SCL (at -15.875 1.27 270) (layer B.SilkS))
    (fp_text user SDA (at -15.875 3.81 270) (layer B.SilkS))
    (fp_text user "128x32 oled display" (at 4.445 0 270) (layer B.SilkS))
    (pad 4 thru_hole circle (at -18.415 3.81 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 SDA))
    (pad 3 thru_hole circle (at -18.415 1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SCK))
    (pad 2 thru_hole circle (at -18.415 -1.27 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 1 thru_hole circle (at -18.415 -3.81 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module crafting-labs:arduino_micro (layer F.Cu) (tedit 605F0BEB)
    (at 167.64 77.47)
    (fp_text reference U2 (at 0 13.97) (layer F.SilkS))
    (fp_text value Arduino_micro (at 0 0) (layer F.Fab))
    (fp_text user usb (at 0 -13.97) (layer F.SilkS))
    (fp_text user RAW (at 5.08 -13.97) (layer F.SilkS))
    (fp_text user GND (at 5.08 -11.43) (layer F.SilkS))
    (fp_text user RST (at 5.08 -8.89) (layer F.SilkS))
    (fp_text user VCC (at 5.08 -6.35) (layer F.SilkS))
    (fp_text user A3 (at 5.08 -3.81) (layer F.SilkS))
    (fp_text user A2 (at 5.08 -1.27) (layer F.SilkS))
    (fp_text user A1 (at 5.08 1.27) (layer F.SilkS))
    (fp_text user A0 (at 5.08 3.81) (layer F.SilkS))
    (fp_text user SCLK (at 5.08 6.35) (layer F.SilkS))
    (fp_text user MISO (at 5.08 8.89) (layer F.SilkS))
    (fp_text user MOSI (at 5.08 11.43) (layer F.SilkS))
    (fp_text user 10 (at 5.08 13.97) (layer F.SilkS))
    (fp_text user micro (at 0 7.62) (layer F.SilkS))
    (fp_text user Arduino (at 0 5.08) (layer F.SilkS))
    (fp_text user 9 (at -5.08 13.97) (layer F.SilkS))
    (fp_text user 8 (at -5.08 11.43) (layer F.SilkS))
    (fp_text user 7 (at -5.08 8.89) (layer F.SilkS))
    (fp_text user 6 (at -5.08 6.35) (layer F.SilkS))
    (fp_text user 5 (at -5.08 3.81) (layer F.SilkS))
    (fp_text user 4 (at -5.08 1.27) (layer F.SilkS))
    (fp_text user SCL (at -5.08 -1.27) (layer F.SilkS))
    (fp_text user SDA (at -5.08 -3.81) (layer F.SilkS))
    (fp_text user GND (at -5.08 -6.35) (layer F.SilkS))
    (fp_text user GND (at -5.08 -8.89) (layer F.SilkS))
    (fp_text user TXD (at -5.08 -11.43) (layer F.SilkS))
    (fp_text user RXD (at -5.08 -13.97) (layer F.SilkS))
    (pad RAW thru_hole circle (at 7.62 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad GND thru_hole circle (at 7.62 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad RST thru_hole circle (at 7.62 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RST))
    (pad VCC thru_hole circle (at 7.62 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 21 thru_hole circle (at 7.62 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 7.62 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 7.62 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 7.62 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 7.62 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 7.62 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 7.62 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 7.62 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -7.62 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -7.62 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -7.62 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -7.62 6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -7.62 3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -7.62 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(SW1-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SCK))
    (pad 2 thru_hole circle (at -7.62 -3.81) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 SDA))
    (pad GND thru_hole circle (at -7.62 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad GND thru_hole circle (at -7.62 -8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad RXD thru_hole circle (at -7.62 -11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad TXD thru_hole circle (at -7.62 -13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  )
  (module Button_Switch_SMD:SW_SPST_TL3305A (layer B.Cu) (tedit 5ABC3A97)
    (at 167.64 96.52)
    (descr https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf)
    (tags "TL3305 Series Tact Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 3.2) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -3.2) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at -3.6 -1.5) (size 1.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(SW1-Pad2)"))
    (pad 2 smd rect (at 3.6 -1.5) (size 1.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(SW1-Pad2)"))
    (pad 1 smd rect (at -3.6 1.5) (size 1.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.6 1.5) (size 1.6 1.4) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3305A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_TL3305A (layer F.Cu) (tedit 6044EF5F)
    (at 171.45 95.25)
    (descr https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf)
    (tags "TL3305 Series Tact Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -3.2) (layer F.SilkS))
    (fp_text value Reset (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 3.6 -1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.6 -1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.6 1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 RST))
    (pad 2 smd rect (at -3.6 1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 RST))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3305A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Crafting Labs" (at 167.64 93.345) (layer B.SilkS))
  (gr_text "Mute\nButton\nv0.2" (at 167.64 89.535) (layer B.SilkS))
  (gr_text "Crafting Labs" (at 167.64 99.695) (layer F.SilkS))
  (gr_text "Mute\nButton\nv0.2" (at 161.925 95.885) (layer F.SilkS))
  (gr_line (start 158.115 100.965) (end 158.115 62.23) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 177.165 100.965) (end 158.115 100.965) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 177.165 62.23) (end 177.165 100.965) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 158.115 62.23) (end 177.165 62.23) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.115 62.23) (xy 177.165 62.23) (xy 177.165 100.965) (xy 158.115 100.965)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.115 62.23) (xy 177.165 62.23) (xy 177.165 100.965) (xy 158.115 100.965)
      )
    )
  )
)
