(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 77)
    (zones 0)
    (modules 16)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J0-Pad0)")
  (net 2 "Net-(J0-Pad37)")
  (net 3 "Net-(J0-Pad36)")
  (net 4 "Net-(J0-Pad35)")
  (net 5 "Net-(J0-Pad34)")
  (net 6 "Net-(J0-Pad33)")
  (net 7 "Net-(J0-Pad32)")
  (net 8 "Net-(J0-Pad31)")
  (net 9 "Net-(J0-Pad30)")
  (net 10 "Net-(J0-Pad29)")
  (net 11 "Net-(J0-Pad28)")
  (net 12 "Net-(J0-Pad27)")
  (net 13 "Net-(J0-Pad26)")
  (net 14 "Net-(J0-Pad25)")
  (net 15 "Net-(J0-Pad24)")
  (net 16 "Net-(J0-Pad23)")
  (net 17 "Net-(J0-Pad22)")
  (net 18 "Net-(J0-Pad21)")
  (net 19 "Net-(J0-Pad20)")
  (net 20 GND)
  (net 21 "Net-(J0-Pad18)")
  (net 22 "Net-(J0-Pad17)")
  (net 23 "Net-(J0-Pad16)")
  (net 24 "Net-(J0-Pad15)")
  (net 25 "Net-(J0-Pad14)")
  (net 26 "Net-(J0-Pad13)")
  (net 27 "Net-(J0-Pad12)")
  (net 28 "Net-(J0-Pad11)")
  (net 29 "Net-(J0-Pad10)")
  (net 30 "Net-(J0-Pad9)")
  (net 31 "Net-(J0-Pad8)")
  (net 32 "Net-(J0-Pad7)")
  (net 33 "Net-(J0-Pad6)")
  (net 34 "Net-(J0-Pad5)")
  (net 35 "Net-(J0-Pad4)")
  (net 36 "Net-(J0-Pad3)")
  (net 37 "Net-(J0-Pad2)")
  (net 38 "Net-(J0-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J0-Pad0)")
    (add_net "Net-(J0-Pad10)")
    (add_net "Net-(J0-Pad11)")
    (add_net "Net-(J0-Pad12)")
    (add_net "Net-(J0-Pad13)")
    (add_net "Net-(J0-Pad14)")
    (add_net "Net-(J0-Pad15)")
    (add_net "Net-(J0-Pad16)")
    (add_net "Net-(J0-Pad17)")
    (add_net "Net-(J0-Pad18)")
    (add_net "Net-(J0-Pad19)")
    (add_net "Net-(J0-Pad2)")
    (add_net "Net-(J0-Pad20)")
    (add_net "Net-(J0-Pad21)")
    (add_net "Net-(J0-Pad22)")
    (add_net "Net-(J0-Pad23)")
    (add_net "Net-(J0-Pad24)")
    (add_net "Net-(J0-Pad25)")
    (add_net "Net-(J0-Pad26)")
    (add_net "Net-(J0-Pad27)")
    (add_net "Net-(J0-Pad28)")
    (add_net "Net-(J0-Pad29)")
    (add_net "Net-(J0-Pad3)")
    (add_net "Net-(J0-Pad30)")
    (add_net "Net-(J0-Pad31)")
    (add_net "Net-(J0-Pad32)")
    (add_net "Net-(J0-Pad33)")
    (add_net "Net-(J0-Pad34)")
    (add_net "Net-(J0-Pad35)")
    (add_net "Net-(J0-Pad36)")
    (add_net "Net-(J0-Pad37)")
    (add_net "Net-(J0-Pad4)")
    (add_net "Net-(J0-Pad5)")
    (add_net "Net-(J0-Pad6)")
    (add_net "Net-(J0-Pad7)")
    (add_net "Net-(J0-Pad8)")
    (add_net "Net-(J0-Pad9)")
  )
  (module Connector_Dsub:DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm (layer F.Cu) (tedit 59FEDEE2)
    (at 167.132 -74.93)
    (descr "37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 9.9mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 11.32mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "37-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 9.9mm mounting-holes-distance 63.5mm mounting-hole-offset 63.5mm")
    (fp_text reference J0 (at -24.93 -2.8) (layer F.SilkS))
    (fp_text value DB37 (at -24.93 20.81) (layer F.Fab))
    (fp_text user %R (at -24.93 16.225) (layer F.Fab))
    (pad 0 thru_hole circle (at 6.82 1.42) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J0-Pad0)"))
    (pad 0 thru_hole circle (at -56.68 1.42) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J0-Pad0)"))
    (pad 37 thru_hole circle (at -48.475 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J0-Pad37)"))
    (pad 36 thru_hole circle (at -45.705 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J0-Pad36)"))
    (pad 35 thru_hole circle (at -42.935 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J0-Pad35)"))
    (pad 34 thru_hole circle (at -40.165 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J0-Pad34)"))
    (pad 33 thru_hole circle (at -37.395 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J0-Pad33)"))
    (pad 32 thru_hole circle (at -34.625 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J0-Pad32)"))
    (pad 31 thru_hole circle (at -31.855 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J0-Pad31)"))
    (pad 30 thru_hole circle (at -29.085 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J0-Pad30)"))
    (pad 29 thru_hole circle (at -26.315 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J0-Pad29)"))
    (pad 28 thru_hole circle (at -23.545 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J0-Pad28)"))
    (pad 27 thru_hole circle (at -20.775 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J0-Pad27)"))
    (pad 26 thru_hole circle (at -18.005 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J0-Pad26)"))
    (pad 25 thru_hole circle (at -15.235 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J0-Pad25)"))
    (pad 24 thru_hole circle (at -12.465 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J0-Pad24)"))
    (pad 23 thru_hole circle (at -9.695 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J0-Pad23)"))
    (pad 22 thru_hole circle (at -6.925 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J0-Pad22)"))
    (pad 21 thru_hole circle (at -4.155 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J0-Pad21)"))
    (pad 20 thru_hole circle (at -1.385 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J0-Pad20)"))
    (pad 19 thru_hole circle (at -49.86 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J0-Pad19)"))
    (pad 18 thru_hole circle (at -47.09 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J0-Pad18)"))
    (pad 17 thru_hole circle (at -44.32 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J0-Pad17)"))
    (pad 16 thru_hole circle (at -41.55 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J0-Pad16)"))
    (pad 15 thru_hole circle (at -38.78 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J0-Pad15)"))
    (pad 14 thru_hole circle (at -36.01 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J0-Pad14)"))
    (pad 13 thru_hole circle (at -33.24 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J0-Pad13)"))
    (pad 12 thru_hole circle (at -30.47 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J0-Pad12)"))
    (pad 11 thru_hole circle (at -27.7 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J0-Pad11)"))
    (pad 10 thru_hole circle (at -24.93 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J0-Pad10)"))
    (pad 9 thru_hole circle (at -22.16 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J0-Pad9)"))
    (pad 8 thru_hole circle (at -19.39 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J0-Pad8)"))
    (pad 7 thru_hole circle (at -16.62 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J0-Pad7)"))
    (pad 6 thru_hole circle (at -13.85 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J0-Pad6)"))
    (pad 5 thru_hole circle (at -11.08 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J0-Pad5)"))
    (pad 4 thru_hole circle (at -8.31 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J0-Pad4)"))
    (pad 3 thru_hole circle (at -5.54 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J0-Pad3)"))
    (pad 2 thru_hole circle (at -2.77 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J0-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-37_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at -25.908 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J15 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 25 "Net-(J0-Pad14)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 19.812 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J14 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 31 "Net-(J0-Pad8)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 42.672 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J13 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 13 "Net-(J0-Pad26)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 65.532 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J12 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 32 "Net-(J0-Pad7)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 88.392 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J11 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 14 "Net-(J0-Pad25)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 111.252 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J10 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 33 "Net-(J0-Pad6)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 134.112 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J9 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 15 "Net-(J0-Pad24)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 156.972 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J8 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 34 "Net-(J0-Pad5)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 179.832 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J7 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 16 "Net-(J0-Pad23)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 202.692 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J6 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 35 "Net-(J0-Pad4)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 225.552 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J5 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 17 "Net-(J0-Pad22)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 248.412 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J4 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 36 "Net-(J0-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 271.272 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J3 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 18 "Net-(J0-Pad21)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 294.132 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J2 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 37 "Net-(J0-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 316.992 -95.25)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference J1 (at 0 4) (layer F.SilkS))
    (fp_text value BNC (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 19 "Net-(J0-Pad20)"))
    (pad 2 thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (pad 2 thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 20 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Labjack T7 breakout\n2019.05.04" (at 71.12 -69.596) (layer F.SilkS))
  (gr_line (start 327.152 -107.95) (end 327.152 -64.008) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -36.068 -107.95) (end -36.068 -64.008) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -36.068 -64.008) (end 327.152 -64.008) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -36.068 -107.95) (end 327.152 -107.95) (layer Edge.Cuts) (width 0.05))
  (zone (net 20) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -35.306 -107.188) (xy -35.306 -64.77) (xy 326.39 -64.77) (xy 326.39 -107.188)
      )
    )
  )
)
