(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 900)
    (zones 0)
    (modules 67)
    (nets 62)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 115.9002 80.2132)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 LA)
  (net 2 D0)
  (net 3 D1)
  (net 4 D2)
  (net 5 D3)
  (net 6 D4)
  (net 7 D5)
  (net 8 D6)
  (net 9 LB)
  (net 10 LC)
  (net 11 LD)
  (net 12 LE)
  (net 13 LF)
  (net 14 LG)
  (net 15 LH)
  (net 16 GND)
  (net 17 14)
  (net 18 15)
  (net 19 16)
  (net 20 17)
  (net 21 18)
  (net 22 19)
  (net 23 20)
  (net 24 21)
  (net 25 "Net-(D1-Pad2)")
  (net 26 "Net-(D10-Pad2)")
  (net 27 "Net-(D15-Pad2)")
  (net 28 "Net-(D22-Pad2)")
  (net 29 5V)
  (net 30 VCC)
  (net 31 SRCLK)
  (net 32 RCLK)
  (net 33 OE)
  (net 34 SER)
  (net 35 10)
  (net 36 11)
  (net 37 12)
  (net 38 22)
  (net 39 23)
  (net 40 "Net-(JP3-Pad2)")
  (net 41 "Net-(JP7-Pad2)")
  (net 42 "Net-(JP11-Pad2)")
  (net 43 "Net-(JP15-Pad2)")
  (net 44 BB)
  (net 45 BC)
  (net 46 BD)
  (net 47 BE)
  (net 48 BF)
  (net 49 BG)
  (net 50 BH)
  (net 51 "Net-(U1-Pad9)")
  (net 52 BA)
  (net 53 "Net-(U2-Pad9)")
  (net 54 "Net-(U3-Pad1)")
  (net 55 D7)
  (net 56 "Net-(U3-Pad18)")
  (net 57 "Net-(U3-Pad20)")
  (net 58 "Net-(JP2-Pad2)")
  (net 59 "Net-(JP6-Pad2)")
  (net 60 "Net-(JP10-Pad2)")
  (net 61 "Net-(JP14-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 10)
    (add_net 11)
    (add_net 12)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 18)
    (add_net 19)
    (add_net 20)
    (add_net 21)
    (add_net 22)
    (add_net 23)
    (add_net 5V)
    (add_net BA)
    (add_net BB)
    (add_net BC)
    (add_net BD)
    (add_net BE)
    (add_net BF)
    (add_net BG)
    (add_net BH)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net LA)
    (add_net LB)
    (add_net LC)
    (add_net LD)
    (add_net LE)
    (add_net LF)
    (add_net LG)
    (add_net LH)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(JP10-Pad2)")
    (add_net "Net-(JP11-Pad2)")
    (add_net "Net-(JP14-Pad2)")
    (add_net "Net-(JP15-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(JP7-Pad2)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad20)")
    (add_net OE)
    (add_net RCLK)
    (add_net SER)
    (add_net SRCLK)
    (add_net VCC)
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 219.4052 104.3432 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -7.5 180) (layer F.SilkS))
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-Pad9)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 D0))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 D1))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 D2))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 D3))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 OE))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 RCLK))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 SRCLK))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 D4))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 D5))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 D6))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 D7))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U3-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad20)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 188.9252 117.6782 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9C2D44)
    (at 220.0402 82.1182)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9C2D44)
    (at 220.0402 150.0632)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9C2D44)
    (at 128.6002 150.0632)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.6454 91.821)
    (fp_text reference D1 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D0))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.6454 101.94544)
    (fp_text reference D2 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 D1))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.6454 112.06988)
    (fp_text reference D3 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.6454 122.19432)
    (fp_text reference D4 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.6454 132.31876)
    (fp_text reference D5 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D4))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 134.6454 142.4432)
    (fp_text reference D6 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D5))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 117.777801 156.9212)
    (fp_text reference D7 (at -3.655601 -0.254) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D6))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 172.3136 91.821)
    (fp_text reference D8 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D0))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D10-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 172.3136 101.94544)
    (fp_text reference D9 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 D1))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 172.3136 112.06988)
    (fp_text reference D10 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D10-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 172.3136 122.19432)
    (fp_text reference D11 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 D3))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 172.3136 132.31876)
    (fp_text reference D12 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D4))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D10-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 172.3136 142.4432)
    (fp_text reference D13 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D5))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 155.488334 156.9212)
    (fp_text reference D14 (at -5.044134 -0.254) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D6))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D10-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 209.9818 91.821)
    (fp_text reference D15 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D0))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 209.9818 101.94544)
    (fp_text reference D16 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 D1))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 209.9818 112.06988)
    (fp_text reference D17 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 209.9818 122.19432)
    (fp_text reference D18 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 D3))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 209.9818 132.31876)
    (fp_text reference D19 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D4))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 209.9818 142.4432)
    (fp_text reference D20 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D5))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 193.198867 156.9212)
    (fp_text reference D21 (at -5.416667 0) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D6))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D15-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 247.65 91.821)
    (fp_text reference D22 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D22-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D0))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 247.65 101.94544)
    (fp_text reference D23 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 D1))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D22-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 247.65 112.06988)
    (fp_text reference D24 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D22-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 247.65 122.19432)
    (fp_text reference D25 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D22-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 247.65 132.31876)
    (fp_text reference D26 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D22-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 D4))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 247.65 142.4432)
    (fp_text reference D27 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 D5))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D22-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 230.909401 156.9212)
    (fp_text reference D28 (at -5.535201 0) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D22-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D6))
  )
  (module AOR_custom:PTA6043-2010CIB103 (layer F.Cu) (tedit 5C254BEA)
    (at 117.6528 116.9416 270)
    (fp_text reference RV1 (at 0.1016 -5.2324 270) (layer F.SilkS))
    (fp_text value R_POT (at 0 -5.5 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at -31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 2 thru_hole circle (at -36.75 1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 "Net-(JP3-Pad2)"))
    (pad 3 thru_hole circle (at 36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 GND))
  )
  (module AOR_custom:PTA6043-2010CIB103 (layer F.Cu) (tedit 5C254BEA)
    (at 155.363333 116.9416 270)
    (fp_text reference RV2 (at 0 5.5 270) (layer F.SilkS))
    (fp_text value R_POT (at 0 -5.5 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 2 thru_hole circle (at -36.75 1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 41 "Net-(JP7-Pad2)"))
    (pad 1 thru_hole rect (at -36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad "" np_thru_hole circle (at -32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
  )
  (module AOR_custom:PTA6043-2010CIB103 (layer F.Cu) (tedit 5C254BEA)
    (at 193.073866 116.9416 270)
    (fp_text reference RV3 (at 0 5.5 270) (layer F.SilkS))
    (fp_text value R_POT (at 0 -5.5 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at -31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 2 thru_hole circle (at -36.75 1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 42 "Net-(JP11-Pad2)"))
    (pad 3 thru_hole circle (at 36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 GND))
  )
  (module AOR_custom:PTA6043-2010CIB103 (layer F.Cu) (tedit 5C254BEA)
    (at 230.7844 116.9416 270)
    (fp_text reference RV4 (at 0 5.5 270) (layer F.SilkS))
    (fp_text value R_POT (at 0 -5.5 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 2 thru_hole circle (at -36.75 1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 43 "Net-(JP15-Pad2)"))
    (pad 1 thru_hole rect (at -36.75 -1.75 270) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad "" np_thru_hole circle (at -32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 32.6 4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -31.4 -4.2 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C9C2D44)
    (at 128.6002 82.1182)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 164.4142 96.9772 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Horizontal (layer B.Cu) (tedit 59DE217B)
    (at 127.3302 97.2312 180)
    (descr "Through hole angled IDC box header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at -2.032 -11.43 270) (layer B.SilkS))
    (fp_text value Conn_01x20 (at 6.105 -29.464 180) (layer B.Fab))
    (fp_text user %R (at 8.805 -11.43 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 5V))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 SRCLK))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 RCLK))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 OE))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 SER))
    (pad 8 thru_hole oval (at 2.54 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 10))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 11))
    (pad 10 thru_hole oval (at 2.54 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 12))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 14))
    (pad 12 thru_hole oval (at 2.54 -12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 15))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 16))
    (pad 14 thru_hole oval (at 2.54 -15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 17))
    (pad 15 thru_hole oval (at 0 -17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 18))
    (pad 16 thru_hole oval (at 2.54 -17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 19))
    (pad 17 thru_hole oval (at 0 -20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 20))
    (pad 18 thru_hole oval (at 2.54 -20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 21))
    (pad 19 thru_hole oval (at 0 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 22))
    (pad 20 thru_hole oval (at 2.54 -22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 23))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 145.1102 80.8482 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 145.1102 84.6582 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 145.1102 88.4682 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 125.2982 125.6792)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 30 VCC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 37 12) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 182.4482 137.3632 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP8 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 13 LF) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 59 "Net-(JP6-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 215.9762 126.9492 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP10 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 60 "Net-(JP10-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 10 LC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 183.9722 80.9752)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP11 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 42 "Net-(JP11-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 19 16) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 183.9722 84.7852)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP13 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 23 20) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 42 "Net-(JP11-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 228.1682 92.6592)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP17 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 24 21) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 43 "Net-(JP15-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 144.4752 103.7082 180)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6 180) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 BB))
    (pad 2 smd rect (at -2.7 -3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 BC))
    (pad 3 smd rect (at -2.7 -1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 BD))
    (pad 4 smd rect (at -2.7 -0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 BE))
    (pad 5 smd rect (at -2.7 0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 BF))
    (pad 6 smd rect (at -2.7 1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 BG))
    (pad 7 smd rect (at -2.7 3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 BH))
    (pad 8 smd rect (at -2.7 4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 9 smd rect (at 2.7 4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 11 smd rect (at 2.7 1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 SRCLK))
    (pad 12 smd rect (at 2.7 0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 RCLK))
    (pad 13 smd rect (at 2.7 -0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 OE))
    (pad 14 smd rect (at 2.7 -1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 SER))
    (pad 15 smd rect (at 2.7 -3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 BA))
    (pad 16 smd rect (at 2.7 -4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 181.3052 103.7082 180)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6 180) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 16 smd rect (at 2.7 -4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 15 smd rect (at 2.7 -3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 LA))
    (pad 14 smd rect (at 2.7 -1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad9)"))
    (pad 13 smd rect (at 2.7 -0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 OE))
    (pad 12 smd rect (at 2.7 0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 RCLK))
    (pad 11 smd rect (at 2.7 1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 SRCLK))
    (pad 10 smd rect (at 2.7 3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 VCC))
    (pad 9 smd rect (at 2.7 4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at -2.7 4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 7 smd rect (at -2.7 3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 LH))
    (pad 6 smd rect (at -2.7 1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 LG))
    (pad 5 smd rect (at -2.7 0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 LF))
    (pad 4 smd rect (at -2.7 -0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 LE))
    (pad 3 smd rect (at -2.7 -1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 LD))
    (pad 2 smd rect (at -2.7 -3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 LC))
    (pad 1 smd rect (at -2.7 -4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 LB))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 140.0302 137.9982 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 LA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 58 "Net-(JP2-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 117.6782 86.8172 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at 0 1.8 180) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 17 14) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 40 "Net-(JP3-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 143.8402 137.9982 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 58 "Net-(JP2-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 12 LE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 117.6782 90.3732 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP5 (at 0 1.8 180) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 180) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 40 "Net-(JP3-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers B.Cu B.Mask)
      (net 21 18) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 178.6382 137.3632 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP6 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 9 LB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 59 "Net-(JP6-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 153.4922 87.5792)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP7 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 18 15) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 41 "Net-(JP7-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5CB7F110)
    (at 153.4922 91.3892)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP9 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 41 "Net-(JP7-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 22 19) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 219.7862 126.9492 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP12 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 60 "Net-(JP10-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 14 LG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 237.3122 131.5212 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP14 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 11 LD) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 61 "Net-(JP14-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 228.1682 88.8492)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP15 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 20 17) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers B.Cu B.Mask)
      (net 43 "Net-(JP15-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 241.1222 131.5212 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP16 (at 0 -1.8 270) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 61 "Net-(JP14-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 15 LH) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.5702 143.7132)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 58 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 180.6702 142.4432)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(JP6-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 216.7382 132.2832)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 "Net-(D15-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 60 "Net-(JP10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 239.7252 137.3632 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 61 "Net-(JP14-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 "Net-(D22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Horizontal (layer B.Cu) (tedit 59DE1F47)
    (at 127.3302 131.2672 180)
    (descr "Through hole angled IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J5 (at -2.032 -5.08 270) (layer B.SilkS))
    (fp_text value Conn_01x10 (at 6.105 -16.51 180) (layer B.Fab))
    (fp_text user %R (at 8.805 -5.08 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 5V))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 SRCLK))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 RCLK))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 OE))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 SER))
    (pad 8 thru_hole oval (at 2.54 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 12))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 22))
    (pad 10 thru_hole oval (at 2.54 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 23))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text L (at 225.6282 89.1032) (layer B.SilkS))
  (gr_text R (at 225.6282 92.9132) (layer B.SilkS))
  (gr_text L (at 181.4322 81.2292) (layer B.SilkS))
  (gr_text R (at 181.4322 85.0392) (layer B.SilkS))
  (gr_text L (at 150.9522 87.5792) (layer B.SilkS))
  (gr_text R (at 150.9522 91.3892) (layer B.SilkS))
  (gr_text R (at 115.1382 90.6272) (layer B.SilkS))
  (gr_text L (at 115.1382 86.8172) (layer B.SilkS))
  (gr_text HIGH (at 128.6002 125.6792) (layer B.SilkS))
  (gr_text "PIN 12" (at 126.0602 123.9012) (layer B.SilkS))
  (gr_text GND (at 147.3962 86.5632) (layer B.SilkS))
  (gr_text GND (at 147.1422 82.7532) (layer B.SilkS))
  (gr_text 5V (at 140.5382 86.8172) (layer B.SilkS))
  (gr_text 5V (at 140.5382 83.0072) (layer B.SilkS))
  (gr_text L (at 236.0422 134.3152) (layer F.SilkS))
  (gr_text R (at 242.6462 134.3152) (layer F.SilkS))
  (gr_text L (at 214.9602 129.4892) (layer F.SilkS))
  (gr_text R (at 220.2942 129.4892) (layer F.SilkS))
  (gr_text R (at 183.9722 139.6492) (layer F.SilkS))
  (gr_text L (at 177.3682 139.6492) (layer F.SilkS))
  (gr_text R (at 145.3642 140.4112) (layer F.SilkS))
  (gr_text L (at 138.7602 140.4112) (layer F.SilkS))
  (gr_text "ACP3-E-SLD-PCB\nREV E, 4-18-2019" (at 188.2902 125.2982) (layer B.SilkS))
  (gr_text "ACP3-E-SLD-PCB\nREV E, 4-18-2019" (at 164.6682 115.5192 90) (layer F.SilkS))
  (gr_line (start 250.5202 78.3082) (end 250.5202 158.3182) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.0902 158.3182) (end 112.0902 78.3082) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.0902 78.3082) (end 250.5202 78.3082) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.0902 158.3182) (end 250.5202 158.3182) (layer Edge.Cuts) (width 0.15))
  (zone (net 16) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.0902 78.3082) (xy 250.5202 78.3082) (xy 250.5202 158.3182) (xy 112.0902 158.3182)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.0902 78.3082) (xy 250.5202 78.3082) (xy 250.5202 158.3182) (xy 112.0902 158.3182)
      )
    )
  )
)
