(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 210)
    (no_connects 11)
    (area 135.712999 75.641999 199.059001 116.255001)
    (thickness 1.6002)
    (drawings 7)
    (tracks 347)
    (zones 0)
    (modules 25)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.925 0.925)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 97.74 106.71)
    (grid_origin 97.79 106.68)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (gerberprecision 5)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/rfid/))
  )
  (net 0 "")
  (net 1 /VMID)
  (net 2 GNDREF)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(C10-Pad2)")
  (net 8 +3V3)
  (net 9 "Net-(R2-Pad2)")
  (net 10 /TX1)
  (net 11 /TX2)
  (net 12 /RX)
  (net 13 "Net-(D4-Pad2)")
  (net 14 /UART_TX)
  (net 15 /UART_RX)
  (net 16 /SDB)
  (net 17 /SDA)
  (net 18 /SCL)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SDB)
    (add_net /TX1)
    (add_net /TX2)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net /VMID)
    (add_net GNDREF)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C25-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C30-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad3)")
    (add_net "Net-(D10-Pad4)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad3)")
    (add_net "Net-(D11-Pad4)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D12-Pad3)")
    (add_net "Net-(D12-Pad4)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D13-Pad3)")
    (add_net "Net-(D13-Pad4)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad3)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad3)")
    (add_net "Net-(D5-Pad4)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad3)")
    (add_net "Net-(D6-Pad4)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad3)")
    (add_net "Net-(D7-Pad4)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad3)")
    (add_net "Net-(D8-Pad4)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad3)")
    (add_net "Net-(D9-Pad4)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R8-Pad1)")
  )
  (module rfid-reader-components:IDC_Header_SMD_10pins (layer B.Cu) (tedit 57A0F63C)
    (at 192.88 86.72 180)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P1 (at 5.08 9.652 180) (layer B.SilkS))
    (fp_text value CONN_02X05 (at 5.08 -3.191 180) (layer B.Fab))
    (pad 1 smd oval (at 0 0 180) (size 0.89 4.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 0 6.5 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 16 /SDB))
    (pad 3 smd rect (at 2.54 0 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 18 /SCL))
    (pad 4 smd rect (at 2.54 6.5 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 8 +3V3))
    (pad 5 smd rect (at 5.08 0 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 17 /SDA))
    (pad 6 connect rect (at 5.08 6.5 180) (size 0.89 4.8) (layers B.Cu B.Mask)
      (net 2 GNDREF))
    (pad 7 smd rect (at 7.62 0 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GNDREF))
    (pad 8 smd rect (at 7.62 6.5 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 14 /UART_TX))
    (pad 9 smd rect (at 10.16 0 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 15 /UART_RX))
    (pad 10 smd rect (at 10.16 6.5 180) (size 0.89 4.8) (layers B.Cu B.Paste B.Mask)
      (net 8 +3V3))
  )
  (module Inductors:Inductor_1212 (layer F.Cu) (tedit 57A3A86A)
    (at 178.79 91.18 180)
    (attr smd)
    (fp_text reference L1 (at 4.11 0.07 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 -2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.75 0 180) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX1))
    (pad 2 smd rect (at 1.75 0 180) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_1212 (layer F.Cu) (tedit 57A3AAEC)
    (at 178.79 105.68 180)
    (attr smd)
    (fp_text reference L2 (at 4.16 0.01 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 -2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.75 0 180) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /TX2))
    (pad 2 smd rect (at 1.75 0 180) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5428D7CB)
    (at 152.265 107.63)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference SYM (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen_07Jul2012 (at 0.30988 6.56082) (layer F.SilkS) hide)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5789132E)
    (at 180.483 99.798 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.302 0 180) (layer F.SilkS))
    (fp_text value 68n (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /VMID))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A3A868)
    (at 178.79 94.68)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.3 -0.05) (layer F.SilkS))
    (fp_text value 51p (at 3.175 2.54) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A3A872)
    (at 178.79 102.68 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.3 0 180) (layer F.SilkS))
    (fp_text value 51p (at -3.175 2.54 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A3AAF2)
    (at 191.44 108.73)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -1.62 -1.61) (layer F.SilkS))
    (fp_text value 27p (at 1.905 1.905) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A3AAE8)
    (at 184.215 108.78 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.095 1.55 180) (layer F.SilkS))
    (fp_text value 27p (at -1.905 -1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 578912A7)
    (at 167.894 92.329)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -3.683 0) (layer F.SilkS))
    (fp_text value 51p (at -3.175 2.54) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 578912B6)
    (at 167.767 99.441)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.683 0) (layer F.SilkS))
    (fp_text value 51p (at -3.175 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 578912A9)
    (at 167.894 89.916)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.683 0) (layer F.SilkS))
    (fp_text value 150p (at -3.175 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 578912BE)
    (at 167.767 101.854 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 3.683 0 180) (layer F.SilkS))
    (fp_text value 150p (at 3.175 2.54 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 578912A3)
    (at 167.894 94.742)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -4.191 0) (layer F.SilkS))
    (fp_text value 68n (at 3.175 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57A3A85B)
    (at 190.691 92.265 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at -3.579 0.145 180) (layer F.SilkS))
    (fp_text value LED (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57A3A858)
    (at 190.691 94.932)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.379 0.038) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57A3A865)
    (at 185.23 93.662 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 1.27 1.462 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57A3A870)
    (at 180.61 97.512 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.39 -0.058 180) (layer F.SilkS))
    (fp_text value 820 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /VMID))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 578912A0)
    (at 167.767 97.155)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.683 0) (layer F.SilkS))
    (fp_text value 560 (at -3.175 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 5789133D)
    (at 187.94114 112.93 180)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference Y1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 27.120MHz (at -7.62 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0 180) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 4.84886 0 180) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model Crystals.3dshapes/Q_49U3HMS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 57A3AACA)
    (at 176.84 113.03)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at -2.54 14.2) (layer F.SilkS))
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 57A3AB2C)
    (at 142.865 84.08)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (fp_text reference REF** (at -1.875 43.82) (layer F.SilkS))
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A3A84D)
    (at 195.54 105.68 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 1.93 90) (layer F.SilkS))
    (fp_text value .1u (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 57A3A841)
    (at 195.54 100.029 270)
    (attr smd)
    (fp_text reference C16 (at -0.019 -1.92 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module rfid-reader-components:QFN_32 (layer F.Cu) (tedit 0)
    (at 189.29 102.18 270)
    (fp_text reference U1 (at 0 -5.95 270) (layer F.SilkS))
    (fp_text value RC522 (at 0 5.95 270) (layer F.Fab))
    (pad 1 smd oval (at -2.857 -1.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 2 smd oval (at -2.857 -1.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 3 smd oval (at -2.857 -0.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 4 smd oval (at -2.857 -0.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 5 smd oval (at -2.857 0.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 6 smd oval (at -2.857 0.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (pad 7 smd oval (at -2.857 1.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd oval (at -2.857 1.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd oval (at -1.75 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd oval (at -1.25 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 11 smd oval (at -0.75 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX1))
    (pad 12 smd oval (at -0.25 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 13 smd oval (at 0.25 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /TX2))
    (pad 14 smd oval (at 0.75 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (pad 15 smd oval (at 1.25 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 16 smd oval (at 1.75 2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VMID))
    (pad 17 smd oval (at 2.857 1.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX))
    (pad 18 smd oval (at 2.857 1.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd oval (at 2.857 0.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd oval (at 2.857 0.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd oval (at 2.857 -0.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (pad 22 smd oval (at 2.857 -0.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 23 smd oval (at 2.857 -1.25) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd oval (at 2.857 -1.75) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /UART_RX))
    (pad 25 smd oval (at 1.75 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd oval (at 1.25 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd oval (at 0.75 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd oval (at 0.25 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd oval (at -0.25 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd oval (at -0.75 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd oval (at -1.25 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /UART_TX))
    (pad 32 smd oval (at -1.75 -2.857 270) (size 0.25 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDREF))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 135.763 75.692) (end 135.763 116.205) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 199.009 75.692) (end 135.763 75.692) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.763 116.205) (end 199.009 116.205) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 199.009 116.205) (end 199.009 75.692) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text playtrak.com.mx (at 152.34 103.33) (layer F.SilkS))
  (gr_text "RFID READER" (at 152.156 101.487) (layer F.SilkS))
  (gr_text PLAYTRAK (at 152.756 98.987) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.819712 84.88) (xy 148.415 84.88) (xy 148.415 81.88) (xy 169.819712 81.88)
      )
    )
  )
  (zone (net 2) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.154)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 198.29 115.68) (xy 174.79 115.68) (xy 174.79 76.18) (xy 198.29 76.18)
      )
    )
  )
  (zone (net 2) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.79 76.18) (xy 198.29 76.18) (xy 198.29 115.68) (xy 174.79 115.68)
      )
    )
  )
)
