<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="35.281" y1="54" x2="35.281" y2="33" width="0" layer="20"/>
<wire x1="17.25" y1="54" x2="35.281" y2="54" width="0" layer="20"/>
<wire x1="43.631" y1="12.5" x2="43.631" y2="34.5" width="0" layer="20"/>
<wire x1="28" y1="12.5" x2="43.631" y2="12.5" width="0" layer="20"/>
<wire x1="71" y1="34.5" x2="71" y2="61.5" width="0" layer="20"/>
<wire x1="17.25" y1="61.5" x2="17.25" y2="54" width="0" layer="20"/>
<wire x1="35.281" y1="33" x2="29" y2="33" width="0" layer="20"/>
<wire x1="22" y1="28" x2="22" y2="17" width="0" layer="20"/>
<wire x1="71" y1="61.5" x2="17.25" y2="61.5" width="0" layer="20"/>
<wire x1="22" y1="17" x2="28" y2="17" width="0" layer="20"/>
<wire x1="28" y1="17" x2="28" y2="12.5" width="0" layer="20"/>
<wire x1="71" y1="34.5" x2="65.5" y2="34.5" width="0" layer="20"/>
<wire x1="56" y1="34.5" x2="43.631" y2="34.5" width="0" layer="20"/>
<wire x1="22" y1="28" x2="29" y2="28" width="0" layer="20"/>
<wire x1="29" y1="28" x2="29" y2="33" width="0" layer="20"/>
<wire x1="56" y1="34.5" x2="56.5" y2="34" width="0" layer="20"/>
<wire x1="56.5" y1="34" x2="65" y2="34" width="0" layer="20"/>
<wire x1="65" y1="34" x2="65.5" y2="34.5" width="0" layer="20"/>
<text>SX</text>
<text>SY</text>
<text>CY</text>
<text>CX</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP10SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="pic18f25k22">
<description>PIC18F2xK22</description>
<packages>
<package name="SSOP28">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="switch-tact">
<description>&lt;b&gt;Diptronics THMD &amp; SMD tact switches&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;DTS-3: 3.5x6mm THMD tact switch
&lt;li&gt;DTS-6, DTS-64: 6x6mm THMD tact switch
&lt;li&gt;DTSM-3: 3.5x6mm SMD tact switch
&lt;li&gt;DTSM-6, DTSM-64: 6x6mm SMD tact switch
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DTS-6-2">
</package>
<package name="DTS-6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="-" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="100 nF"/>
<element name="CX" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="CY" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="D" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="IC1" library="pic18f25k22" package="SSOP28" value="PIC18F25K22-E/SS"/>
<element name="JP1" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R11" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R12" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R13" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R14" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R15" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R5" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R6" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R7" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R8" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="R9" library="SparkFun-Passives" package="0805" value="10k"/>
<element name="SX" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="SY" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="S1" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="S2" library="switch-tact" package="DTS-6" value="DTS-6"/>
<element name="S3" library="switch-tact" package="DTS-6" value="DTS-6"/>
<element name="S4" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="S5" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="S6" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="S7" library="switch-tact" package="DTS-6" value="DTS-6"/>
<element name="S8" library="switch-tact" package="DTS-6" value="DTS-6"/>
<element name="S9" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="S10" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="S11" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="S12" library="switch-tact" package="DTS-6-2" value="DTS-6-2"/>
<element name="+1" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="-1" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="-2" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="+2" library="testpad" package="TP10SQ" value="TPSQTP10SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="A">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="B">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="X">
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="9"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
</signal>
<signal name="Y">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="10"/>
<contactref element="S4" pad="2"/>
</signal>
<signal name="Z">
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="11"/>
<contactref element="S11" pad="2"/>
</signal>
<signal name="R">
<contactref element="R15" pad="2"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="L">
<contactref element="IC1" pad="15"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="DU">
<contactref element="IC1" pad="17"/>
<contactref element="R12" pad="2"/>
<contactref element="S5" pad="2"/>
</signal>
<signal name="DD">
<contactref element="IC1" pad="18"/>
<contactref element="R13" pad="2"/>
<contactref element="S6" pad="2"/>
</signal>
<signal name="DR">
<contactref element="IC1" pad="21"/>
<contactref element="R14" pad="2"/>
<contactref element="S7" pad="3"/>
<contactref element="S7" pad="4"/>
</signal>
<signal name="CX">
<contactref element="CX" pad="TP"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="CY">
<contactref element="CY" pad="TP"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="26"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="25"/>
</signal>
<signal name="RUMBLE">
<contactref element="IC1" pad="24"/>
</signal>
<signal name="DL">
<contactref element="IC1" pad="22"/>
<contactref element="R1" pad="2"/>
<contactref element="S8" pad="3"/>
<contactref element="S8" pad="4"/>
</signal>
<signal name="D">
<contactref element="D" pad="TP"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="3.3V">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="20"/>
<contactref element="+" pad="TP"/>
<contactref element="C1" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="+1" pad="TP"/>
<contactref element="+2" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="19"/>
<contactref element="IC1" pad="8"/>
<contactref element="-" pad="TP"/>
<contactref element="C1" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S3" pad="2"/>
<contactref element="S3" pad="1"/>
<contactref element="S4" pad="1"/>
<contactref element="S7" pad="2"/>
<contactref element="S7" pad="1"/>
<contactref element="S8" pad="2"/>
<contactref element="S8" pad="1"/>
<contactref element="S6" pad="1"/>
<contactref element="S12" pad="1"/>
<contactref element="S11" pad="1"/>
<contactref element="S5" pad="1"/>
<contactref element="-2" pad="TP"/>
<contactref element="-1" pad="TP"/>
<contactref element="S9" pad="1"/>
<contactref element="S10" pad="1"/>
</signal>
<signal name="PGD">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="PGC">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="MCLR">
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SX">
<contactref element="SX" pad="TP"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="SY">
<contactref element="SY" pad="TP"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="LT">
<contactref element="IC1" pad="16"/>
<contactref element="R11" pad="2"/>
<contactref element="S10" pad="2"/>
</signal>
<signal name="S">
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="12"/>
<contactref element="S12" pad="2"/>
</signal>
<signal name="RT">
<contactref element="IC1" pad="13"/>
<contactref element="R8" pad="2"/>
<contactref element="S9" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
