(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "unconnected-(J1-Pin_2-Pad2)")
  (net 3 "unconnected-(J1-Pin_3-Pad3)")
  (net 4 "UART_RX")
  (net 5 "UART_TX")
  (net 6 "UART_DTR")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (at 93.65 105 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "fluke-87v-clock-programming-adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.7434) (layer "F.SilkS"))
    (fp_text value "UART" (at 0 15.03 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "unconnected-(J1-Pin_2-Pad2)") (pinfunction "Pin_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "unconnected-(J1-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "UART_RX") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "UART_TX") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "UART_DTR") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 113.411 104.013)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.Fab"))
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Library:4mm_banana_plug" (layer "F.Cu")
    (at 109.525 95 180)
    (property "Sheetfile" "fluke-87v-clock-programming-adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP3" (at 0 -4.064 180 unlocked) (layer "F.Fab"))
    (fp_text value "GND" (at 0 -4.5 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.0254 0.0254 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 0 0 180) (size 6 13) (drill (offset 0 3.5)) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Library:4mm_banana_plug" (layer "F.Cu")
    (at 128.575 95 180)
    (property "Sheetfile" "fluke-87v-clock-programming-adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP4" (at 0 -4.064 180 unlocked) (layer "F.Fab"))
    (fp_text value "DTR" (at 0 -4.5 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.0254 0.0254 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 6 "UART_DTR") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 0 0 180) (size 6 13) (drill (offset 0 3.5)) (layers "F.Cu" "F.Mask")
      (net 6 "UART_DTR") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Library:4mm_banana_plug" (layer "F.Cu")
    (at 71.425 95 180)
    (property "Sheetfile" "fluke-87v-clock-programming-adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP1" (at 0 -4.064 180 unlocked) (layer "F.Fab"))
    (fp_text value "TX" (at 0 -4.5 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.0254 0.0254 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 5 "UART_TX") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 0 0 180) (size 6 13) (drill (offset 0 3.5)) (layers "F.Cu" "F.Mask")
      (net 5 "UART_TX") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Library:4mm_banana_plug" (layer "F.Cu")
    (at 90.475 95 180)
    (property "Sheetfile" "fluke-87v-clock-programming-adapter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr through_hole)
    (fp_text reference "TP2" (at 0 -4.064 180 unlocked) (layer "F.Fab"))
    (fp_text value "RX" (at 0 -4.5 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.0254 0.0254 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 4 "UART_RX") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 0 0 180) (size 6 13) (drill (offset 0 3.5)) (layers "F.Cu" "F.Mask")
      (net 4 "UART_RX") (pinfunction "1") (pintype "passive"))
  )
  (gr_line (start 67.945 84.582) (end 67.945 107.188)
    (layer "Edge.Cuts"))
  (gr_line (start 67.945 84.582) (end 131.953 84.582)
    (layer "Edge.Cuts"))
  (gr_line (start 131.953 84.582) (end 131.953 107.188)
    (layer "Edge.Cuts"))
  (gr_line (start 67.945 107.188) (end 131.953 107.188)
    (layer "Edge.Cuts"))
  (gr_text "miekush 2023" (at 125.8062 105.8926) (layer "B.Cu"))
  (gr_text "github.com/miekush" (at 100 101.5) (layer "B.SilkS"))
  (gr_text "hackster.io/miekush" (at 100 90) (layer "B.SilkS"))
  (gr_text "DTR" (at 106.35 103.2256 90) (layer "F.SilkS"))
  (gr_text "GND" (at 93.65 103.2256 90) (layer "F.SilkS"))
  (gr_text "Fluke 87V Alarm Clock\nProgramming Adapter" (at 70.5 105.5) (layer "F.SilkS"))
  (gr_text "TX" (at 103.81 103.2256 90) (layer "F.SilkS"))
  (gr_text "Designed By:\nMike Kushnerik" (at 129.5 105.5) (layer "F.SilkS"))
  (gr_text "RX" (at 101.27 103.2256 90) (layer "F.SilkS"))
)
