(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 55.88 147.32)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 131.51 123.44)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Hole 3/3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 66.74 133.6)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Hole 2/3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 66.74 108.2)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "Hole 1/3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 55.88 147.32) (end 150.8 147.32) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150.8 47.32) (end 150.8 147.32) (layer "Edge.Cuts") (width 0.1))
  (gr_line locked (start 55.88 147.32) (end 55.88 47.32) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 55.88 47.32) (end 150.8 47.32) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Denkovi DAEnetIP4 RELAY_5 \nEightwood Box Enclosure Adapter" (at 104.14 58.42) (layer "F.SilkS"))
)
