<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="68" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="53" y2="0" width="0" layer="20"/>
<wire x1="53" y1="0" x2="55" y2="2" width="0" layer="20" curve="90"/>
<wire x1="55" y1="2" x2="55" y2="68" width="0" layer="20"/>
<wire x1="55" y1="68" x2="53" y2="70" width="0" layer="20" curve="90"/>
<wire x1="53" y1="70" x2="2" y2="70" width="0" layer="20"/>
<wire x1="2" y1="70" x2="0" y2="68" width="0" layer="20" curve="90"/>
<text>diag</text>
<text>temp</text>
<text>LED</text>
<text>lever</text>
<text>level</text>
<text>prsr</text>
<text>JAW 2022-12</text>
<text>www.A791RL.com</text>
<text>espresso/HX/c</text>
</plain>
<libraries>
<library name="jaw-conn">
<packages>
<package name="HEADER-6X1-PTH">
</package>
<package name="HEADER-1X2-THM">
</package>
<package name="HEADER-3X2-PTH">
</package>
<package name="HEADER-3X1-PTH">
</package>
</packages>
</library>
<library name="jaw-ic">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="jaw">
<packages>
<package name="SMD1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SMD0603">
</package>
<package name="PUI-0540">
</package>
<package name="SMD0603D">
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
<package name="SOT-23-3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="jaw-conn" package="HEADER-6X1-PTH" value="HEADER-6X1-PTH">
<attribute name="NAME"/>
</element>
<element name="U1" library="jaw-ic" package="TQFP32-08" value="STM32F030/32-QFP32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN2" library="jaw-conn" package="HEADER-6X1-PTH" value="HEADER-6X1-PTH">
<attribute name="NAME"/>
</element>
<element name="CN1" library="jaw-conn" package="HEADER-1X2-THM" value="HEADER-1X2-THM">
<attribute name="NAME"/>
</element>
<element name="CN5" library="jaw-conn" package="HEADER-3X2-PTH" value="HEADER-3X2-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="jaw" package="SMD0603" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPK1" library="jaw" package="PUI-0540" value="SPKR-PUI-0540">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="jaw" package="SMD0603" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="jaw" package="SMD0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN3" library="jaw-conn" package="HEADER-3X2-PTH" value="HEADER-3X2-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN4" library="jaw-conn" package="HEADER-3X1-PTH" value="HEADER-3X1-PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="jaw" package="SMD0603D" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="jaw" package="SMD0603" value="0u1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="jaw" package="SMD0603" value="0u1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="jaw" package="SOD-323" value="DIODESOD-323">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SEL1" library="jaw-conn" package="HEADER-1X2-THM" value="HEADER-1X2-THM">
<attribute name="NAME"/>
</element>
<element name="SEL2" library="jaw-conn" package="HEADER-1X2-THM" value="HEADER-1X2-THM">
<attribute name="NAME"/>
</element>
<element name="R21" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="jaw" package="SMD0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="REG1" library="jaw" package="SOT-23-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="jaw" package="SMD0603" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jaw" package="SMD0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="jaw" package="SMD0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="jaw" package="SMD0603" value="0u1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="jaw" package="SMD0603" value="0u1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jaw" package="SMD0603" value="150k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jaw" package="SMD0603" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="jaw" package="SMD0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="jaw" package="SMD0603" value="0u1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="jaw" package="SMD0603" value="0u1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="jaw" package="SMD0603" value="150k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="jaw" package="SMD1210" value="100u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$3" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="C15" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="J1" pad="P$5"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="SPK1" pad="P1"/>
<contactref element="CN4" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="R22" pad="2"/>
<contactref element="REG1" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="C14" pad="1"/>
<contactref element="CN3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="P$6"/>
<contactref element="CN1" pad="P$2"/>
<contactref element="CN2" pad="P$4"/>
<contactref element="CN2" pad="P$3"/>
<contactref element="CN2" pad="P$2"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="32"/>
<contactref element="CN5" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="CN4" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="SEL1" pad="P$2"/>
<contactref element="SEL2" pad="P$2"/>
<contactref element="C9" pad="2"/>
<contactref element="REG1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="CN3" pad="6"/>
</signal>
<signal name="SWPRESSURE">
<contactref element="CN1" pad="P$1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="SWLEVER">
<contactref element="CN2" pad="P$1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="LEVEL">
<contactref element="CN2" pad="P$5"/>
<contactref element="Q1" pad="1"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="LEVELTANK">
<contactref element="CN2" pad="P$6"/>
<contactref element="Q2" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="RX">
<contactref element="CN5" pad="3"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="BOOT0">
<contactref element="CN5" pad="5"/>
<contactref element="U1" pad="31"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="TX">
<contactref element="CN5" pad="4"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="NRST">
<contactref element="CN5" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="ADCLEVELTANK">
<contactref element="U1" pad="7"/>
<contactref element="R8" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="IOPRESSURE">
<contactref element="U1" pad="6"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="IOLEVER">
<contactref element="U1" pad="9"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="SPK1" pad="P2"/>
<contactref element="Q5" pad="3"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R12" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="C28" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="P$1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="IOLAMP">
<contactref element="R13" pad="1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="P$2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="IOPUMP">
<contactref element="R14" pad="1"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="P$3"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="P$4"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="IOSOLEN">
<contactref element="R15" pad="1"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="IOHEATER">
<contactref element="R16" pad="1"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="IOLEDR">
<contactref element="R17" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="IOLEDG">
<contactref element="R18" pad="1"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="IOLEDB">
<contactref element="R19" pad="2"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="ADCTEMP">
<contactref element="U1" pad="11"/>
<contactref element="R21" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="LED1" pad="C"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="IOBEEP">
<contactref element="U1" pad="10"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="IOLED">
<contactref element="LED1" pad="A"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="18"/>
<contactref element="SEL1" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="25"/>
<contactref element="SEL2" pad="P$1"/>
</signal>
<signal name="N$17">
<contactref element="CN4" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="I2CSDA">
<contactref element="U1" pad="2"/>
</signal>
<signal name="I2CSCL">
<contactref element="U1" pad="3"/>
</signal>
<signal name="IOPROBE">
<contactref element="U1" pad="27"/>
<contactref element="R5" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="CN5" pad="1"/>
<contactref element="REG1" pad="3"/>
<contactref element="R23" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="ADCLEVEL">
<contactref element="R4" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="C11" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C13" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="CN3" pad="5"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="CN3" pad="3"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="CN3" pad="1"/>
<contactref element="R17" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
