(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 58)
    (no_connects 0)
    (area 162.924999 64.424999 182.575001 114.575001)
    (thickness 1.6)
    (drawings 33)
    (tracks 253)
    (zones 0)
    (modules 16)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6096)
    (via_drill 0.4064)
    (via_min_size 0.4064)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C104-Pad1)")
  (net 4 //ROMCS)
  (net 5 "Net-(D101-Pad2)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 /A1)
  (net 9 /A9)
  (net 10 /A8)
  (net 11 /A7)
  (net 12 /A6)
  (net 13 /A4)
  (net 14 /A2)
  (net 15 /A0)
  (net 16 /D0)
  (net 17 /D1)
  (net 18 /D5)
  (net 19 //WR)
  (net 20 "Net-(J2-Pad3)")
  (net 21 /A5)
  (net 22 /A3)
  (net 23 "Net-(J2-Pad6)")
  (net 24 "Net-(J2-Pad7)")
  (net 25 /A10)
  (net 26 "Net-(J2-Pad9)")
  (net 27 /D4)
  (net 28 /D3)
  (net 29 /D7)
  (net 30 /D2)
  (net 31 /D6)
  (net 32 /A11)
  (net 33 /A12)
  (net 34 /A13)
  (net 35 /A14)
  (net 36 /A15)
  (net 37 //MREQ)
  (net 38 //M1)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.3048)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net //M1)
    (add_net //MREQ)
    (add_net //ROMCS)
    (add_net //WR)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(D101-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad9)")
  )
  (net_class PWR ""
    (clearance 0.2032)
    (trace_width 0.4064)
    (via_dia 0.7112)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 165.1 76.2 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x14 (at 0 -35.35 180) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /A1))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /A9))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /A8))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /A7))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /A6))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /A4))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /A2))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /A0))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /D0))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /D1))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D5))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 177.5 71.75 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C101 (at -0.13 1.7 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 174.645 89.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C102 (at 0.145 1.535 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer F.Cu) (tedit 58CC8C08)
    (at 174.52 81.915 180)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C103 (at 0.02 1.915 180) (layer F.SilkS))
    (fp_text value 10uF/10V (at 0 2.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.375 0 180) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.375 0 180) (size 1.95 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A6A4AF0)
    (at 170 83.75 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C104 (at -4.25 0 90) (layer F.SilkS))
    (fp_text value 33pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MicroMELF_Hadsoldering (layer F.Cu) (tedit 5905DC0B)
    (at 172.55 66.675)
    (descr "Diode, MicroMELF, hand-soldering, http://www.vishay.com/docs/85597/bzm55-se.pdf")
    (tags "MicroMELF Diode")
    (attr smd)
    (fp_text reference D101 (at -0.05 1.5 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.6) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 2.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 //ROMCS))
    (pad 2 smd rect (at 1.45 0) (size 2.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D101-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MicroMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x14_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 180.34 76.2 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x14 (at 0 -35.35 180) (layer B.Fab))
    (fp_text user %R (at 0 -16.51 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 //WR))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /A5))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /A3))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /A10))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /D4))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /D3))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /D7))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /D2))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /D6))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x14_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 167.64 112.395 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J101 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Address (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /A11))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /A12))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /A13))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /A14))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /A15))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 165.1 66.675)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J102 (at 0 7.325) (layer F.SilkS))
    (fp_text value Control (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 //ROMCS))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 //M1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 //MREQ))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 174.545 85.725 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R101 (at 0 1.725 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C104-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 178.65 66.675 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R102 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D101-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-28W_7.5x17.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A6A4A3C)
    (at 172.72 100.965)
    (descr "28-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at -2.72 -9.965) (layer F.SilkS))
    (fp_text value 62256 (at 0.28 0.035 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /A14))
    (pad 2 smd rect (at -4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /A12))
    (pad 3 smd rect (at -4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /A1))
    (pad 4 smd rect (at -4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /A9))
    (pad 5 smd rect (at -4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /A8))
    (pad 6 smd rect (at -4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /A7))
    (pad 7 smd rect (at -4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /A6))
    (pad 8 smd rect (at -4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /A4))
    (pad 9 smd rect (at -4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /A2))
    (pad 10 smd rect (at -4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /A0))
    (pad 11 smd rect (at -4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /D0))
    (pad 12 smd rect (at -4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /D1))
    (pad 13 smd rect (at -4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /D5))
    (pad 14 smd rect (at -4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 4.7 8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /D6))
    (pad 16 smd rect (at 4.7 6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /D2))
    (pad 17 smd rect (at 4.7 5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /D7))
    (pad 18 smd rect (at 4.7 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /D3))
    (pad 19 smd rect (at 4.7 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /D4))
    (pad 20 smd rect (at 4.7 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C104-Pad1)"))
    (pad 21 smd rect (at 4.7 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /A10))
    (pad 22 smd rect (at 4.7 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C104-Pad1)"))
    (pad 23 smd rect (at 4.7 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /A11))
    (pad 24 smd rect (at 4.7 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /A3))
    (pad 25 smd rect (at 4.7 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /A5))
    (pad 26 smd rect (at 4.7 -5.715) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /A13))
    (pad 27 smd rect (at 4.7 -6.985) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 //WR))
    (pad 28 smd rect (at 4.7 -8.255) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-28W_7.5x17.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A6A367B)
    (at 171.8 73.66)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U101 (at -1.8 6.34) (layer F.SilkS))
    (fp_text value 74HC251 (at 0.285 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C104-Pad1)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D101-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 //MREQ))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /A15))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /A14))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /A13))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 //M1))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 //M1))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 177.5 77.39 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R103 (at 4.525 -0.935 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 //WR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ZX Speccy:logo-speccypl" (layer B.Cu) (tedit 0)
    (at 177 84.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module "ZX Speccy:fatla_eu" (layer B.Cu) (tedit 0)
    (at 168.275 104.14 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (gr_text v.0.1 (at 181.5 112.5 270) (layer B.Cu))
  (gr_text "Based on Wilf Rigter's design" (at 175 84 270) (layer B.SilkS))
  (gr_text "Internal 32KB RAM mapped 8K-40K" (at 167.5 82.55 90) (layer F.SilkS))
  (gr_text A15 (at 177.8 110.49) (layer F.SilkS))
  (gr_text A14 (at 175.26 110.49) (layer F.SilkS))
  (gr_text A13 (at 172.72 110.49) (layer F.SilkS))
  (gr_text A12 (at 170.18 110.49) (layer F.SilkS))
  (gr_text A11 (at 167.64 110.49) (layer F.SilkS))
  (gr_text /MREQ (at 167.005 71.755 90) (layer F.SilkS))
  (gr_text /M1 (at 167.64 69.215 90) (layer F.SilkS))
  (gr_text /ROMCS (at 167.005 66.675 90) (layer F.SilkS))
  (dimension 19.5 (width 0.3) (layer Dwgs.User)
    (gr_text "19.500 mm" (at 172.75 118.85) (layer Dwgs.User))
    (feature1 (pts (xy 182.5 114.5) (xy 182.5 120.2)))
    (feature2 (pts (xy 163 114.5) (xy 163 120.2)))
    (crossbar (pts (xy 163 117.5) (xy 182.5 117.5)))
    (arrow1a (pts (xy 182.5 117.5) (xy 181.373496 118.086421)))
    (arrow1b (pts (xy 182.5 117.5) (xy 181.373496 116.913579)))
    (arrow2a (pts (xy 163 117.5) (xy 164.126504 118.086421)))
    (arrow2b (pts (xy 163 117.5) (xy 164.126504 116.913579)))
  )
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50.000 mm" (at 186.35 89.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 182.5 114.5) (xy 187.7 114.5)))
    (feature2 (pts (xy 182.5 64.5) (xy 187.7 64.5)))
    (crossbar (pts (xy 185 64.5) (xy 185 114.5)))
    (arrow1a (pts (xy 185 114.5) (xy 184.413579 113.373496)))
    (arrow1b (pts (xy 185 114.5) (xy 185.586421 113.373496)))
    (arrow2a (pts (xy 185 64.5) (xy 184.413579 65.626504)))
    (arrow2b (pts (xy 185 64.5) (xy 185.586421 65.626504)))
  )
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50.000 mm" (at 158.15 89.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 163 64.5) (xy 156.8 64.5)))
    (feature2 (pts (xy 163 114.5) (xy 156.8 114.5)))
    (crossbar (pts (xy 159.5 114.5) (xy 159.5 64.5)))
    (arrow1a (pts (xy 159.5 64.5) (xy 160.086421 65.626504)))
    (arrow1b (pts (xy 159.5 64.5) (xy 158.913579 65.626504)))
    (arrow2a (pts (xy 159.5 114.5) (xy 160.086421 113.373496)))
    (arrow2b (pts (xy 159.5 114.5) (xy 158.913579 113.373496)))
  )
  (dimension 19.5 (width 0.3) (layer Dwgs.User)
    (gr_text "19.500 mm" (at 172.75 58.65) (layer Dwgs.User))
    (feature1 (pts (xy 182.5 64.5) (xy 182.5 57.3)))
    (feature2 (pts (xy 163 64.5) (xy 163 57.3)))
    (crossbar (pts (xy 163 60) (xy 182.5 60)))
    (arrow1a (pts (xy 182.5 60) (xy 181.373496 60.586421)))
    (arrow1b (pts (xy 182.5 60) (xy 181.373496 59.413579)))
    (arrow2a (pts (xy 163 60) (xy 164.126504 60.586421)))
    (arrow2b (pts (xy 163 60) (xy 164.126504 59.413579)))
  )
  (gr_line (start 163 114) (end 163 65.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.5 114.5) (end 163 114) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182 114.5) (end 163.5 114.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.5 114) (end 182 114.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.5 65) (end 182.5 114) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182 64.5) (end 182.5 65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164 64.5) (end 182 64.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163 65.5) (end 164 64.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163 64.5) (xy 182.5 64.5) (xy 182.5 114.5) (xy 163 114.5)
      )
    )
  )
)
