(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 45)
    (no_connects 0)
    (area 135.839999 63.42 246.74 137.210001)
    (thickness 1.6)
    (drawings 12)
    (tracks 108)
    (zones 0)
    (modules 28)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 1.2)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.6)
    (uvia_drill 0.2)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 3.6)
    (pad_drill 1.4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFECE6B)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 30VAC+)
  (net 7 30VAC-)
  (net 8 "Net-(D2-Pad2)")
  (net 9 "Net-(D3-Pad1)")
  (net 10 "Net-(J1-Pad1)")
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J3-Pad1)")
  (net 13 "Net-(J4-Pad1)")
  (net 14 "Net-(Q1-Pad2)")
  (net 15 "Net-(Q1-Pad1)")
  (net 16 "Net-(Q2-Pad2)")
  (net 17 "Net-(Q2-Pad1)")
  (net 18 "Net-(R1-Pad1)")
  (net 19 Onset)
  (net 20 "Net-(R2-Pad1)")
  (net 21 Hold)
  (net 22 dGND)
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 1.2)
    (via_drill 0.8)
    (uvia_dia 0.6)
    (uvia_drill 0.2)
    (add_net GND)
    (add_net Hold)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net Onset)
    (add_net dGND)
  )
  (net_class fatPower ""
    (clearance 0.4)
    (trace_width 2)
    (via_dia 4.8)
    (via_drill 3.2)
    (uvia_dia 2.4)
    (uvia_drill 0.2)
    (add_net 30VAC+)
    (add_net 30VAC-)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
  )
  (net_class power ""
    (clearance 0.4)
    (trace_width 1)
    (via_dia 2.4)
    (via_drill 1.6)
    (uvia_dia 1.2)
    (uvia_drill 0.4)
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
  )
  (module TO_SOT_Packages_THT:TO-220-2_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 161.29 84.455 90)
    (descr "TO-220-2, Vertical, RM 5.08mm")
    (tags "TO-220-2 Vertical RM 5.08mm")
    (fp_text reference D3 (at 2.54 -3.62 90) (layer F.SilkS))
    (fp_text value STTH30R061PI (at 2.54 3.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-2_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module GBPC-W:GBPC-W (layer F.Cu) (tedit 5AB94538)
    (at 225.425 88.265 225)
    (fp_text reference D1 (at 8 -3 225) (layer F.SilkS))
    (fp_text value D_Bridge_+-AA (at 9 2.5 225) (layer F.Fab))
    (fp_text user - (at 16 -2 225) (layer F.SilkS))
    (fp_text user AC (at 2 -2 225) (layer F.SilkS))
    (fp_text user AC (at 16 -16 225) (layer F.SilkS))
    (fp_text user ~ (at 16 -16 225) (layer F.SilkS))
    (fp_text user ~ (at 16 -16 225) (layer F.SilkS))
    (fp_text user + (at 2 -16 225) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 0 225) (size 2 2) (drill 1.07) (layers *.Cu *.Mask)
      (net 6 30VAC+))
    (pad 4 thru_hole circle (at 18 -18 225) (size 2 2) (drill 1.07) (layers *.Cu *.Mask)
      (net 7 30VAC-))
    (pad 2 thru_hole circle (at 18 0 225) (size 2 2) (drill 1.07) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 1 thru_hole circle (at 0 -18 225) (size 2 2) (drill 1.07) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 171.45 78.74 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.31 90) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 6.31 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 169.545 128.27 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 2.5 -6.31 270) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 6.31 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D35.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5ABB91AD)
    (at 189.865 82.55)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=35mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 35mm Electrolytic Capacitor")
    (fp_text reference C3 (at 0 -10.795) (layer F.SilkS))
    (fp_text value 4700µF (at 5 18.81) (layer F.Fab))
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 10 0) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D35.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D35.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5ABB91B3)
    (at 200.025 118.745 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=35mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 35mm Electrolytic Capacitor")
    (fp_text reference C4 (at 0 -8.89 180) (layer F.SilkS))
    (fp_text value 4700µF (at 5 18.81 180) (layer F.Fab))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D35.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-2_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 153.67 84.455 90)
    (descr "TO-220-2, Vertical, RM 5.08mm")
    (tags "TO-220-2 Vertical RM 5.08mm")
    (fp_text reference D2 (at 2.54 -3.62 90) (layer F.SilkS))
    (fp_text value STTH30R061PI (at 2.54 3.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-2_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 142.24 68.58)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J1 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad1)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 226.06 68.58)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J2 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 142.24 132.08)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J3 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad1)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 220.98 132.08)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J4 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 153.035 110.49 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value BS170 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 152.4 102.235 270)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 270) (layer F.SilkS))
    (fp_text value BS170 (at 1.27 2.79 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5ABA96B2)
    (at 148.59 114.935 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R1 (at 6.35 0 270) (layer F.SilkS))
    (fp_text value 180Ω (at 6 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 Onset))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5ABA969E)
    (at 148.59 97.155 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R2 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value 180Ω (at 7 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 Hold))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5ABA96AB)
    (at 173.99 105.41 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R3 (at 6.35 0 270) (layer F.SilkS))
    (fp_text value 180Ω (at 6.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5ABA96A8)
    (at 173.99 99.06 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R4 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value 180Ω (at 6.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5ABA96AE)
    (at 168.91 110.49 270)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R5 (at 6.35 0 270) (layer F.SilkS))
    (fp_text value 470Ω (at 6.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal (layer F.Cu) (tedit 5ABA96A6)
    (at 168.91 104.775 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference R6 (at 6.35 0 90) (layer F.SilkS))
    (fp_text value 470Ω (at 6.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 139.7 102.235)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value TLP523-2 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R2-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 dGND))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R1-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 dGND))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 153.67 92.075)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U2 (at 2.54 -3.62) (layer F.SilkS))
    (fp_text value LM7810ACT (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 153.67 122.555)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U3 (at 2.54 -3.62) (layer F.SilkS))
    (fp_text value LM7810ACT (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 161.29 103.505 90)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 2.54 -3.62 90) (layer F.SilkS))
    (fp_text value IRF1310NPBF (at 2.54 3.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 161.29 109.855 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q4 (at 2.54 -3.62 270) (layer F.SilkS))
    (fp_text value IRF1310NPBF (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 5AB99DB6)
    (at 140.97 92.075 180)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J5 (at -2.27 1.27 270) (layer F.SilkS))
    (fp_text value HOLD (at 2.27 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 dGND))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 21 Hold))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Samtec:SL-102-X-XX_1x02 (layer F.Cu) (tedit 590274D5)
    (at 140.97 122.555 180)
    (descr "Low profile, screw machine socket strip, through hole, 100mil / 2.54mm pitch")
    (tags "samtec socket strip tht single")
    (fp_text reference J6 (at -2.27 1.27 270) (layer F.SilkS))
    (fp_text value ONSET (at 2.27 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 dGND))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 2 2) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 Onset))
    (model ${KISYS3DMOD}/Connectors_Samtec.3dshapes/SL-102-X-XX_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_03x5.00mm_Vertical locked (layer F.Cu) (tedit 5AB9A26B)
    (at 240.665 131.445 90)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 03; pin pitch: 5.00mm; Vertical || order number: 1755529 12A || order number: 1924208 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x03_G_5.00mm")
    (zone_connect 1)
    (fp_text reference J7 (at 5 -5.8 90) (layer F.SilkS))
    (fp_text value "-30, G, 30" (at 5 4.8 90) (layer F.Fab))
    (fp_text user %R (at 5 -3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 30VAC-) (zone_connect 1))
    (pad 2 thru_hole oval (at 5 0 90) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 1))
    (pad 3 thru_hole oval (at 10 0 90) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 30VAC+) (zone_connect 1))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_03x5.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_02x5.00mm_Vertical (layer F.Cu) (tedit 5ABB9803)
    (at 156.21 71.755)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 02; pin pitch: 5.00mm; Vertical || order number: 1755516 12A || order number: 1924198 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x02_G_5.00mm")
    (fp_text reference Solenoid1 (at -6.35 -5.715) (layer F.SilkS) hide)
    (fp_text value 20Ω (at 2.5 4.8) (layer F.Fab))
    (fp_text user %R (at 3.5 -3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 5 0) (size 2 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_02x5.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 135.89 137.16) (end 137.16 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.89 63.5) (end 135.89 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 246.38 137.16) (end 137.16 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 246.38 63.5) (end 246.38 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.89 63.5) (end 246.38 63.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.89 63.5) (end 246.38 63.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "+ -" (at 145.415 121.285 270) (layer F.SilkS))
  (gr_text "+ -" (at 145.415 90.805 270) (layer F.SilkS))
  (gr_text "-30|G|+30\nVAC|N|VAC\n|D|" (at 230.505 126.365 90) (layer F.SilkS))
  (gr_text SOLENOID (at 159.385 64.77 180) (layer F.SilkS))
  (gr_text ONSET (at 137.795 121.285 270) (layer F.SilkS))
  (gr_text HOLD (at 137.795 90.805 270) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 246.38 63.5) (xy 246.38 137.16) (xy 135.89 137.16) (xy 135.89 63.5)
      )
    )
  )
)
