(kicad_pcb (version 20171130) (host pcbnew "(2018-02-05 revision d1a45d147)-makepkg")
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 693)
    (zones 0)
    (modules 67)
    (nets 84)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 107.475 123.85)
    (grid_origin 107.475 123.85)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5P)
  (net 2 +BATT)
  (net 3 CHGSTAT)
  (net 4 GND)
  (net 5 "Net-(IC1-Pad7)")
  (net 6 "Net-(IC1-Pad8)")
  (net 7 "Net-(IC2-Pad1)")
  (net 8 "Net-(IC2-Pad3)")
  (net 9 VBUS)
  (net 10 SW_B)
  (net 11 SW_A)
  (net 12 XL1)
  (net 13 XL2)
  (net 14 "Net-(U3-Pad15)")
  (net 15 +3V0)
  (net 16 "Net-(U3-Pad20)")
  (net 17 "Net-(U3-Pad21)")
  (net 18 "Net-(U3-Pad22)")
  (net 19 "Net-(U3-Pad23)")
  (net 20 LCD_DC)
  (net 21 NFC1)
  (net 22 NFC2)
  (net 23 LCD_CLK)
  (net 24 LCD_MOSI)
  (net 25 LCD_RST)
  (net 26 LCD_CS)
  (net 27 LCD_TE)
  (net 28 QSPI_~CS)
  (net 29 QSPI_DIO1)
  (net 30 QSPI_CLK)
  (net 31 QSPI_DIO0)
  (net 32 ~RESET)
  (net 33 QSPI_DIO2)
  (net 34 QSPI_DIO3)
  (net 35 SWCLK)
  (net 36 SWDIO)
  (net 37 MIC_BCLK)
  (net 38 MIC_SEL)
  (net 39 MIC_WS)
  (net 40 LED_DAT)
  (net 41 LED_POW)
  (net 42 "Net-(U3-Pad53)")
  (net 43 "Net-(U3-Pad54)")
  (net 44 ACC_INT)
  (net 45 GES_INT)
  (net 46 ACC_AG_NT)
  (net 47 MIC_DATAOUT)
  (net 48 "Net-(U3-Pad61)")
  (net 49 "Net-(U3-Pad62)")
  (net 50 IIC_SCL)
  (net 51 IIC_SDA)
  (net 52 D-)
  (net 53 D+)
  (net 54 "Net-(U5-Pad13)")
  (net 55 "Net-(U5-Pad12)")
  (net 56 "Net-(U5-Pad9)")
  (net 57 "Net-(R10-Pad1)")
  (net 58 "Net-(R11-Pad1)")
  (net 59 "Net-(R13-Pad1)")
  (net 60 "Net-(R12-Pad1)")
  (net 61 "Net-(C9-Pad2)")
  (net 62 "Net-(C10-Pad2)")
  (net 63 "Net-(Q2-Pad2)")
  (net 64 LCD_LEDA)
  (net 65 LCD_BL)
  (net 66 "Net-(C13-Pad1)")
  (net 67 "Net-(R16-Pad1)")
  (net 68 "Net-(R15-Pad1)")
  (net 69 "Net-(C17-Pad1)")
  (net 70 "Net-(U2-Pad4)")
  (net 71 "Net-(U7-Pad3)")
  (net 72 "Net-(D2-Pad4)")
  (net 73 "Net-(D3-Pad4)")
  (net 74 "Net-(J1-Pad4)")
  (net 75 "Net-(U3-Pad48)")
  (net 76 "Net-(U3-Pad60)")
  (net 77 "Net-(U3-Pad12)")
  (net 78 "Net-(U3-Pad52)")
  (net 79 "Net-(U3-Pad36)")
  (net 80 "Net-(U3-Pad37)")
  (net 81 "Net-(U3-Pad35)")
  (net 82 "Net-(U3-Pad59)")
  (net 83 "Net-(U3-Pad49)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V0)
    (add_net +5P)
    (add_net +BATT)
    (add_net ACC_AG_NT)
    (add_net ACC_INT)
    (add_net CHGSTAT)
    (add_net D+)
    (add_net D-)
    (add_net GES_INT)
    (add_net GND)
    (add_net IIC_SCL)
    (add_net IIC_SDA)
    (add_net LCD_BL)
    (add_net LCD_CLK)
    (add_net LCD_CS)
    (add_net LCD_DC)
    (add_net LCD_LEDA)
    (add_net LCD_MOSI)
    (add_net LCD_RST)
    (add_net LCD_TE)
    (add_net LED_DAT)
    (add_net LED_POW)
    (add_net MIC_BCLK)
    (add_net MIC_DATAOUT)
    (add_net MIC_SEL)
    (add_net MIC_WS)
    (add_net NFC1)
    (add_net NFC2)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC2-Pad1)")
    (add_net "Net-(IC2-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad23)")
    (add_net "Net-(U3-Pad35)")
    (add_net "Net-(U3-Pad36)")
    (add_net "Net-(U3-Pad37)")
    (add_net "Net-(U3-Pad48)")
    (add_net "Net-(U3-Pad49)")
    (add_net "Net-(U3-Pad52)")
    (add_net "Net-(U3-Pad53)")
    (add_net "Net-(U3-Pad54)")
    (add_net "Net-(U3-Pad59)")
    (add_net "Net-(U3-Pad60)")
    (add_net "Net-(U3-Pad61)")
    (add_net "Net-(U3-Pad62)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U5-Pad9)")
    (add_net "Net-(U7-Pad3)")
    (add_net QSPI_CLK)
    (add_net QSPI_DIO0)
    (add_net QSPI_DIO1)
    (add_net QSPI_DIO2)
    (add_net QSPI_DIO3)
    (add_net QSPI_~CS)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net SW_A)
    (add_net SW_B)
    (add_net VBUS)
    (add_net XL1)
    (add_net XL2)
    (add_net ~RESET)
  )
  (module Badge-PCB:SNT-4A (layer B.Cu) (tedit 5E1B6BA3)
    (at 114.959 87.327 270)
    (descr SNT-4A)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC2 (at 0.1375 -2.422) (layer B.SilkS))
    (fp_text value S-1000C32-I4T1U (at -22.024 -1.279 90) (layer B.SilkS) hide)
    (fp_text user %R (at 0.112334 -0.214 270) (layer B.Fab))
    (pad 4 smd rect (at -0.325 0.85 270) (size 0.3 0.52) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (pad 3 smd rect (at 0.325 0.85 270) (size 0.3 0.52) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(IC2-Pad3)"))
    (pad 2 smd rect (at 0.325 -0.83 270) (size 0.3 0.52) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.325 -0.83 270) (size 0.3 0.52) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(IC2-Pad1)"))
    (model ${KIPRJMOD}/3d_part_models/SNT-4A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:Crystal_SMD_MicroCrystal_CM9V-T1A-2pin_1.6x1.0mm (layer B.Cu) (tedit 5E1B6219)
    (at 129.944 103.604)
    (descr "SMD Crystal MicroCrystal CM9V-T1A series http://www.microcrystal.com/images/_Product-Documentation/01_TF_ceramic_Packages/01_Datasheet/CM9V-T1A.pdf, 1.6x1.0mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 1.9404 0.053) (layer B.SilkS))
    (fp_text value 32.768 (at 0 -1.7) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.6 0) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 XL1))
    (pad 1 smd rect (at -0.6 0) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 13 XL2))
    (model ${KIPRJMOD}/3d_part_models/xtal_CM9V-T1A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SON127P600X500X80-9N (layer B.Cu) (tedit 5E1B2FD9)
    (at 134.1704 85.5468 90)
    (fp_text reference U1 (at -3.9232 -1.5054 180) (layer B.SilkS))
    (fp_text value W25Q32JVSS (at 10.26471 -4.78919 90) (layer B.Fab))
    (pad 9 smd rect (at 0 0 90) (size 2.3 4) (layers B.Cu B.Mask))
    (pad 8 smd rect (at 2.335 1.905 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 7 smd rect (at 2.335 0.635 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 34 QSPI_DIO3))
    (pad 6 smd rect (at 2.335 -0.635 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 30 QSPI_CLK))
    (pad 5 smd rect (at 2.335 -1.905 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 29 QSPI_DIO1))
    (pad 4 smd rect (at -2.335 -1.905 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -2.335 -0.635 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 33 QSPI_DIO2))
    (pad 2 smd rect (at -2.335 0.635 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 31 QSPI_DIO0))
    (pad 1 smd rect (at -2.335 1.905 90) (size 1.06 0.42) (layers B.Cu B.Paste B.Mask)
      (net 28 QSPI_~CS))
    (model ${KIPRJMOD}/3d_part_models/SON127P600X500X80-9N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SW_SPST_TL3305A (layer F.Cu) (tedit 5E1B2045)
    (at 131.1224 116.4586)
    (descr https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf)
    (tags "TL3305 Series Tact Switch")
    (attr smd)
    (fp_text reference SW1 (at 5.969 -2.0574 -180) (layer F.SilkS))
    (fp_text value SW_DIP_x01 (at 0 3.2 -180) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd rect (at 3.6 -1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 SW_A))
    (pad 1 smd rect (at -3.6 -1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 SW_A))
    (pad 2 smd rect (at 3.6 1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -3.6 1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/TL3305AFxxxxG.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SW_SPST_TL3305A (layer F.Cu) (tedit 5E1B2045)
    (at 108.8466 116.484)
    (descr https://www.e-switch.com/system/asset/product_line/data_sheet/213/TL3305.pdf)
    (tags "TL3305 Series Tact Switch")
    (attr smd)
    (fp_text reference SW2 (at -6.0706 -2.3114 -180) (layer F.SilkS))
    (fp_text value SW_DIP_x01 (at 0 3.2 -180) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd rect (at 3.6 -1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 SW_B))
    (pad 1 smd rect (at -3.6 -1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 SW_B))
    (pad 2 smd rect (at 3.6 1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -3.6 1.5) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/TL3305AFxxxxG.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SM02B-SRSS-TB (layer B.Cu) (tedit 5E199609)
    (at 103.665 83.845 180)
    (descr <b>SM02B-SRSS-TB</b><br>)
    (fp_text reference J2 (at 3 0.5 270) (layer B.SilkS))
    (fp_text value SM02B-SRSS-TB (at -0.347136 -0.391283 180) (layer B.Fab))
    (pad 4 smd rect (at 1.8 -1.9 180) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.8 -1.9 180) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.5 1.975 180) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.5 1.975 180) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (model ${KIPRJMOD}/3d_part_models/JST_GH_SM02B-GHS-TB_1x02-1MP_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:APDS-9960 (layer F.Cu) (tedit 5E1B0984)
    (at 120.0988 116.5602 90)
    (attr smd)
    (fp_text reference U7 (at 1.9812 -0.0254) (layer F.SilkS))
    (fp_text value APDS-9960 (at 0.01778 2.39522 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.6985 -1.45288 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 51 IIC_SDA))
    (pad 2 smd rect (at 0.6985 -0.4826 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 45 GES_INT))
    (pad 3 smd rect (at 0.6985 0.4826 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U7-Pad3)"))
    (pad 4 smd rect (at 0.6985 1.45288 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U7-Pad3)"))
    (pad 5 smd rect (at -0.6985 1.45288 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V0))
    (pad 6 smd rect (at -0.6985 0.4826 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at -0.6985 -0.4826 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 50 IIC_SCL))
    (pad 8 smd rect (at -0.6985 -1.45288 90) (size 0.59944 0.71882) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C13-Pad1)"))
    (model ${KIPRJMOD}/3d_part_models/APDS_9962.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 134.165 111.41)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 1.448) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 51 IIC_SDA))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 140.241 84.226)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at -1.524 -1.016) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 35 SWCLK))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 140.241 86.766)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at -1.524 -1.016) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 36 SWDIO))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 127.033 86.512 270)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 1.6256 0.98298 270) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 1.45 270) (layer B.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1 1) (layers B.Cu B.Mask)
      (net 53 D+))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 124.493 86.512 270)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 1.45542 1.14554 270) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 1.45 270) (layer B.Fab))
    (pad 1 smd circle (at 0 0 270) (size 1 1) (layers B.Cu B.Mask)
      (net 52 D-))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 108.5418 84.353)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at -0.1016 -1.6002) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 15 +3V0))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 121.953 86.512)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at -1.19888 1.36144 90) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 9 VBUS))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 140.241 89.306)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at -1.524 -1.27) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 4 GND))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 118.524 78.257)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 1.5494 -0.5842 90) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 1 +5P))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 131.1986 111.440578)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 1.448) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 50 IIC_SCL))
  )
  (module Badge-PCB:Test_Point_Pad_d1.0mm (layer B.Cu) (tedit 59B53D91)
    (at 140.241 81.686)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at -2.032 -0.762) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 32 ~RESET))
  )
  (module Badge-PCB:SOT-23-5 (layer B.Cu) (tedit 5E19981F)
    (at 114.959 84.827 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -0.009 2.3155) (layer B.SilkS))
    (fp_text value S-1318 (at 0 -2.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(IC2-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (model ${KIPRJMOD}/3d_part_models/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SPH0645LM4H-B (layer B.Cu) (tedit 5E1B18F1)
    (at 139.2504 104.8254 270)
    (descr http://www.digikey.com/products/en?keywords=423-1405-1-ND)
    (solder_mask_margin 0.0254)
    (attr smd)
    (fp_text reference MIC1 (at 0 3.77 270) (layer B.SilkS))
    (fp_text value SPH0645LM4H-B (at 0 -2.76 270) (layer B.Fab))
    (fp_text user REF** (at 0 0.6 270) (layer B.Fab))
    (pad 6 smd rect (at 0 2.074 270) (size 0.6 0.522) (layers B.Cu B.Paste B.Mask)
      (net 47 MIC_DATAOUT))
    (pad 5 smd rect (at 0.9 2.074 270) (size 0.6 0.522) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 4 smd rect (at 0.9 1.252 270) (size 0.6 0.522) (layers B.Cu B.Paste B.Mask)
      (net 37 MIC_BCLK))
    (pad 2 smd rect (at -0.9 1.252 270) (size 0.6 0.522) (layers B.Cu B.Paste B.Mask)
      (net 38 MIC_SEL))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.325 0.325) (drill 0.325) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -0.9 2.074 270) (size 0.6 0.522) (layers B.Cu B.Paste B.Mask)
      (net 39 MIC_WS))
    (pad 3 smd circle (at 0.662 0 270) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd circle (at -0.662 0 270) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd circle (at 0 0.662 270) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd circle (at 0 -0.662 270) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/SPH0645LM4H_B009.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:PSON80P300X300X100-8N (layer F.Cu) (tedit 5E1B0BA8)
    (at 139.4028 109.6514)
    (solder_mask_margin 0.0254)
    (fp_text reference U6 (at 0.127 -2.4638) (layer F.SilkS))
    (fp_text value BME680 (at 6.621335 2.352976) (layer F.Fab))
    (pad 1 smd rect (at 1.2 -1.2) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.2 -0.4) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R15-Pad1)"))
    (pad 3 smd rect (at 1.2 0.4) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 51 IIC_SDA))
    (pad 4 smd rect (at 1.2 1.2) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 50 IIC_SCL))
    (pad 5 smd rect (at -1.2 1.22) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R16-Pad1)"))
    (pad 6 smd rect (at -1.2 0.4) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V0))
    (pad 7 smd rect (at -1.2 -0.4) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 8 smd rect (at -1.2 -1.2) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/BME680_cp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SOT-23 (layer B.Cu) (tedit 5E1997FF)
    (at 120.556 83.337 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0.4445 -2.413) (layer B.SilkS))
    (fp_text value DMG3414U (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5P))
    (model ${KIPRJMOD}/3d_part_models/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SOT-23 (layer B.Cu) (tedit 5E1997FF)
    (at 127.18794 107.35778)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.54254 1.0033) (layer B.SilkS))
    (fp_text value DMG3414U (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(Q2-Pad2)"))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 65 LCD_BL))
    (model ${KIPRJMOD}/3d_part_models/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SOT-23 (layer B.Cu) (tedit 5E1997FF)
    (at 107.565 79.03)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.3 -0.05 90) (layer B.SilkS))
    (fp_text value DMG3414U (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(C17-Pad1)"))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 41 LED_POW))
    (model ${KIPRJMOD}/3d_part_models/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 110.221 84.2 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 1.804 -0.048 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 112.9298 111.3782 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 2.5 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 112.9298 109.3782 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at 2.5 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 123.731 118.008)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 2.54 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 116.529278 116.888676 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 2.247078 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(C13-Pad1)"))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 112.9298 112.3782)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at -2.5 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 112.9298 110.3782)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at -2.5 0) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 112.221 84.2 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 1.804 -0.08 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 115.705 81.016 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at -1.8665 0.0285 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 129.3444 105.8414 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 2.04724 0.02286 270) (layer B.SilkS))
    (fp_text value 18pF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 13 XL2))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 115.705 77.016 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -1.8665 -0.0345 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +5P))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 132.3416 77.6728 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at -0.0762 -1.27 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(C17-Pad1)"))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 117.635 84.327 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 1.804 0 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 130.5382 105.8414 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 2.06248 0.00762 270) (layer B.SilkS))
    (fp_text value 18pF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 XL1))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0402 (layer B.Cu) (tedit 5E19835C)
    (at 111.221 84.2 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 1.804 -0.064 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 117.4298 107.8782 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 -1.5 90) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 119.4298 109.8782)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 2.5 0) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 119.4298 108.8782)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 2.5 0) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 140.6474 108.795 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0.055 -1.2324 90) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 138.082 111.335 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 0.125 -1.293 270) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 116.529278 118.158676 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 2.286 0 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 132.0876 109.2704 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 2.032 0 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 IIC_SCL))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 133.3576 109.2704 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at 2.032 0 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 IIC_SDA))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 109.865 79.49 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R20 (at -2.0574 0.0508 270) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 270) (layer B.Fab))
    (fp_text user %R (at 0 1.35 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 LED_POW))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 111.955 114.56 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 1.7526 -0.0508 180) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 SW_B))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 126.645 109.75 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0.0381 -1.14808 180) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 LCD_BL))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 134.285 114.56 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 1.8542 -0.0762 180) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 SW_A))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 119.475 80.85 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0.0874 1.0944 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5P))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 126.13892 104.34534 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -0.1143 1.26746 90) (layer B.SilkS))
    (fp_text value 33 (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 LCD_LEDA))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 113.205 77.016 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 1.7295 0.029 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(IC1-Pad8)"))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 113.205 81.016)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -1.64 0.054) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 CHGSTAT))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:R_0402 (layer B.Cu) (tedit 5E19951D)
    (at 119.4298 110.8782)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 2.5 0) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:PQFN24P43_350X300X102L35X23N (layer B.Cu) (tedit 5E1B0A3D)
    (at 116.4298 111.3782 270)
    (solder_mask_margin 0.0254)
    (fp_text reference U5 (at 2.9618 -0.0352) (layer B.SilkS))
    (fp_text value LSM9DS1 (at 9.46349 -2.52374 270) (layer B.Fab))
    (pad 18 smd rect (at 1.505 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 4 GND))
    (pad 17 smd rect (at 1.47 0.645 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 4 GND))
    (pad 16 smd rect (at 1.47 0.215 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 4 GND))
    (pad 15 smd rect (at 1.47 -0.215 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 4 GND))
    (pad 14 smd rect (at 1.47 -0.645 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 4 GND))
    (pad 13 smd rect (at 1.505 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 54 "Net-(U5-Pad13)"))
    (pad 12 smd rect (at 1.075 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 55 "Net-(U5-Pad12)"))
    (pad 11 smd rect (at 0.645 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 46 ACC_AG_NT))
    (pad 10 smd rect (at 0.215 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 44 ACC_INT))
    (pad 9 smd rect (at -0.215 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 56 "Net-(U5-Pad9)"))
    (pad 8 smd rect (at -0.645 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 57 "Net-(R10-Pad1)"))
    (pad 7 smd rect (at -1.075 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 58 "Net-(R11-Pad1)"))
    (pad 6 smd rect (at -1.505 -1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 59 "Net-(R13-Pad1)"))
    (pad 5 smd rect (at -1.47 -0.645 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 60 "Net-(R12-Pad1)"))
    (pad 4 smd rect (at -1.47 -0.215 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 51 IIC_SDA))
    (pad 3 smd rect (at -1.47 0.215 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 15 +3V0))
    (pad 2 smd rect (at -1.47 0.645 270) (size 0.53 0.28) (layers B.Cu B.Paste)
      (net 50 IIC_SCL))
    (pad 1 smd rect (at -1.505 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 15 +3V0))
    (pad 24 smd rect (at -1.075 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 61 "Net-(C9-Pad2)"))
    (pad 23 smd rect (at -0.645 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 15 +3V0))
    (pad 22 smd rect (at -0.215 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 15 +3V0))
    (pad 21 smd rect (at 0.215 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 62 "Net-(C10-Pad2)"))
    (pad 20 smd rect (at 0.645 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 4 GND))
    (pad 19 smd rect (at 1.075 1.225 270) (size 0.28 0.53) (layers B.Cu B.Paste)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/LGA-24L_3.5x3_0.43p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:RIGADO_BMD-340-A-R (layer B.Cu) (tedit 5E1B0DA2)
    (at 134 96.85 180)
    (solder_mask_margin 0.0254)
    (fp_text reference U3 (at -4.594315 5.909865) (layer B.SilkS))
    (fp_text value BMD-340-A-R (at -2.032 -6.39289) (layer B.Fab))
    (pad 68 smd rect (at 6.85 3.85 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 53 D+))
    (pad 67 smd rect (at 6.85 2.75 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 52 D-))
    (pad 66 smd rect (at 6.85 1.65 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (pad 65 smd rect (at 6.85 0.55 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 64 smd rect (at 6.85 -0.55 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 51 IIC_SDA))
    (pad 63 smd rect (at 6.85 -1.65 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 50 IIC_SCL))
    (pad 62 smd rect (at 6.85 -2.75 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U3-Pad62)"))
    (pad 61 smd rect (at 6.85 -3.85 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U3-Pad61)"))
    (pad 60 smd rect (at -1.75 2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(U3-Pad60)"))
    (pad 59 smd rect (at -0.65 2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(U3-Pad59)"))
    (pad 58 smd rect (at 0.45 2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 34 QSPI_DIO3))
    (pad 57 smd rect (at 1.55 2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 30 QSPI_CLK))
    (pad 56 smd rect (at 2.65 2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 29 QSPI_DIO1))
    (pad 55 smd rect (at 4.15 1.1 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 54 smd rect (at 4.15 0 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U3-Pad54)"))
    (pad 53 smd rect (at 4.15 -1.1 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U3-Pad53)"))
    (pad 52 smd rect (at 2.65 -2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(U3-Pad52)"))
    (pad 51 smd rect (at 1.55 -2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 44 ACC_INT))
    (pad 50 smd rect (at 0.45 -2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 46 ACC_AG_NT))
    (pad 49 smd rect (at -0.65 -2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(U3-Pad49)"))
    (pad 48 smd rect (at -1.75 -2.6 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(U3-Pad48)"))
    (pad 47 smd rect (at -2.85 -1.65 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 46 smd rect (at -2.85 1.65 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 45 smd rect (at -2.85 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 44 smd rect (at -2.3 3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 36 SWDIO))
    (pad 43 smd rect (at -1.75 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 35 SWCLK))
    (pad 42 smd rect (at -1.2 3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 40 LED_DAT))
    (pad 41 smd rect (at -0.65 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 28 QSPI_~CS))
    (pad 40 smd rect (at -0.1 3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 31 QSPI_DIO0))
    (pad 39 smd rect (at 0.45 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 32 ~RESET))
    (pad 38 smd rect (at 1 3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 33 QSPI_DIO2))
    (pad 37 smd rect (at 1.55 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(U3-Pad37)"))
    (pad 36 smd rect (at 2.1 3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(U3-Pad36)"))
    (pad 35 smd rect (at 2.65 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(U3-Pad35)"))
    (pad 34 smd rect (at 3.2 3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 41 LED_POW))
    (pad 33 smd rect (at 3.75 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 27 LCD_TE))
    (pad 32 smd rect (at 4.3 3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 26 LCD_CS))
    (pad 31 smd rect (at 4.85 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 25 LCD_RST))
    (pad 30 smd rect (at 5.95 4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 29 smd rect (at 5.95 3.3 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 28 smd rect (at 5.05 2.75 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 24 LCD_MOSI))
    (pad 27 smd rect (at 5.95 2.2 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 23 LCD_CLK))
    (pad 26 smd rect (at 5.05 1.65 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 22 NFC2))
    (pad 25 smd rect (at 5.95 1.1 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 21 NFC1))
    (pad 24 smd rect (at 5.05 0.55 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 20 LCD_DC))
    (pad 23 smd rect (at 5.95 0 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U3-Pad23)"))
    (pad 22 smd rect (at 5.05 -0.55 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U3-Pad22)"))
    (pad 21 smd rect (at 5.95 -1.1 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U3-Pad21)"))
    (pad 20 smd rect (at 5.05 -1.65 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U3-Pad20)"))
    (pad 19 smd rect (at 5.95 -2.2 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 SW_B))
    (pad 18 smd rect (at 5.05 -2.75 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 17 smd rect (at 5.95 -3.3 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 16 smd rect (at 5.95 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 15 smd rect (at 4.85 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U3-Pad15)"))
    (pad 14 smd rect (at 4.3 -3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 13 XL2))
    (pad 13 smd rect (at 3.75 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 XL1))
    (pad 12 smd rect (at 3.2 -3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(U3-Pad12)"))
    (pad 11 smd rect (at 2.65 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 45 GES_INT))
    (pad 10 smd rect (at 2.1 -3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 SW_A))
    (pad 9 smd rect (at 1.55 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 47 MIC_DATAOUT))
    (pad 8 smd rect (at 1 -3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 39 MIC_WS))
    (pad 7 smd rect (at 0.45 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 38 MIC_SEL))
    (pad 6 smd rect (at -0.1 -3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 37 MIC_BCLK))
    (pad 5 smd rect (at -0.65 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -1.2 -3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1.75 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -2.3 -3.5 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -2.85 -4.4 180) (size 0.5 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/BMD_340_A_R077.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:SON50P300X200X100-9N-D (layer B.Cu) (tedit 5E1B11BF)
    (at 114.705 79.016 180)
    (descr MCP73831T-2ACI/MC-1)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 3 0 270) (layer B.SilkS))
    (fp_text value MCP73831T-2ACI_MC (at 2.1754 14.856 270) (layer B.SilkS) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.75 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5P))
    (pad 2 smd rect (at -1.5 0.25 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5P))
    (pad 3 smd rect (at -1.5 -0.25 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad 4 smd rect (at -1.5 -0.75 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad 5 smd rect (at 1.5 -0.75 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 CHGSTAT))
    (pad 6 smd rect (at 1.5 -0.25 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 7 smd rect (at 1.5 0.25 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at 1.5 0.75 90) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at 0 0 90) (size 1.55 1.75) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/DFN8_2x3MC-L.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0805_2012Metric (layer B.Cu) (tedit 5E19838E)
    (at 124.179534 114.111819)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 3.048 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask)(roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask)(roundrect_rratio 0.25)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:C_0805_2012Metric (layer B.Cu) (tedit 5E19838E)
    (at 124.179534 116.270819)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 3.048 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask)(roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask)(roundrect_rratio 0.25)
      (net 15 +3V0))
    (model ${KIPRJMOD}/3d_part_models/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:D_SOD-323 (layer B.Cu) (tedit 5E199408)
    (at 123.604 83.35 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at -0.0632 1.651 270) (layer B.SilkS))
    (fp_text value D (at 0.1 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 1.85 90) (layer B.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 VBUS))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +5P))
    (model ${KIPRJMOD}/3d_part_models/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5E199436)
    (at 132.9512 78.7142)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D2 (at 4.6482 2.8702) (layer F.SilkS))
    (fp_text value SK6812 (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 40 LED_DAT))
    (pad 4 smd rect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(D2-Pad4)"))
    (pad 3 smd rect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C17-Pad1)"))
    (model ${KIPRJMOD}/3d_part_models/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5E199436)
    (at 107.4496 78.7396)
    (descr https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D3 (at -4.445 2.3622) (layer F.SilkS))
    (fp_text value SK6812 (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(D2-Pad4)"))
    (pad 4 smd rect (at -2.45 1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(D3-Pad4)"))
    (pad 3 smd rect (at -2.45 -1.6) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C17-Pad1)"))
    (model ${KIPRJMOD}/3d_part_models/LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:USB_Micro-B_Molex-105017-0001 (layer B.Cu) (tedit 5E1B19A1)
    (at 125 78.85)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J1 (at 5.475 -1.5) (layer B.SilkS))
    (fp_text value USB_B_Micro (at 0.3 -4.3375) (layer B.Fab))
    (fp_text user "PCB Edge" (at 0 -2.6875) (layer Dwgs.User))
    (fp_text user %R (at 0 -0.8875) (layer B.Fab))
    (pad 6 smd rect (at 1 -1.2375) (size 1.5 1.9) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 6 thru_hole circle (at -2.5 1.4625) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -0.65 1.4625) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 52 D-))
    (pad 1 smd rect (at -1.3 1.4625) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 1 +5P))
    (pad 5 smd rect (at 1.3 1.4625) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 4 smd rect (at 0.65 1.4625) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 1.4625) (size 0.4 1.35) (layers B.Cu B.Paste B.Mask)
      (net 53 D+))
    (pad 6 thru_hole circle (at 2.5 1.4625) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 6 smd rect (at -1 -1.2375) (size 1.5 1.9) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 6 thru_hole oval (at -3.5 -1.2375 180) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 6 thru_hole oval (at 3.5 -1.2375) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 6 smd rect (at 2.9 -1.2375) (size 1.2 1.9) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 6 smd rect (at -2.9 -1.2375) (size 1.2 1.9) (layers B.Cu B.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/3d_part_models/USB-MicroB_Molex_105017.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:0545482271 (layer B.Cu) (tedit 5E1994EE)
    (at 121.6937 97.48944 90)
    (descr 0545482271)
    (tags Connector)
    (attr smd)
    (fp_text reference TFT1 (at 0 0 -90) (layer B.SilkS))
    (fp_text value DISP_TFT_1.54IN_240X240_22P (at 38.039 -0.5268 -90) (layer B.SilkS) hide)
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -5.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 64 LCD_LEDA))
    (pad 2 smd rect (at -4.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -4.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -3.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 5 smd rect (at -3.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 6 smd rect (at -2.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 15 +3V0))
    (pad 7 smd rect (at -2.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 8 smd rect (at -1.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 9 smd rect (at -1.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 10 smd rect (at -0.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 11 smd rect (at -0.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 12 smd rect (at 0.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 13 smd rect (at 0.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 14 smd rect (at 1.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 15 smd rect (at 1.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 16 smd rect (at 2.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 20 LCD_DC))
    (pad 17 smd rect (at 2.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 23 LCD_CLK))
    (pad 18 smd rect (at 3.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 26 LCD_CS))
    (pad 19 smd rect (at 3.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 27 LCD_TE))
    (pad 20 smd rect (at 4.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 25 LCD_RST))
    (pad 21 smd rect (at 4.75 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 24 LCD_MOSI))
    (pad 22 smd rect (at 5.25 2.05 90) (size 0.3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 23 smd rect (at -7.525 0.15) (size 1.3 1.65) (layers B.Cu B.Paste B.Mask))
    (pad 24 smd rect (at 7.525 0.15) (size 1.3 1.65) (layers B.Cu B.Paste B.Mask))
    (model ${KIPRJMOD}/3d_part_models/0545482271.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Badge-PCB:pcb-top locked (layer F.Cu) (tedit 5E18C012)
    (at 96.9848 100.0248)
    (fp_text reference Ref** (at -2.54 3.9878) (layer F.SilkS) hide)
    (fp_text value Val** (at -2.4638 6.223) (layer F.SilkS) hide)
    (fp_line (start 41.956168 14.73113) (end 41.956168 14.73113) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.662121 14.760193) (end 41.956168 14.73113) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.382052 14.845278) (end 41.662121 14.760193) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.123834 14.983123) (end 41.382052 14.845278) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.895339 15.170469) (end 41.123834 14.983123) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.707993 15.398964) (end 40.895339 15.170469) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.570147 15.657181) (end 40.707993 15.398964) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.485062 15.93725) (end 40.570147 15.657181) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.455998 16.231297) (end 40.485062 15.93725) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.485062 16.525344) (end 40.455998 16.231297) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.570146 16.805413) (end 40.485062 16.525344) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.707992 17.063631) (end 40.570146 16.805413) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.895338 17.292127) (end 40.707992 17.063631) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.123833 17.479473) (end 40.895338 17.292127) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.382052 17.617318) (end 41.123833 17.479473) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.662121 17.702403) (end 41.382052 17.617318) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.956168 17.731466) (end 41.662121 17.702403) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.250214 17.702401) (end 41.956168 17.731466) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.530281 17.617315) (end 42.250214 17.702401) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.788498 17.479469) (end 42.530281 17.617315) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.016991 17.292123) (end 42.788498 17.479469) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.204336 17.063628) (end 43.016991 17.292123) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.342181 16.805411) (end 43.204336 17.063628) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.427265 16.525343) (end 43.342181 16.805411) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.456328 16.231297) (end 43.427265 16.525343) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.427264 15.937251) (end 43.456328 16.231297) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.34218 15.657184) (end 43.427264 15.937251) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.204335 15.398967) (end 43.34218 15.657184) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.016991 15.170472) (end 43.204335 15.398967) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.788497 14.983127) (end 43.016991 15.170472) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.530281 14.845281) (end 42.788497 14.983127) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.250214 14.760195) (end 42.530281 14.845281) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.956168 14.73113) (end 42.250214 14.760195) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.456128 14.73113) (end 4.456128 14.73113) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.162081 14.760194) (end 4.456128 14.73113) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.882013 14.845279) (end 4.162081 14.760194) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.623796 14.983124) (end 3.882013 14.845279) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.395301 15.17047) (end 3.623796 14.983124) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.207956 15.398965) (end 3.395301 15.17047) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.070111 15.657182) (end 3.207956 15.398965) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.985026 15.93725) (end 3.070111 15.657182) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.955962 16.231297) (end 2.985026 15.93725) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.985026 16.525344) (end 2.955962 16.231297) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.07011 16.805412) (end 2.985026 16.525344) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.207955 17.06363) (end 3.07011 16.805412) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.395301 17.292125) (end 3.207955 17.06363) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.623795 17.479471) (end 3.395301 17.292125) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.882013 17.617317) (end 3.623795 17.479471) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.162081 17.702402) (end 3.882013 17.617317) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.456128 17.731466) (end 4.162081 17.702402) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.750175 17.702402) (end 4.456128 17.731466) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.030243 17.617317) (end 4.750175 17.702402) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.288461 17.479471) (end 5.030243 17.617317) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.516955 17.292125) (end 5.288461 17.479471) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.704301 17.06363) (end 5.516955 17.292125) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.842146 16.805412) (end 5.704301 17.06363) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.92723 16.525344) (end 5.842146 16.805412) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.956294 16.231297) (end 5.92723 16.525344) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.92723 15.93725) (end 5.956294 16.231297) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.842145 15.657182) (end 5.92723 15.93725) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.7043 15.398965) (end 5.842145 15.657182) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.516955 15.17047) (end 5.7043 15.398965) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.28846 14.983124) (end 5.516955 15.17047) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.030243 14.845279) (end 5.28846 14.983124) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.750175 14.760194) (end 5.030243 14.845279) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.456128 14.73113) (end 4.750175 14.760194) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.62991 -12.983974) (end 10.62991 -12.983974) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.496277 -12.970582) (end 10.62991 -12.983974) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.371962 -12.932153) (end 10.496277 -12.970582) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.259584 -12.871306) (end 10.371962 -12.932153) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.161763 -12.790663) (end 10.259584 -12.871306) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.081119 -12.692842) (end 10.161763 -12.790663) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.020273 -12.580464) (end 10.081119 -12.692842) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 9.981844 -12.456148) (end 10.020273 -12.580464) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 9.968452 -12.322516) (end 9.981844 -12.456148) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 9.968452 7.285073) (end 9.968452 -12.322516) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 9.981844 7.418706) (end 9.968452 7.285073) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.020273 7.543021) (end 9.981844 7.418706) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.081119 7.655399) (end 10.020273 7.543021) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.161763 7.75322) (end 10.081119 7.655399) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.259584 7.833864) (end 10.161763 7.75322) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.371962 7.89471) (end 10.259584 7.833864) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.496277 7.933139) (end 10.371962 7.89471) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.62991 7.946531) (end 10.496277 7.933139) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 13.858655 7.946531) (end 10.62991 7.946531) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 13.992288 7.933139) (end 13.858655 7.946531) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.116603 7.89471) (end 13.992288 7.933139) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.228981 7.833864) (end 14.116603 7.89471) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.326802 7.75322) (end 14.228981 7.833864) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.407446 7.655399) (end 14.326802 7.75322) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.468292 7.543021) (end 14.407446 7.655399) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.506721 7.418706) (end 14.468292 7.543021) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.520113 7.285073) (end 14.506721 7.418706) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.520113 -12.322516) (end 14.520113 7.285073) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.506721 -12.456148) (end 14.520113 -12.322516) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.468292 -12.580464) (end 14.506721 -12.456148) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.407446 -12.692842) (end 14.468292 -12.580464) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.326802 -12.790663) (end 14.407446 -12.692842) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.228981 -12.871306) (end 14.326802 -12.790663) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 14.116603 -12.932153) (end 14.228981 -12.871306) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 13.992288 -12.970582) (end 14.116603 -12.932153) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 13.858655 -12.983974) (end 13.992288 -12.970582) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 10.62991 -12.983974) (end 13.858655 -12.983974) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.956168 -22.76839) (end 41.956168 -22.76839) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.802814 -22.760664) (end 41.956168 -22.76839) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.653886 -22.737954) (end 41.802814 -22.760664) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.372331 -22.650597) (end 41.653886 -22.737954) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.117532 -22.512347) (end 41.372331 -22.650597) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.895522 -22.329234) (end 41.117532 -22.512347) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.712332 -22.107287) (end 40.895522 -22.329234) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.573993 -21.852537) (end 40.712332 -22.107287) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.486538 -21.571011) (end 40.573993 -21.852537) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.463777 -21.422092) (end 40.486538 -21.571011) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.455998 -21.26874) (end 40.463777 -21.422092) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.485062 -20.974693) (end 40.455998 -21.26874) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.570147 -20.694624) (end 40.485062 -20.974693) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.707993 -20.436407) (end 40.570147 -20.694624) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 40.895339 -20.207912) (end 40.707993 -20.436407) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.123834 -20.020566) (end 40.895339 -20.207912) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.382052 -19.882721) (end 41.123834 -20.020566) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.662121 -19.797636) (end 41.382052 -19.882721) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.956168 -19.768573) (end 41.662121 -19.797636) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.250214 -19.797638) (end 41.956168 -19.768573) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.530281 -19.882724) (end 42.250214 -19.797638) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.788497 -20.02057) (end 42.530281 -19.882724) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.016991 -20.207915) (end 42.788497 -20.02057) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.204335 -20.43641) (end 43.016991 -20.207915) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.34218 -20.694627) (end 43.204335 -20.43641) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.427264 -20.974694) (end 43.34218 -20.694627) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.456328 -21.26874) (end 43.427264 -20.974694) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.448549 -21.422091) (end 43.456328 -21.26874) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.425788 -21.57101) (end 43.448549 -21.422091) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.338334 -21.852534) (end 43.425788 -21.57101) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.199996 -22.107284) (end 43.338334 -21.852534) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.016808 -22.32923) (end 43.199996 -22.107284) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.794799 -22.512344) (end 43.016808 -22.32923) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.540002 -22.650594) (end 42.794799 -22.512344) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.258448 -22.737953) (end 42.540002 -22.650594) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.109522 -22.760663) (end 42.258448 -22.737953) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.956168 -22.76839) (end 42.109522 -22.760663) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.456128 -22.76839) (end 4.456128 -22.76839) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.302774 -22.760664) (end 4.456128 -22.76839) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.153847 -22.737954) (end 4.302774 -22.760664) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.872292 -22.650596) (end 4.153847 -22.737954) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.617494 -22.512346) (end 3.872292 -22.650596) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.395484 -22.329233) (end 3.617494 -22.512346) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.212295 -22.107286) (end 3.395484 -22.329233) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.073957 -21.852536) (end 3.212295 -22.107286) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.986502 -21.57101) (end 3.073957 -21.852536) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.963741 -21.422092) (end 2.986502 -21.57101) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.955962 -21.26874) (end 2.963741 -21.422092) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.985026 -20.974693) (end 2.955962 -21.26874) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.070111 -20.694625) (end 2.985026 -20.974693) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.207956 -20.436408) (end 3.070111 -20.694625) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.395301 -20.207913) (end 3.207956 -20.436408) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.623796 -20.020567) (end 3.395301 -20.207913) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.882013 -19.882722) (end 3.623796 -20.020567) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.162081 -19.797637) (end 3.882013 -19.882722) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.456128 -19.768573) (end 4.162081 -19.797637) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.750175 -19.797637) (end 4.456128 -19.768573) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.030243 -19.882722) (end 4.750175 -19.797637) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.28846 -20.020567) (end 5.030243 -19.882722) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.516955 -20.207913) (end 5.28846 -20.020567) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.7043 -20.436408) (end 5.516955 -20.207913) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.842145 -20.694625) (end 5.7043 -20.436408) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.92723 -20.974693) (end 5.842145 -20.694625) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.956294 -21.26874) (end 5.92723 -20.974693) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.948515 -21.422092) (end 5.956294 -21.26874) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.925754 -21.57101) (end 5.948515 -21.422092) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.838299 -21.852536) (end 5.925754 -21.57101) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.699961 -22.107286) (end 5.838299 -21.852536) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.516772 -22.329233) (end 5.699961 -22.107286) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.294762 -22.512346) (end 5.516772 -22.329233) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 5.039964 -22.650596) (end 5.294762 -22.512346) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.758409 -22.737954) (end 5.039964 -22.650596) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.609482 -22.760664) (end 4.758409 -22.737954) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.456128 -22.76839) (end 4.609482 -22.760664) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.634738 -24.018443) (end 4.777554 -24.018443) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.949638 -24.002647) (end 41.634738 -24.018443) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.255237 -23.956271) (end 41.949638 -24.002647) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.550015 -23.880837) (end 42.255237 -23.956271) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.832452 -23.777862) (end 42.550015 -23.880837) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.101028 -23.648868) (end 42.832452 -23.777862) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.354223 -23.495374) (end 43.101028 -23.648868) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.590518 -23.3189) (end 43.354223 -23.495374) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.808392 -23.120967) (end 43.590518 -23.3189) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.006326 -22.903092) (end 43.808392 -23.120967) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.182799 -22.666797) (end 44.006326 -22.903092) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.336293 -22.413602) (end 44.182799 -22.666797) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.465287 -22.145026) (end 44.336293 -22.413602) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.568262 -21.862589) (end 44.465287 -22.145026) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.643696 -21.567811) (end 44.568262 -21.862589) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.690072 -21.262212) (end 44.643696 -21.567811) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.705868 -20.947311) (end 44.690072 -21.262212) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.705868 15.90987) (end 44.705868 -20.947311) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.690072 16.224777) (end 44.705868 15.90987) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.643696 16.530392) (end 44.690072 16.224777) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.568262 16.825196) (end 44.643696 16.530392) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.465287 17.107666) (end 44.568262 16.825196) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.336293 17.376282) (end 44.465287 17.107666) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.182799 17.629521) (end 44.336293 17.376282) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 44.006326 17.865862) (end 44.182799 17.629521) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.808392 18.083784) (end 44.006326 17.865862) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.590518 18.281767) (end 43.808392 18.083784) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.354223 18.458287) (end 43.590518 18.281767) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 43.101028 18.611824) (end 43.354223 18.458287) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.832452 18.740858) (end 43.101028 18.611824) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.550015 18.843865) (end 42.832452 18.740858) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 42.255237 18.919325) (end 42.550015 18.843865) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.949638 18.965717) (end 42.255237 18.919325) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 41.634738 18.981519) (end 41.949638 18.965717) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.777554 18.981519) (end 41.634738 18.981519) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.462648 18.965717) (end 4.777554 18.981519) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.157033 18.919325) (end 4.462648 18.965717) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.86223 18.843865) (end 4.157033 18.919325) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.57976 18.740858) (end 3.86223 18.843865) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.311145 18.611824) (end 3.57976 18.740858) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.057907 18.458287) (end 3.311145 18.611824) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.821565 18.281767) (end 3.057907 18.458287) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.603643 18.083784) (end 2.821565 18.281767) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.405661 17.865862) (end 2.603643 18.083784) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.229141 17.629521) (end 2.405661 17.865862) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.075603 17.376282) (end 2.229141 17.629521) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.94657 17.107666) (end 2.075603 17.376282) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.843563 16.825196) (end 1.94657 17.107666) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.768103 16.530392) (end 1.843563 16.825196) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.721711 16.224777) (end 1.768103 16.530392) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.705909 15.90987) (end 1.721711 16.224777) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.705909 -20.947311) (end 1.705909 15.90987) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.721711 -21.262212) (end 1.705909 -20.947311) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.768103 -21.567811) (end 1.721711 -21.262212) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.843563 -21.862589) (end 1.768103 -21.567811) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.94657 -22.145026) (end 1.843563 -21.862589) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.075603 -22.413602) (end 1.94657 -22.145026) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.229141 -22.666797) (end 2.075603 -22.413602) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.405661 -22.903091) (end 2.229141 -22.666797) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.603643 -23.120965) (end 2.405661 -22.903091) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.821565 -23.318899) (end 2.603643 -23.120965) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.057907 -23.495373) (end 2.821565 -23.318899) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.311145 -23.648867) (end 3.057907 -23.495373) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.57976 -23.777861) (end 3.311145 -23.648867) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 3.86223 -23.880835) (end 3.57976 -23.777861) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.157033 -23.95627) (end 3.86223 -23.880835) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.462648 -24.002646) (end 4.157033 -23.95627) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4.777554 -24.018443) (end 4.462648 -24.002646) (layer Edge.Cuts) (width 0.1))
  )
  (zone (net 2) (net_name +BATT) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1524) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.9972 83.7434) (xy 119.1082 83.7434) (xy 118.143 82.6766) (xy 103.8174 82.6766) (xy 103.8174 81.0764)
        (xy 104.49812 81.08402) (xy 105.10772 81.71902) (xy 115.857 81.7114) (xy 115.857 79.0952) (xy 116.8222 79.0952)
        (xy 118.5494 81.5082) (xy 119.9972 82.9306)
      )
    )
  )
  (zone (net 15) (net_name +3V0) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.315 74.32) (xy 143.035 74.32) (xy 143.035 120.04) (xy 97.315 120.04)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.315 74.32) (xy 143.035 74.32) (xy 143.035 120.04) (xy 97.315 120.04)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.695 101.97) (xy 137.095 101.97) (xy 137.095 91.74) (xy 141.695 91.74)
      )
    )
  )
  (zone (net 1) (net_name +5P) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.855 78.24) (xy 118.555 78.24) (xy 119.015 78.72) (xy 119.065 80.97) (xy 118.885 81.43)
        (xy 116.975 78.87) (xy 115.855 78.87)
      )
    )
  )
)
