(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 107)
    (no_connects 2)
    (area 105.276778 41.866199 139.674386 111.0156)
    (thickness 1.6)
    (drawings 21)
    (tracks 633)
    (zones 0)
    (modules 58)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDD)
  (net 2 +3V3)
  (net 3 /AREF)
  (net 4 /~RESET)
  (net 5 /TX)
  (net 6 /RX)
  (net 7 /SDA)
  (net 8 /SCL)
  (net 9 "Net-(U1-Pad9)")
  (net 10 "Net-(U1-Pad10)")
  (net 11 /DIO1)
  (net 12 "Net-(U1-Pad13)")
  (net 13 /NSS)
  (net 14 /MOSI)
  (net 15 /MISO)
  (net 16 /SCK)
  (net 17 "Net-(U1-Pad19)")
  (net 18 "Net-(U1-Pad22)")
  (net 19 /RST)
  (net 20 "Net-(U1-Pad24)")
  (net 21 "Net-(U1-Pad25)")
  (net 22 "Net-(U1-Pad26)")
  (net 23 /DIO0)
  (net 24 "Net-(U2-Pad7)")
  (net 25 "Net-(U2-Pad11)")
  (net 26 "Net-(U2-Pad12)")
  (net 27 "Net-(J4-Pad1)")
  (net 28 /XTAL1)
  (net 29 /XTAL2)
  (net 30 /DIO2)
  (net 31 "Net-(U1-Pad11)")
  (net 32 "Net-(C6-Pad2)")
  (net 33 "Net-(D1-Pad2)")
  (net 34 /LED)
  (net 35 "Net-(U3-Pad2)")
  (net 36 "Net-(J2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /AREF)
    (add_net /DIO0)
    (add_net /DIO1)
    (add_net /DIO2)
    (add_net /LED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /NSS)
    (add_net /RST)
    (add_net /RX)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net /~RESET)
    (add_net GNDD)
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad2)")
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 127.6858 83.5152)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 110.2868 108.331)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 122.174 108.9406)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 127.6858 101.3714)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 120.523 73.3552)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE56D6)
    (at 116.9924 57.9882)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5B14D69A)
    (at 120.7008 48.75276)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.34544) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5B14D69A)
    (at 116.9924 55.20436)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.34544) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5B14D69A)
    (at 110.6678 55.20436)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.34544) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5B14D69A)
    (at 110.6678 48.75276)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.34544) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 127.6858 87.5538)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 127.9652 76.2762)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 124.841 83.5152)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 118.9736 77.7748)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 117.983 70.0278)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 124.079 62.4332)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5B14D141)
    (at 127.2794 52.2732)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.3302) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5B14D69A)
    (at 121.5136 45.39996)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.34544) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 123.1646 65.3542)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE533F)
    (at 111.9886 85.0138)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE533F)
    (at 110.11408 79.883)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE533F)
    (at 110.7694 86.53272)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE533F)
    (at 110.13948 83.09356)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 113.7412 64.897)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 113.7412 61.6458)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE56D6)
    (at 110.5916 57.9628)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 127.6858 108.3564)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 116.078 67.7672)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 121.6914 59.7408)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 122.6312 101.346)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE533F)
    (at 110.11408 76.6318)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 124.1806 87.5792)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE5019)
    (at 110.68304 100.82276)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5AECDCCB)
    (at 124.1806 90.87536 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.43764 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 5AEE1B59)
    (at 118.969375 83.506663 135)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 -6.05 135) (layer F.SilkS) hide)
    (fp_text value ATMEGA328P-AN (at 0 6.05 135) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /DIO1))
    (pad 2 smd rect (at -4.25 -2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /DIO2))
    (pad 3 smd rect (at -4.25 -1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 4 smd rect (at -4.25 -0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 5 smd rect (at -4.25 0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 6 smd rect (at -4.25 1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 7 smd rect (at -4.25 2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /XTAL1))
    (pad 8 smd rect (at -4.25 2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /XTAL2))
    (pad 9 smd rect (at -2.8 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /LED))
    (pad 13 smd rect (at 0.4 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /NSS))
    (pad 15 smd rect (at 2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 17 smd rect (at 4.25 2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /SCK))
    (pad 18 smd rect (at 4.25 2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 19 smd rect (at 4.25 1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /AREF))
    (pad 21 smd rect (at 4.25 -0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 22 smd rect (at 4.25 -1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /RST))
    (pad 24 smd rect (at 4.25 -2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /SDA))
    (pad 28 smd rect (at 0.4 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL))
    (pad 29 smd rect (at -0.4 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /~RESET))
    (pad 30 smd rect (at -1.2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /RX))
    (pad 31 smd rect (at -2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /TX))
    (pad 32 smd rect (at -2.8 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /DIO0))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_KMR2 (layer F.Cu) (tedit 5AEE0FC6)
    (at 124.2748 106.591 180)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at -0.06096 -0.01524 180) (layer F.SilkS))
    (fp_text value RESET (at -0.12 -2.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.45 180) (layer F.Fab))
    (pad 1 smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /~RESET))
    (pad 2 smd rect (at -2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 1 smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /~RESET))
    (pad 2 smd rect (at 2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_KMR2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Electronics/_projects/_in_production/20180422.3  LoRaWAN Node 1 rev. 2/KiCAD/lib_3d/SW_SPST_KMR2.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:CON-SMA-EDGE-CLEAR (layer B.Cu) (tedit 5AEDF96C)
    (at 115.73764 46.8884)
    (fp_text reference J4 (at -4.40944 -1.143) (layer F.SilkS))
    (fp_text value SMA (at -4.91744 -0.0762) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 1.524 4.064) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at -2.54 0) (size 1.524 4.064) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDD))
    (pad 4 smd rect (at 2.54 0) (size 1.524 4.064) (layers B.Cu B.Paste B.Mask)
      (net 1 GNDD))
    (pad 3 smd rect (at -2.54 0) (size 1.524 4.064) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 5 smd rect (at 2.54 0) (size 1.524 4.064) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model "D:/Electronics/_projects/_in_production/20180422.3  LoRaWAN Node 1 rev. 2/KiCAD/lib_3d/CON-SMA-EDGE.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5AEDEEEA)
    (at 112.24768 77.22032 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.2512 -0.06604 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /AREF))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AEE077A)
    (at 114.20348 91.06912 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.00504 -3.77444 360) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5AEDEEB0)
    (at 114.18316 77.24216 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.24968 -0.02032 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5AEE08B9)
    (at 125.68352 57.47512)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AEE0731)
    (at 112.25784 91.06912 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.00004 -1.78816 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /~RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5AEE0756)
    (at 116.14912 91.06412 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.05236 -1.94056 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5AEDF94F)
    (at 125.2601 48.2346)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5AEE1B43)
    (at 112.65916 102.4128)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at -2.50952 -0.49276) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /~RESET))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Crystal_Resonator_Murata_3.2x1.3 (layer F.Cu) (tedit 5AEE1B4D)
    (at 126.1364 92.1826 90)
    (fp_text reference Y1 (at 3.78044 -0.03048 180) (layer F.SilkS))
    (fp_text value Crystal_GND2 (at 2.09 1.68 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 0.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /XTAL1))
    (pad 2 smd rect (at 1.4 0 90) (size 0.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 3 smd rect (at 2.8 0 90) (size 0.4 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /XTAL2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE4F95)
    (at 116.7892 60.69076)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:VIA-0.6mm (layer F.Cu) (tedit 5AEE56D6)
    (at 110.27156 45.70476)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GNDD) (zone_connect 2))
  )
  (module lib_fp:Battery_Keystone_2460_1xAA (layer B.Cu) (tedit 5AEE69C9)
    (at 119.07774 54.1782 270)
    (fp_text reference BT1 (at 0 -10.16 270) (layer B.SilkS) hide)
    (fp_text value 3.3V (at 5.08 10.16 270) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 3 3) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 51.99 0 270) (size 3 3) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 3 thru_hole circle (at 49.23 -6 270) (size 2.64 2.64) (drill 2.64) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.76 6 270) (size 2.64 2.64) (drill 2.64) (layers *.Cu *.Mask))
    (model "D:/Electronics/_projects/_in_production/20180422.3  LoRaWAN Node 1 rev. 2/KiCAD/lib_3d/Battery_Keystone_2460_1xAA.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:RFM95W (layer F.Cu) (tedit 5AEEE68C)
    (at 119.02848 66.93432 180)
    (attr smd)
    (fp_text reference U2 (at 0 9 180) (layer F.SilkS) hide)
    (fp_text value RFM95W (at 0 -9 180) (layer F.Fab))
    (pad 1 smd rect (at -8 -7 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -8 -5 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 3 smd rect (at -8 -3 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 4 smd rect (at -8 -1 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 /SCK))
    (pad 5 smd rect (at -8 1 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 /NSS))
    (pad 6 smd rect (at -8 3 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 /RST))
    (pad 7 smd rect (at -8 5 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -8 7 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 9 smd rect (at 8 7 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad1)"))
    (pad 10 smd rect (at 8 5 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 11 smd rect (at 8 3 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 8 1 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 8 -1 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 14 smd rect (at 8 -3 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /DIO0))
    (pad 15 smd rect (at 8 -5 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /DIO1))
    (pad 16 smd rect (at 8 -7 180) (size 2.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /DIO2))
    (model C:/Engineering/KiCAD_Libraries/3D/Modules/VRML/RFM95W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Electronics/_projects/_in_production/20180422.3  LoRaWAN Node 1 rev. 2/KiCAD/lib_3d/RFM96W.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B15041D)
    (at 112.23752 87.54796 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0.01956 -1.72212 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 /~RESET))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B1452F5)
    (at 126.0856 77.4016 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -0.0078 -1.6256 360) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module "lib_fp:Connector Coaxial U.FL_Hirose_U.FL-R-SMT-1_Vertical" (layer F.Cu) (tedit 5B15454F)
    (at 115.7242 47.5412 90)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference J5 (at 1.7958 4.4178 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0.475 3.2 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.475 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.475 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 1 smd rect (at -1.05 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at 0.475 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (at (xyz 0.018701 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Electronics/_projects/_in_production/20180422.3  LoRaWAN Node 1 rev. 2/KiCAD/lib_3d/Connector Coaxial U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B145327)
    (at 126.0856 81.0108 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -2.1234 0 180) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /LED))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B14534C)
    (at 124.1806 77.24216 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.098 0.0254 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /NSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-23-5 (layer F.Cu) (tedit 5B154165)
    (at 124.8772 94.6506)
    (descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
    (tags TSOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0.1162 0.0152) (layer F.SilkS) hide)
    (fp_text value 24AA02E64T (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.31 -0.95) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCL))
    (pad 2 smd rect (at -1.31 0) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -1.31 0.95) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /SDA))
    (pad 4 smd rect (at 1.31 0.95) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 5 smd rect (at 1.31 -0.95) (size 1.22 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TSOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B1558F3)
    (at 112.70996 94.67088 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0.51816 -2.51968 180) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SDA))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5B15592B)
    (at 112.74044 98.51699 90)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0.50855 -2.55016 180) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(C6-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /TX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text "uFL\n" (at 120.4468 46.8122) (layer F.SilkS))
  (gr_text 24AA02E64T (at 127.9144 94.8182 90) (layer F.SilkS))
  (gr_text 1 (at 110.14964 102.87) (layer F.SilkS))
  (gr_text 1 (at 110.19028 98.99396) (layer F.SilkS))
  (gr_text 1 (at 110.12932 95.18396) (layer F.SilkS))
  (gr_arc (start 125.323509 48.2092) (end 125.348909 44.6532) (angle 89.59075139) (layer Edge.Cuts) (width 0.1))
  (gr_text "LoRaWAN Node" (at 121.75236 50.27168) (layer B.SilkS))
  (gr_text RESET (at 124.2822 109.0676) (layer F.SilkS))
  (gr_text "BAT1 3.7V\n[+]" (at 121.285 54.2036) (layer F.SilkS))
  (gr_text [-] (at 119.0752 108.6612) (layer F.SilkS))
  (gr_text "J1 I2C\nJ2 FTDI\nJ3 SPI" (at 117.475 102.42296) (layer F.SilkS))
  (gr_text RFM95W (at 121.2088 57.5818) (layer F.SilkS))
  (gr_text "LoRaWAN Node\nWA.06.01\nrev. 2" (at 110.65256 52.43576) (layer F.SilkS))
  (gr_text ATMEGA328P (at 119.507 76.6572) (layer F.SilkS))
  (gr_arc (start 110.2106 45.6184) (end 109.2454 45.6184) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 127.9144 108.9787) (end 128.8796 108.9787) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 110.2233 108.9787) (end 110.2233 109.9439) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.9144 109.9439) (end 110.2233 109.9439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.8796 48.2092) (end 128.8796 108.9787) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.349 44.6532) (end 110.2106 44.6532) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.2454 45.6184) (end 109.2581 108.9787) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.20476 44.60748) (xy 109.19968 109.99216) (xy 128.91516 109.98708) (xy 128.91516 44.60748) (xy 109.20476 44.6024)
      )
    )
  )
  (zone (net 1) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.92024 44.61256) (xy 128.91516 110.00232) (xy 109.1946 109.97184) (xy 109.20476 44.6024)
      )
    )
  )
)
