(kicad_pcb (version 4) (host pcbnew 4.0.3+e1-6302~38~ubuntu16.04.1-stable)
  (general
    (links 68)
    (no_connects 0)
    (area 74.949999 64.949999 117.550001 94.050001)
    (thickness 1.6)
    (drawings 4)
    (tracks 262)
    (zones 0)
    (modules 25)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/paul/))
  )
  (net 0 "")
  (net 1 /DTR)
  (net 2 /RESET)
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 VCC)
  (net 6 /CH2)
  (net 7 /CH3)
  (net 8 "Net-(IC1-Pad7)")
  (net 9 "Net-(IC1-Pad8)")
  (net 10 /OSD_SW1)
  (net 11 /OSD_SW2)
  (net 12 "Net-(IC1-Pad11)")
  (net 13 "Net-(IC1-Pad13)")
  (net 14 "Net-(IC1-Pad14)")
  (net 15 /MOSI)
  (net 16 /MISO)
  (net 17 /SCK)
  (net 18 "Net-(IC1-Pad19)")
  (net 19 "Net-(IC1-Pad22)")
  (net 20 "Net-(IC1-Pad23)")
  (net 21 /RSSI)
  (net 22 "Net-(IC1-Pad26)")
  (net 23 /RX)
  (net 24 /TX)
  (net 25 /CH1)
  (net 26 "Net-(J1-Pad1)")
  (net 27 "Net-(P1-Pad2)")
  (net 28 "Net-(P1-Pad4)")
  (net 29 /AUD)
  (net 30 /VID)
  (net 31 /OSD)
  (net 32 /SPI_SEL)
  (net 33 "Net-(R8-Pad2)")
  (net 34 /RX_VID)
  (net 35 "Net-(U2-Pad1)")
  (net 36 /OLED_SCL)
  (net 37 /OLED_SDA)
  (net 38 /OLED_RES)
  (net 39 /OLED_DC)
  (net 40 /I2C_SDA)
  (net 41 /I2C_SCL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /AUD)
    (add_net /CH1)
    (add_net /CH2)
    (add_net /CH3)
    (add_net /DTR)
    (add_net /I2C_SCL)
    (add_net /I2C_SDA)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /OLED_DC)
    (add_net /OLED_RES)
    (add_net /OLED_SCL)
    (add_net /OLED_SDA)
    (add_net /OSD)
    (add_net /OSD_SW1)
    (add_net /OSD_SW2)
    (add_net /RESET)
    (add_net /RSSI)
    (add_net /RX)
    (add_net /RX_VID)
    (add_net /SCK)
    (add_net /SPI_SEL)
    (add_net /TX)
    (add_net /VID)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U2-Pad1)")
    (add_net VCC)
  )
  (module footprints:RX5808 (layer B.Cu) (tedit 578E9636)
    (at 96.25 80.6)
    (fp_text reference U1 (at 0.2 -0.1) (layer B.SilkS))
    (fp_text value RX5808 (at 0 1.7) (layer B.Fab))
    (pad 9 smd rect (at 14 -9.72) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 39 /OLED_DC))
    (pad 8 smd rect (at 14 -7.18) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 32 /SPI_SEL))
    (pad 7 smd rect (at 14 -4.64) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 38 /OLED_RES))
    (pad 6 smd rect (at 14 -2.1) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 5 smd rect (at 14 0.44) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 4 smd rect (at 14 2.98) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 21 /RSSI))
    (pad 3 smd rect (at 14 5.52) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /AUD))
    (pad 2 smd rect (at 14 8.06) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 34 /RX_VID))
    (pad 1 smd rect (at 14 10.6) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 10 smd rect (at -14 -4.64) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 11 smd rect (at -14 -7.18) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J1-Pad1)"))
    (pad 12 smd rect (at -14 -9.72) (size 3 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model /home/paul/kicad/modules/packages3d/RX5808.wrl
      (at (xyz -0.55118 -0.4333 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 92.75 80.25 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0.25 0.25 180) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at -0.4 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /CH2))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /CH3))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /OSD_SW1))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /OSD_SW2))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /OLED_SCL))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /MISO))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCK))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /OLED_SDA))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /RSSI))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /I2C_SDA))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /I2C_SCL))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /RX))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /TX))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /CH1))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 83.05 84.75)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.95 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /DTR))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 93.5 72.25 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.75 0.25 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 93.45 74 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.7 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 0)
    (at 99.25 91.25 180)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C4 (at -0.25 0 360) (layer F.SilkS))
    (fp_text value 470uF (at -0.09906 3.59918 180) (layer F.Fab))
    (fp_text user + (at -7.25 0 180) (layer F.SilkS))
    (pad 2 smd rect (at 3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -3.88874 0 180) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module footprints:SMA_Edge_thru_hole (layer F.Cu) (tedit 57A6B411)
    (at 79 72.25)
    (fp_text reference J1 (at 2.5 -0.25 180) (layer F.SilkS))
    (fp_text value SMA (at -0.1 -5.6) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J1-Pad1)"))
    (pad 2 thru_hole rect (at 0 -2.55) (size 2 2) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole rect (at 0 2.57) (size 2 2) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 3 thru_hole rect (at -2.55 -2.55) (size 2 2) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 4 thru_hole rect (at -2.55 2.55) (size 2 2) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model /home/paul/kicad/modules/packages3d/SMA-106.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 90 0 270))
    )
  )
  (module footprints:SMD_Jumper (layer F.Cu) (tedit 57A99067)
    (at 110.25 86 270)
    (fp_text reference JP1 (at 0.25 -2.25 360) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.5 0) (size 1.524 0.762) (layers F.Cu F.Paste F.Mask)
      (net 30 /VID))
    (pad 2 smd rect (at 0.5 0) (size 1.524 0.762) (layers F.Cu F.Paste F.Mask)
      (net 34 /RX_VID))
  )
  (module Pin_Headers:Pin_Header_Straight_1x09 (layer B.Cu) (tedit 0)
    (at 116 91.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -3 0) (layer B.SilkS))
    (fp_text value Fatshark (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 4 thru_hole oval (at 0 -7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 /AUD))
    (pad 6 thru_hole oval (at 0 -12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 /VID))
    (pad 7 thru_hole oval (at 0 -15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 /CH3))
    (pad 8 thru_hole oval (at 0 -17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 /CH2))
    (pad 9 thru_hole oval (at 0 -20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 /CH1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x09.wrl
      (at (xyz 0 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 78 91.66 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -3 0.16 180) (layer F.SilkS))
    (fp_text value FTDI (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /DTR))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /TX))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /RX))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 96.17 67.75 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0.25 -2.92 180) (layer F.SilkS))
    (fp_text value "I2C OLED" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /I2C_SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /I2C_SDA))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 83.15 82.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.35 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 104.75 77.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.25 0) (layer F.SilkS))
    (fp_text value 1k (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad13)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /OSD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 108.4 73.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.35 0) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad14)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /SPI_SEL))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 108.4 71)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.35 0) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /MOSI))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /OLED_DC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 108.35 68.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.4 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /OLED_RES))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCK))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 104.75 80)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.25 -0.25) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad11)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /OSD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5418A00F)
    (at 103 86.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.75 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /RSSI))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 109.9 83 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.35 0 180) (layer F.SilkS))
    (fp_text value 10 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /VID))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:VSSOP-8 (layer F.Cu) (tedit 57928462)
    (at 104.5 83.45 90)
    (fp_text reference U2 (at -3.05 1.75 180) (layer F.SilkS))
    (fp_text value TS5A3359 (at -0.3 3.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 1.6 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -0.8 1.6 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 /RX_VID))
    (pad 3 smd rect (at -0.3 1.6 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /OSD))
    (pad 4 smd rect (at 0.2 1.6 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 5 smd rect (at 0.2 -1.5 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 /OSD_SW2))
    (pad 6 smd rect (at -0.3 -1.5 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 /OSD_SW1))
    (pad 7 smd rect (at -0.8 -1.5 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R8-Pad2)"))
    (pad 8 smd rect (at -1.3 -1.5 90) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (model /home/paul/kicad/modules/packages3d/VSSOP8.wrl
      (at (xyz -0.0215 -0.0025 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 270 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57B916F9)
    (at 102 74)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference W1 (at 0.25 1.75) (layer F.SilkS) hide)
    (fp_text value MOSI (at 2.5 1.25) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 15 /MOSI))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57B916E7)
    (at 102 71)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference W2 (at 0 1.75) (layer F.SilkS) hide)
    (fp_text value MISO (at 2.5 1.25) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 16 /MISO))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57B916D6)
    (at 99.5 71)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference W3 (at -0.25 1.75) (layer F.SilkS) hide)
    (fp_text value SCK (at -2.25 0) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 17 /SCK))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57B91690)
    (at 84.5 79.75)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference W4 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value RST (at 0 -1.75) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 /RESET))
  )
  (module footprints:OSC_CSTCE16M0V53-R0 (layer F.Cu) (tedit 57B917C5)
    (at 95.2 87.25 180)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference Y1 (at 2.7 0 180) (layer F.SilkS))
    (fp_text value 16Mhz (at -3.3 -1 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad8)"))
    (pad 2 smd rect (at 0 0 270) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0.95 0 270) (size 1.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad7)"))
    (model ../../../../../home/paul/kicad/modules/packages3d/CSTCE.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393700787 0.393700787 0.393700787))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 75 94) (end 75 65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5 94) (end 75 94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5 65) (end 117.5 94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75 65) (end 117.5 65) (layer Edge.Cuts) (width 0.1))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.25 65.25) (xy 75.25 65.25) (xy 75.25 93.75) (xy 117.25 93.75)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.25 65.25) (xy 117.25 93.75) (xy 75.25 93.75) (xy 75.25 65.25)
      )
    )
  )
)
