<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38.1" y2="0" width="0" layer="20"/>
<wire x1="38.1" y1="0" x2="38.1" y2="25.4" width="0" layer="20"/>
<wire x1="38.1" y1="25.4" x2="0" y2="25.4" width="0" layer="20" locked="yes"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20" locked="yes"/>
<hole x="3.175" y="22.225" drill="2.54"/>
<hole x="34.925" y="3.175" drill="2.794"/>
<text>-V In-</text>
<text>Batt</text>
<text>-LED+</text>
<text>ISLAND LABS</text>
<text>ISLAND LABS</text>
<text>P/N G22C47</text>
<text>Supply</text>
<text>+LED-</text>
<text>Batt</text>
<text>Out</text>
<text>-</text>
<text>Rev A0</text>
<text>Out</text>
<text>-</text>
<text>ISLAND LABS</text>
</plain>
<libraries>
<library name="rcl_gianni">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="resistor gianni">
<packages>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear-technology">
<description>&lt;b&gt;Linear Technology Devices&lt;/b&gt;&lt;p&gt;
http://www.linear-tech.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DFN10-3X3">
<description>&lt;b&gt;DD Package 10-Lead Plastic DFN (3mm × 3mm)&lt;/b&gt;&lt;p&gt;
(Reference LTC DWG # 05-08-1669)&lt;br&gt;
Source: http://www.linear.com .. 4062fa.pdf</description>
</package>
</packages>
</library>
<library name="Gianni Lib">
<description>Generated from &lt;b&gt;10V_Ref_TH_1smd.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="DP_DEVICES.V6_M1X3">
</package>
<package name="RCL_GIANNI_C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="IC_ROTTO">
</package>
</packages>
</library>
<library name="dp_devices.v6">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="M1X2">
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SOIC 150 mil</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="FUSC3216X85N">
<description>&lt;b&gt;MF-NSMF050-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="Gianni Lib" package="RCL_GIANNI_C1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor gianni" package="SMC_D" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear-technology" package="DFN10-3X3" value="LTC4079">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Gianni Lib" package="DP_DEVICES.V6_M1X3" value="DP_DEVICES.V6_CON_HEADER_1X03-PTH">
<attribute name="NAME"/>
</element>
<element name="J3" library="Gianni Lib" package="DP_DEVICES.V6_M1X3" value="DP_DEVICES.V6_CON_HEADER_1X03-PTH">
<attribute name="NAME"/>
</element>
<element name="J1" library="dp_devices.v6" package="M1X2" value="CON_HEADER_1X02-PTH">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl_gianni" package="R0805" value="2M55">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl_gianni" package="R0805" value="261k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl_gianni" package="R0805" value="4k13">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl_gianni" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Gianni Lib" package="RCL_GIANNI_C1206" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Gianni Lib" package="RCL_GIANNI_C1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="DMP3099">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08285"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl_gianni" package="R0805" value="261k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl_gianni" package="R0805" value="261k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl_gianni" package="R0805" value="261k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="resistor gianni" package="R1206" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="resistor gianni" package="R1206" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="maxim" package="SO08" value="MAX8212CS">
<attribute name="MF" value="MAXIM"/>
<attribute name="MPN" value="MAX8211CSA+"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9725911"/>
<attribute name="OC_NEWARK" value="68K5031"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="resistor gianni" package="R1206" value="50k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Gianni Lib" package="IC_ROTTO" value=""/>
<element name="U$2" library="Gianni Lib" package="IC_ROTTO" value=""/>
<element name="F1" library="SamacSys_Parts" package="FUSC3216X85N" value="MF-NSMF050-2">
<attribute name="DESCRIPTION" value="Bourns 0.5A Surface Mount Resettable Fuse, 13.2V"/>
<attribute name="HEIGHT" value="0.85mm"/>
<attribute name="MANUFACTURER_NAME" value="Bourns"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MF-NSMF050-2"/>
<attribute name="MOUSER_PART_NUMBER" value="652-MF-NSMF050-2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="SamacSys_Parts" package="FUSC3216X85N" value="200mA">
<attribute name="DESCRIPTION" value="Bourns 0.5A Surface Mount Resettable Fuse, 13.2V"/>
<attribute name="HEIGHT" value="0.85mm"/>
<attribute name="MANUFACTURER_NAME" value="Bourns"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MF-NSMF050-2"/>
<attribute name="MOUSER_PART_NUMBER" value="652-MF-NSMF050-2"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="BATT">
<contactref element="IC1" pad="10"/>
<contactref element="C4" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="R10" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="R5" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="FB">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="6"/>
<contactref element="C1" pad="-"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="EXP"/>
<contactref element="C4" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="GND"/>
<contactref element="IC1" pad="P$2"/>
<contactref element="IC1" pad="P$3"/>
<contactref element="IC1" pad="P$4"/>
<contactref element="IC1" pad="P$5"/>
<contactref element="IC1" pad="P$6"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="5"/>
<contactref element="R6" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="IPROG">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="FBG">
<contactref element="IC1" pad="8"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="CHRG">
<contactref element="IC1" pad="7"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="-LED">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="HYST">
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="TRESH">
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="GATE">
<contactref element="R10" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R9" pad="2"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="TRIM">
<contactref element="R5" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="V_OUT">
<contactref element="J3" pad="2"/>
<contactref element="F2" pad="1"/>
</signal>
<signal name="IC">
</signal>
<signal name="N$1">
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="3"/>
<contactref element="F2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
