(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 20)
    (zones 0)
    (modules 62)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 0.5)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 "Net-(D1-Pad1)")
  (net 3 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 8.3439 96.94926 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at 8.3312 96.04756 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at 10.17016 96.03232 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 10.17778 96.94164 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at 3.20548 96.02724 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at 1.36652 96.04248 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 1.37922 96.94418 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 3.2131 96.93656 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -3.79984 96.9391 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -5.63372 96.94672 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at -5.64642 96.04502 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at -3.80746 96.02978 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 10.19556 78.22692 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 8.36168 78.23454 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at 8.34898 77.33284 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at 10.18794 77.3176 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 1.36398 78.232 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at 3.19786 78.22438 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at 1.35128 77.3303 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at 3.19024 77.31506 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -5.63372 78.22692 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -3.79984 78.2193 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at -3.80746 77.30998 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at -5.64642 77.32522 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -12.61364 78.22692 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at -10.78738 77.30998 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at -12.62634 77.32522 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -10.77976 78.2193 180)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888 180) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -12.74572 93.61424)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at -2.19408 88.41994 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C8)
    (at -16.19408 84.02828 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C8)
    (at -2.19408 84.02828 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C8)
    (at -9.19408 84.02828 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at -16.19408 88.41994 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at -9.19408 88.41994 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C8)
    (at 4.80592 84.02828 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 4.80592 88.41994 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B4B45C8)
    (at 11.80592 84.02828 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 11.80592 88.41994 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.65 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.65 270) (layer B.SilkS))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99DB)
    (at -12.73302 94.51594)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F998E)
    (at -14.57198 94.53118)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:HOLE-UNPLATED-200MIL (layer F.Cu) (tedit 5E5F99E9)
    (at -14.5796 93.62186)
    (attr virtual)
    (fp_text reference V (at 0 -2) (layer F.SilkS) hide)
    (fp_text value HOLE-PLATED-200MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.94996 1.19888) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -16.19504 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -16.22044 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at -16.19758 88.42248 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at -16.19758 84.03082 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -9.19504 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -2.19504 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at 4.80496 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at 11.80496 93.54566)
    (attr smd)
    (fp_text reference J4 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -9.22044 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at -2.22044 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at 4.77956 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x01 (layer F.Cu) (tedit 58FF6D5C)
    (at 11.77956 78.88478)
    (attr smd)
    (fp_text reference J1 (at 0 -2.3495) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at -9.19758 84.03082 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at -2.19758 84.03082 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 4.80242 84.03082 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 11.80242 84.03082 90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at -9.19758 88.42248 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at -2.19758 88.42248 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 4.80242 88.42248 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 11.80242 88.42248 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.65 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 14.28242 75.63358) (end 14.2875 96.2279) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -18.83918 75.63358) (end -18.83918 96.2279) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -18.83918 96.2279) (end 14.2875 96.2279) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -18.83918 75.63358) (end 14.28242 75.63358) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 9.3348 77.66558) (end 9.3348 94.16288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 2.3348 77.66558) (end 2.3348 94.16288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -4.6652 77.66558) (end -4.6652 94.16288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 7.3348 77.66558) (end 7.3348 94.16288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0.3348 77.66558) (end 0.3348 94.16288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -6.6652 77.66558) (end -6.6652 94.16288) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 8.3348 77.66558) (end 9.3348 77.66558) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 1.3348 77.66558) (end 2.3348 77.66558) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -5.6652 77.66558) (end -4.6652 77.66558) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 8.3348 94.16288) (end 7.3348 94.16288) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 1.3348 94.16288) (end 0.3348 94.16288) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -5.6652 94.16288) (end -6.6652 94.16288) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -12.6652 77.66558) (end -11.6652 77.66558) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -12.6652 94.16288) (end -13.6652 94.16288) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -11.6652 77.66558) (end -11.6652 94.16288) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -13.6652 77.66558) (end -13.6652 94.16288) (layer Edge.Cuts) (width 0.05))
)
