(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 0)
    (area 119.885 81.192999 136.965 111.593001)
    (thickness 1.6)
    (drawings 16)
    (tracks 7)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.8)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A1A042C)
    (at 125.73 92.456 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference REF** (at -3.683 7.112 90) (layer F.SilkS) hide)
    (fp_text value SOT-23 (at 0 10.16 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.127 7.239 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A1A0483)
    (at 123.19 96.393 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x03_Pitch2.54mm (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 32bitfun.com (at 125.73 98.552) (layer B.Mask))
  (gr_text "SOT23\nAdapter" (at 125.73 92.329) (layer B.Mask))
  (gr_line (start 127 89.535) (end 124.46 89.535) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.46 92.71) (end 121.285 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127 92.71) (end 127 89.535) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 92.71) (end 121.285 92.71) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 99.441) (end 121.285 92.71) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 92.71) (end 130.175 92.71) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.175 99.441) (end 130.175 92.71) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 99.441) (end 130.175 99.441) (layer Edge.Cuts) (width 0.15))
  (gr_text 3 (at 128.27 98.806) (layer F.SilkS))
  (gr_text 2 (at 125.73 98.806) (layer F.SilkS))
  (gr_text 1 (at 123.19 98.806) (layer F.SilkS))
  (gr_text 3 (at 124.46 90.932) (layer F.SilkS))
  (gr_text 2 (at 128.143 93.472) (layer F.SilkS))
  (gr_text 1 (at 123.317 93.472) (layer F.SilkS))
)
