(kicad_pcb (version 20171130) (host pcbnew no-vcs-found-fe62760~61~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 65)
    (zones 0)
    (modules 3)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.254)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(J1-Pad7)")
  (net 4 "Net-(J1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (module customraskey:Pi_I2C_castellated (layer F.Cu) (tedit 5A7A2A82)
    (at 106.9875 68.077381 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x08 (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A7A2EA8)
    (at 116.4 71.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value 0.1uf (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5A7A2EB7)
    (at 110.3 72.6 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value ATECC508A (at 0 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad7)"))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 17 (at 106.4 69.7) (layer F.SilkS))
  (gr_text 3 (at 123.7 69.7) (layer F.SilkS))
  (gr_text "raskey\nv1" (at 116.4 74.8) (layer F.SilkS))
  (gr_line (start 105.5 76.2) (end 119.5 76.2) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 105.5 67.9) (end 105.5 76.2) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 119.5 70.5) (end 119.5 76.2) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 124 70.5) (end 119.5 70.5) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 126.2 69.2) (end 124 70.5) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 126.2 67.9) (end 126.2 69.2) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 105.5 67.9) (end 126.2 67.9) (layer Edge.Cuts) (width 0.254))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.4 66.6) (xy 126.8 66.6) (xy 126.8 77.4) (xy 105.4 77.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.4 66.6) (xy 126.8 66.6) (xy 126.8 77.4) (xy 105.4 77.4)
      )
    )
  )
)
