<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.867221875" y1="0" x2="32.66" y2="0" width="0" layer="20"/>
<wire x1="32.66" y1="0" x2="34.341" y2="1.681" width="0" layer="20" curve="90"/>
<wire x1="34.341" y1="1.681" x2="34.341" y2="17.370371875" width="0" layer="20"/>
<wire x1="34.341" y1="17.370371875" x2="32.671371875" y2="19.04" width="0" layer="20" curve="90"/>
<wire x1="32.671371875" y1="19.04" x2="1.26" y2="19.04" width="0" layer="20"/>
<wire x1="1.26" y1="19.04" x2="0" y2="17.78" width="0" layer="20" curve="90"/>
<wire x1="0" y1="17.78" x2="0" y2="0.867221875" width="0" layer="20"/>
<wire x1="0" y1="0.867221875" x2="0.867221875" y2="0" width="0" layer="20" curve="90"/>
<text>RV-Project.Com
Test Board SB4
1-9-21</text>
<text>+</text>
<text>Non Polarized.  Buzzer active &lt;50 Ohms.</text>
<text>1.25A</text>
</plain>
<libraries>
<library name="a-lib">
<description>Archive Library (for old designs) - do not use for new components.</description>
<packages>
<package name="BUZZER_SMALL">
<description>Pitch: 0.3"&lt;br&gt;Dia: 0.45"&lt;br&gt;Drill: 0.035" dia</description>
</package>
<package name="SMA-DIODE_ALT">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;SMA diode.&lt;br&gt;
Pad Size: 0.25"x0.09"</description>
</package>
<package name="SURFACEPAD25X1">
<description>Pad Size: 0.25"x0.1"</description>
</package>
</packages>
</library>
<library name="a-lib_SMD">
<description>All SMD Devices; Actives, Passives, Connectors</description>
<packages>
<package name="LED-1206">
</package>
<package name="1206-RES">
</package>
<package name="SMA-DIODE_ALT">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;SMA diode.&lt;br&gt;
Pad Size: 0.25"x0.09"</description>
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="KEYSTONE_4919">
</package>
</packages>
</library>
<library name="a-lib_Passives">
<description>Thru-Hole Passives (Resistors, Capacitors)</description>
<packages>
<package name="ASMDC">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BZ1" library="a-lib" package="BUZZER_SMALL" value="BUZZERMALLORY_PT1140PEQ">
<attribute name="VOLTAGE" value="9-20V"/>
</element>
<element name="D1" library="a-lib" package="SMA-DIODE_ALT" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE" value="1A"/>
<attribute name="VOLTAGE" value="1000V"/>
</element>
<element name="D2" library="a-lib" package="SMA-DIODE_ALT" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE" value="1A"/>
<attribute name="VOLTAGE" value="1000V"/>
</element>
<element name="D3" library="a-lib" package="SMA-DIODE_ALT" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE" value="1A"/>
<attribute name="VOLTAGE" value="1000V"/>
</element>
<element name="D4" library="a-lib" package="SMA-DIODE_ALT" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE" value="1A"/>
<attribute name="VOLTAGE" value="1000V"/>
</element>
<element name="JP3" library="a-lib" package="SURFACEPAD25X1" value=""/>
<element name="JP4" library="a-lib" package="SURFACEPAD25X1" value=""/>
<element name="JP5" library="a-lib" package="SURFACEPAD25X1" value=""/>
<element name="JP6" library="a-lib" package="SURFACEPAD25X1" value=""/>
<element name="LED1" library="a-lib_SMD" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib_SMD" package="1206-RES" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="U$1" library="a-lib_SMD" package="SMA-DIODE_ALT" value="ZENER 3-7V">
<attribute name="PARTNO" value="ZMM7V5"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="7.5V"/>
<attribute name="WATTAGE" value="1/2Watt"/>
</element>
<element name="TB1" library="a-lib_Connectors" package="KEYSTONE_4919" value=""/>
<element name="TB2" library="a-lib_Connectors" package="KEYSTONE_4919" value=""/>
<element name="F1" library="a-lib_Passives" package="ASMDC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="A"/>
<contactref element="D3" pad="C"/>
<contactref element="F1" pad="P$1"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="BZ1" pad="+"/>
<contactref element="U$1" pad="A"/>
<contactref element="JP4" pad="P$1"/>
<contactref element="JP5" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="D4" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="TB1" pad="T1"/>
<contactref element="TB1" pad="T2"/>
</signal>
<signal name="N$3">
<contactref element="BZ1" pad="-"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="JP6" pad="P$1"/>
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="TB2" pad="T2"/>
<contactref element="TB2" pad="T1"/>
<contactref element="F1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
