(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 21)
    (no_connects 0)
    (area 109.144999 76.124999 143.585001 96.595001)
    (thickness 1.6)
    (drawings 55)
    (tracks 67)
    (zones 0)
    (modules 17)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 132.08 93.98)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 VCC)
  (net 9 "Net-(Q1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net VCC)
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 57C1879D)
    (at 126.365 85.725 270)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at 0.9525 -1.905 360) (layer B.SilkS))
    (fp_text value 10uF/25v (at 4.445 0.635 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x01 (layer F.Cu) (tedit 57C18830)
    (at 137.16 94.615 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -2.54 360) (layer B.SilkS))
    (fp_text value GND (at -1.905 0.762 360) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 45))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579B1C5F)
    (at 138.43 85.725 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 5.715 0 180) (layer B.SilkS))
    (fp_text value 39K (at 3.81 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ../../../../../../dev/Coco/Circuits/Libraries/smisioto/walter/pth_resistors/rc03.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579B1C5C)
    (at 141.605 78.105 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 1.905 0 360) (layer B.SilkS))
    (fp_text value 20K (at 3.81 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 GND))
    (model ../../../../../../dev/Coco/Circuits/Libraries/smisioto/walter/pth_resistors/rc03.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579B1C59)
    (at 135.255 78.105 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 1.905 0 360) (layer B.SilkS))
    (fp_text value 220K (at 3.81 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 GND))
    (model ../../../../../../dev/Coco/Circuits/Libraries/smisioto/walter/pth_resistors/rc03.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 579B1C55)
    (at 132.08 85.725 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 5.715 0 180) (layer B.SilkS))
    (fp_text value 220K (at 3.81 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 VCC))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model ../../../../../../dev/Coco/Circuits/Libraries/smisioto/walter/pth_resistors/rc03.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57C181AA)
    (at 118.745 81.28 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R6 (at 3.81 0 180) (layer B.SilkS))
    (fp_text value 1K (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 GND))
    (model ../../../../../../dev/Coco/Circuits/Libraries/smisioto/walter/pth_resistors/rc03.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 57C181A7)
    (at 111.125 78.105)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at 3.81 0) (layer B.SilkS))
    (fp_text value 100R (at 3.81 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 VCC))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(Q1-Pad3)"))
    (model ../../../../../../dev/Coco/Circuits/Libraries/smisioto/walter/pth_resistors/rc03.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 57C18533)
    (at 135.89 88.9)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.54 0) (layer B.SilkS))
    (fp_text value 100p (at 2.54 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 5 0) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x01 (layer B.Cu) (tedit 579B1D18)
    (at 139.7 92.075 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 2.54 360) (layer B.SilkS))
    (fp_text value "SOUND IN" (at 0.635 -5.08 270) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x01 (layer B.Cu) (tedit 579B1D0F)
    (at 132.08 92.075 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -2.54 360) (layer B.SilkS))
    (fp_text value "SOUND OUT 2" (at 5.715 6.985 360) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(C4-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x01 (layer F.Cu) (tedit 579B1D12)
    (at 132.08 94.615 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -2.54 360) (layer B.SilkS))
    (fp_text value "SOUND OUT 1" (at 5.08 6.985 360) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C4-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57C187A1)
    (at 133.35 88.9 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.27 1.27 180) (layer B.SilkS))
    (fp_text value 10n (at 3.81 -1.905 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 57C184C1)
    (at 127.635 78.74 270)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 0.9525 -1.905 360) (layer B.SilkS))
    (fp_text value 10uF/25v (at 4.445 0 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57C184E4)
    (at 123.825 94.615 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 1.143 2.159 180) (layer B.SilkS))
    (fp_text value 22n (at 1.143 2.159 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C4-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.6 1.6) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow_Oval (layer F.Cu) (tedit 579B3A27)
    (at 122.555 80.9625 90)
    (descr "TO-92 leads molded, narrow, oval pads, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 1.905 180) (layer B.SilkS))
    (fp_text value MPSA13 (at -1.905 0 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 1.27 -1.27 180) (size 1.80086 1.30048) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 1 thru_hole oval (at 0 0 135) (size 1.30048 1.80086) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C4-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 135) (size 1.80086 1.30048) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(Q1-Pad3)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 579B1C36)
    (at 127.635 93.345)
    (fp_text reference P2 (at 2.54 0) (layer B.SilkS))
    (fp_text value 5V (at 0.127 2.159) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 8 VCC))
  )
  (gr_line (start 140.97 96.52) (end 120.015 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 93.98) (end 140.97 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 92.71) (end 140.97 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 87.63) (end 142.24 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Audio daughterboard for clone\nColorware Color Computer 2 composite board v1.2" (at 142.875 82.804) (layer B.SilkS))
  (gr_line (start 120.015 85.09) (end 120.015 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 76.835) (end 109.22 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.855 84.455) (end 119.38 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text OUT (at 133.985 93.345 90) (layer F.SilkS))
  (gr_text IN (at 139.954 93.98) (layer F.SilkS))
  (gr_line (start 142.875 76.2) (end 109.855 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 86.36) (end 143.51 76.835) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 87.63) (end 143.51 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142.875 76.835) (end 142.875 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 109.855 76.835) (end 109.22 76.835) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 109.855 83.82) (end 109.855 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 119.38 85.09) (end 119.38 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Inductor prevents tall objects" (at 146.05 92.075) (layer Dwgs.User))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 142.875 86.36) (xy 142.24 86.995) (xy 142.24 96.52) (xy 120.015 96.52) (xy 120.015 85.09)
        (xy 119.38 84.455) (xy 109.855 84.455) (xy 109.22 83.82) (xy 109.22 76.2) (xy 142.875 76.2)
        (xy 142.875 86.36)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 142.875 86.36) (xy 142.24 86.995) (xy 142.24 96.52) (xy 120.015 96.52) (xy 120.015 85.09)
        (xy 119.38 84.455) (xy 109.855 84.455) (xy 109.22 83.82) (xy 109.22 76.2) (xy 142.875 76.2)
        (xy 142.875 86.36)
      )
    )
  )
)
