<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>B</text>
<text>SDA</text>
<text>GND</text>
<text>SCL</text>
<text>3V3</text>
<text>XSH_B</text>
<wire x1="14.375" y1="16.375" x2="14.3357875" y2="16.3357875" width="0.15" layer="20"/>
<wire x1="14.3357875" y1="16.3357875" x2="13.75" y2="14.921571875" width="0.15" layer="20" curve="45.00009"/>
<wire x1="13.75" y1="14.921571875" x2="13.75" y2="8.5" width="0.15" layer="20"/>
<wire x1="13.75" y1="8.5" x2="11.75" y2="6.5" width="0.15" layer="20" curve="-90"/>
<wire x1="11.75" y1="6.5" x2="5.5" y2="6.5" width="0.15" layer="20"/>
<wire x1="5.5" y1="6.5" x2="3.5" y2="8.5" width="0.15" layer="20" curve="-90"/>
<wire x1="3.5" y1="8.5" x2="3.5" y2="29" width="0.15" layer="20"/>
<wire x1="3.5" y1="29" x2="5.5" y2="31" width="0.15" layer="20" curve="-90"/>
<wire x1="5.5" y1="31" x2="11.75" y2="31" width="0.15" layer="20"/>
<wire x1="11.75" y1="31" x2="13.75" y2="29" width="0.15" layer="20" curve="-90"/>
<wire x1="13.75" y1="29" x2="13.75" y2="22.578428125" width="0.15" layer="20"/>
<wire x1="13.75" y1="22.578428125" x2="14.3357875" y2="21.1642125" width="0.15" layer="20" curve="45.000063"/>
<wire x1="14.3357875" y1="21.1642125" x2="14.375" y2="21.125" width="0.15" layer="20"/>
</plain>
<libraries>
<library name="CindysStuff">
<packages>
<package name="SA_PAD">
</package>
<package name="6PIN_FFC_END">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="XSHUT" library="CindysStuff" package="SA_PAD" value="SA_PAD"/>
<element name="SDA" library="CindysStuff" package="SA_PAD" value="SA_PAD"/>
<element name="GND" library="CindysStuff" package="SA_PAD" value="SA_PAD"/>
<element name="SCL" library="CindysStuff" package="SA_PAD" value="SA_PAD"/>
<element name="3V3" library="CindysStuff" package="SA_PAD" value="SA_PAD"/>
<element name="U$7" library="CindysStuff" package="6PIN_FFC_END" value="6PIN_FFC_END"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="XSHUT" pad="P$1"/>
<contactref element="U$7" pad="XSHUT"/>
</signal>
<signal name="N$2">
<contactref element="SDA" pad="P$1"/>
<contactref element="U$7" pad="SDA"/>
</signal>
<signal name="N$3">
<contactref element="GND" pad="P$1"/>
<contactref element="U$7" pad="GND"/>
</signal>
<signal name="N$4">
<contactref element="SCL" pad="P$1"/>
<contactref element="U$7" pad="SCL"/>
</signal>
<signal name="N$5">
<contactref element="3V3" pad="P$1"/>
<contactref element="U$7" pad="3V3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="U$7" pad="GPIO"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
