(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001030_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C2-Pad2)")
  (net 3 "Net-(J1-PadA5)")
  (net 4 "Net-(J1-PadB5)")
  (net 5 "Net-(J2-Pad7)")
  (net 6 "Net-(J2-Pad8)")
  (net 7 "Net-(J2-Pad5)")
  (net 8 "Net-(C1-Pad2)")
  (net 9 "Net-(J2-Pad9)")
  (net 10 "Net-(J3-Pad9)")
  (net 11 "Net-(J3-Pad8)")
  (net 12 "Net-(J3-Pad7)")
  (net 13 "Net-(J3-Pad6)")
  (net 14 "Net-(J1-PadA6)")
  (net 15 "Net-(J1-PadA7)")
  (net 16 "Net-(J1-PadA8)")
  (net 17 "Net-(J1-PadB8)")
  (net 18 "Net-(J2-Pad6)")
  (net 19 "unconnected-(J1-PadS1)")
  (footprint "Package_DFN_QFN:Texas_X2QFN-12_1.6x1.6mm_P0.4mm" (layer "F.Cu")
    (tedit 5D9F792E)
    (at 123.14 94.87 -90)
    (descr "Texas  X2QFN, 12 Pin (http://www.ti.com/lit/ml/mpqf391c/mpqf391c.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "Texas X2QFN NoLead")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 2.205 0 -270) (layer "F.SilkS"))
    (fp_text value "TUSB320" (at 0 2.1 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.725 -0.2 270) (size 0.85 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -0.725 0.2 270) (size 0.85 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -0.6 0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J2-Pad5)") (pinfunction "PORT") (pintype "input"))
    (pad "4" smd roundrect (at -0.2 0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J2-Pad6)") (pinfunction "VBUS_DET") (pintype "input"))
    (pad "5" smd roundrect (at 0.2 0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J2-Pad8)") (pinfunction "ADDR") (pintype "input"))
    (pad "6" smd roundrect (at 0.6 0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J2-Pad9)") (pinfunction "~{INT}/OUT3") (pintype "open_collector"))
    (pad "7" smd roundrect (at 0.725 0.2 270) (size 0.85 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J3-Pad9)") (pinfunction "SDA/OUT1") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0.725 -0.2 270) (size 0.85 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J3-Pad8)") (pinfunction "SCL/OUT2") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.6 -0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J3-Pad7)") (pinfunction "ID") (pintype "open_collector"))
    (pad "10" smd roundrect (at 0.2 -0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect (at -0.2 -0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J3-Pad6)") (pinfunction "~{EN}") (pintype "input"))
    (pad "12" smd roundrect (at -0.6 -0.825 270) (size 0.2 0.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad2)") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Texas_X2QFN-12_1.6x1.6mm_P0.4mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.96 91.64 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 1.0748 90) (layer "F.SilkS"))
    (fp_text value "0.1μF" (at 0 1.16 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.0564 94.6658 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.8816 0.285 90) (layer "F.SilkS"))
    (fp_text value "887K" (at 0 1.17 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad7)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J2-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.2088 83.5152 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "35V")
    (attr smd)
    (fp_text reference "C1" (at 0 1.143 90) (layer "F.SilkS"))
    (fp_text value "1μF" (at 2.3368 1.1176 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_JAE_DX07S016JA1R1500" (layer "F.Cu")
    (tedit 6056970E)
    (at 122.54 75.78 180)
    (descr "USB TYPE C, USB 2.0, SMT, https://www.jae.com/en/connectors/series/detail/product/id=91780")
    (tags "USB C Type-C Receptacle SMD USB 2.0")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "USB-C Receptacle (USB 2.0)" (at 0 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" smd rect (at -1.4 1.15 180) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "" smd rect (at 1.4 1.15 180) (size 1 2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "" np_thru_hole circle (at -3 -1.95 180) (size 0.6 0.6) (drill 0.6) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole oval (at 3 -1.95 180) (size 0.85 0.6) (drill oval 0.85 0.6) (layers F&B.Cu *.Mask))
    (pad "A1" smd rect (at -3.1 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "A4" smd rect (at -2.35 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C1-Pad2)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "A5" smd rect (at -1.75 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J1-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.75 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(J1-PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.75 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" smd rect (at 2.35 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C1-Pad2)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 3.1 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd rect (at 3.1 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.35 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C1-Pad2)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.25 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.25 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J1-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(J1-PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.25 -3.05 180) (size 0.27 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J1-PadB8)") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" smd rect (at -2.35 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C1-Pad2)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at -3.1 -3.05 180) (size 0.52 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 1.15 180) (size 1.3 2.6) (drill oval 0.6 1.9) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole oval (at 4.32 1.15 180) (size 1.3 2.6) (drill oval 0.6 1.9) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole oval (at 4.32 -2.675 180) (size 1.3 2.3) (drill oval 0.6 1.6) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole oval (at -4.32 -2.675 180) (size 1.3 2.3) (drill oval 0.6 1.6) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_JAE_DX07S016JA1R1500.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 118.72 81.958 180)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.33) (layer "B.SilkS") hide)
    (fp_text value "Left Header Pins" (at 3.023 -9.582 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -10.16 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-PadA5)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-PadB5)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 126.34 81.958 180)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.33) (layer "B.SilkS") hide)
    (fp_text value "Right Header Pins" (at -3.0984 -9.052 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -10.16 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-PadB8)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-PadA8)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-PadA7)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-PadA6)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 121.0564 92.7588 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "tusb320-breakout-board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.8308 -0.0564 90) (layer "B.SilkS"))
    (fp_text value "0K" (at 0 -1.17 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J2-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 117.348 71.6) (end 127.712 71.6) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 128.22 103.632) (mid 128.07121 103.99121) (end 127.712 104.14) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 128.22 103.632) (end 128.22 72.108) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 116.84 72.108) (mid 116.98879 71.74879) (end 117.348 71.6) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 116.84 103.632) (end 116.84 72.108) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 127.712 104.14) (end 117.348 104.14) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 127.712 71.6) (mid 128.07121 71.74879) (end 128.22 72.108) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 117.348 104.14) (mid 116.98879 103.99121) (end 116.84 103.632) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Bridge to connect\nVBUS and VBUS_DET" (at 122.8852 94.6912 90) (layer "B.SilkS"))
  (gr_text "ADDR" (at 120.2182 99.695 270) (layer "F.SilkS"))
  (gr_text "OUT3" (at 120.2182 102.2096 270) (layer "F.SilkS"))
  (gr_text "CC1" (at 120.2182 86.995 270) (layer "F.SilkS"))
  (gr_text "VDD" (at 124.841 92.1512 90) (layer "F.SilkS"))
  (gr_text "TUSB320\nide v1" (at 122.6312 100.9396 90) (layer "F.SilkS"))
  (gr_text "887K" (at 120.2182 97.1804 270) (layer "F.SilkS"))
  (gr_text "VDET" (at 120.2182 94.5896 270) (layer "F.SilkS"))
  (gr_text "SBU1" (at 124.841 84.4804 90) (layer "F.SilkS"))
  (gr_text "D+" (at 124.841 89.5604 90) (layer "F.SilkS"))
  (gr_text "GND" (at 120.2182 81.9658 270) (layer "F.SilkS"))
  (gr_text "OUT2" (at 124.841 99.695 90) (layer "F.SilkS"))
  (gr_text "SBU2" (at 124.841 81.9404 90) (layer "F.SilkS"))
  (gr_text "EN_N" (at 124.841 94.6658 90) (layer "F.SilkS"))
  (gr_text "D-" (at 124.841 87.0204 90) (layer "F.SilkS"))
  (gr_text "CC2" (at 120.2182 89.5604 270) (layer "F.SilkS"))
  (gr_text "VBUS" (at 120.2182 84.4804 270) (layer "F.SilkS"))
  (gr_text "OUT1" (at 124.841 102.3112 90) (layer "F.SilkS"))
  (gr_text "PORT" (at 120.2182 92.1004 270) (layer "F.SilkS"))
  (gr_text "ID" (at 124.841 97.2058 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.7366 103.6828)
        (xy 117.3226 103.6828)
        (xy 117.3226 72.009)
        (xy 127.7366 72.009)
      )
    )
  )
)
