(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 92)
    (no_connects 0)
    (area 20.917855 69.280999 99.082145 100.846001)
    (thickness 1.6)
    (drawings 24)
    (tracks 497)
    (zones 0)
    (modules 44)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.15)
    (trace_clearance 0.15)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.125)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 43.5 77)
    (grid_origin 43.5 75.5)
    (visible_elements FFFFFB7F)
    (pcbplotparams
      (layerselection 0x010c0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C201-Pad2)")
  (net 3 "Net-(C202-Pad2)")
  (net 4 +3V3)
  (net 5 +5V)
  (net 6 "Net-(D601-Pad2)")
  (net 7 /LEDs/LED1)
  (net 8 "Net-(D602-Pad2)")
  (net 9 /LEDs/LED2)
  (net 10 "Net-(D603-Pad2)")
  (net 11 /Connectors/USB_DM)
  (net 12 /Connectors/USB_DP)
  (net 13 "Net-(R201-Pad2)")
  (net 14 "Net-(R202-Pad1)")
  (net 15 /CAN/CAN_S)
  (net 16 /CAN/CAN_H)
  (net 17 /CAN/CAN_L)
  (net 18 /Connectors/NRST)
  (net 19 "Net-(U201-Pad25)")
  (net 20 "Net-(U201-Pad26)")
  (net 21 "Net-(U201-Pad27)")
  (net 22 "Net-(U201-Pad28)")
  (net 23 "Net-(U201-Pad30)")
  (net 24 "Net-(U201-Pad31)")
  (net 25 /Connectors/SWDIO)
  (net 26 /Connectors/SWCLK)
  (net 27 /MCU/CAN_RX)
  (net 28 /MCU/CAN_TX)
  (net 29 /MCU/BOOT0)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /CAN/CAN_H)
    (add_net /CAN/CAN_L)
    (add_net /CAN/CAN_S)
    (add_net /Connectors/NRST)
    (add_net /Connectors/SWCLK)
    (add_net /Connectors/SWDIO)
    (add_net /Connectors/USB_DM)
    (add_net /Connectors/USB_DP)
    (add_net /LEDs/LED1)
    (add_net /LEDs/LED2)
    (add_net /MCU/BOOT0)
    (add_net /MCU/CAN_RX)
    (add_net /MCU/CAN_TX)
    (add_net GND)
    (add_net "Net-(C201-Pad2)")
    (add_net "Net-(C202-Pad2)")
    (add_net "Net-(D601-Pad2)")
    (add_net "Net-(D602-Pad2)")
    (add_net "Net-(D603-Pad2)")
    (add_net "Net-(R201-Pad2)")
    (add_net "Net-(R202-Pad1)")
    (add_net "Net-(U201-Pad25)")
    (add_net "Net-(U201-Pad26)")
    (add_net "Net-(U201-Pad27)")
    (add_net "Net-(U201-Pad28)")
    (add_net "Net-(U201-Pad30)")
    (add_net "Net-(U201-Pad31)")
  )
  (module Crystals:ABM3 (layer F.Cu) (tedit 57348AD0)
    (at 68.55 85.25 90)
    (descr "Abracon Miniature Ceramic Smd Crystal http://www.abracon.com/Resonators/abm3.pdf")
    (tags "smd crystal")
    (attr smd)
    (fp_text reference Y201 (at 0 0 180) (layer F.Fab))
    (fp_text value 8MHz (at 0 3 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 1 smd rect (at -2.05 0 90) (size 1.9 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57348951)
    (at 57.35 85.2 180)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U201 (at 0 0 180) (layer F.Fab))
    (fp_text value STM32F072C8Tx (at 0 6 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (pad 3 smd rect (at -4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
    (pad 6 smd rect (at -4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
    (pad 7 smd rect (at -4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 8 smd rect (at -4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 10 smd rect (at -4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (pad 11 smd rect (at -4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (pad 12 smd rect (at -4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at -0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 0.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 25 smd rect (at 4.35 2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U201-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U201-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U201-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U201-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 4.35 0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U201-Pad30)"))
    (pad 31 smd rect (at 4.35 -0.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U201-Pad31)"))
    (pad 32 smd rect (at 4.35 -0.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 33 smd rect (at 4.35 -1.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 34 smd rect (at 4.35 -1.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad 35 smd rect (at 4.35 -2.25 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 38 smd rect (at 2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
    (pad 43 smd rect (at -0.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (pad 45 smd rect (at -1.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 46 smd rect (at -1.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 47 smd rect (at -2.25 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 573489C1)
    (at 74 93.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R401 (at 0 0 90) (layer F.Fab))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 573489AB)
    (at 59.35 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C206 (at 0 0 270) (layer F.Fab))
    (fp_text value 100nF (at 3.13 -0.67 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 573489BC)
    (at 72.4 93.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C403 (at 0 0 90) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 573489A5)
    (at 57.6 92.9 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R203 (at 0 0 90) (layer F.Fab))
    (fp_text value R (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
  )
  (module usb:Molex-Micro-USB-B-Middle-Mount (layer F.Cu) (tedit 5734895D)
    (at 47 85)
    (fp_text reference P501 (at -1.7 0 90) (layer F.Fab))
    (fp_text value USB_OTG (at -0.1 -8.2) (layer F.Fab) hide)
    (pad 6 smd rect (at 2.75 2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.75 -2.2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -3.65 -5.25) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.55 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.875 1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.875 0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0.875 -1.3) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.875 -0.65) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /Connectors/USB_DM))
    (pad 3 smd rect (at 0.875 0) (size 1.25 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /Connectors/USB_DP))
    (pad 6 smd rect (at -3.65 5.05) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/hd/kicad/footprints/usb.pretty/molex-47491-0001.wrl
      (at (xyz -0.08500000000000001 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 573489C8)
    (at 64.9 87.55 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C201 (at 0 0 180) (layer F.Fab))
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C201-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 573489CD)
    (at 64.9 86 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C202 (at 0 0 180) (layer F.Fab))
    (fp_text value 20pF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C202-Pad2)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 573489D5)
    (at 64.9 82.9)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C203 (at 0 0) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57348990)
    (at 50.95 90.05 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C204 (at 0 0 180) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57348A0F)
    (at 52.4 77.8 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C205 (at 0 0 90) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 573489B0)
    (at 61.1 92.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C207 (at 0 0 270) (layer F.Fab))
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 573489E4)
    (at 71.65 82.05 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C301 (at 0 0 270) (layer F.Fab))
    (fp_text value 10uF (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 573489E7)
    (at 71.65 78.4 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C303 (at 0 0 270) (layer F.Fab))
    (fp_text value 10uF (at 0 0.01 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 573489B7)
    (at 62.85 93.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C402 (at 0 0 270) (layer F.Fab))
    (fp_text value 100nF (at 0.04 -0.07 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 573489FA)
    (at 60.35 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D601 (at 0 0 90) (layer F.Fab))
    (fp_text value LED (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /LEDs/LED1))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57348A03)
    (at 57.15 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D602 (at 0 0 90) (layer F.Fab))
    (fp_text value LED (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 9 /LEDs/LED2))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57348A0B)
    (at 53.95 77.75 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D603 (at 0 0 90) (layer F.Fab))
    (fp_text value LED (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 1 smd rect (at -0.7493 0 270) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57348997)
    (at 52.6 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R201 (at 0 0 90) (layer F.Fab))
    (fp_text value 4K7 (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5734899C)
    (at 54.2 93.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R202 (at 0 0 270) (layer F.Fab))
    (fp_text value 4K7 (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R202-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 573489A1)
    (at 55.8 93.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R204 (at 0 0 90) (layer F.Fab))
    (fp_text value 1K (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /MCU/BOOT0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 573489F5)
    (at 61.95 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R601 (at 0 0 270) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D601-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 573489FE)
    (at 58.75 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R602 (at 0 0 270) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D602-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57348A07)
    (at 55.6 77.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R603 (at 0 0 270) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D603-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer F.Cu) (tedit 573489EC)
    (at 67.05 79 90)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U301 (at 0 0 90) (layer F.Fab))
    (fp_text value MCP1754ST-3302E/MB (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.50114 1.85166 90) (size 1.00076 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0 -1.09982 90) (size 1.99898 2.99974) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd trapezoid (at 0 0.7493 270) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57348955)
    (at 67.8 91.8)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U401 (at -0.1 -0.1 90) (layer F.Fab))
    (fp_text value TJA1051/3 (at 0 3.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /MCU/CAN_TX))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MCU/CAN_RX))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CAN/CAN_S))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tagconnect:TC2030-NL (layer F.Cu) (tedit 57228EC4)
    (at 45.2 93 180)
    (fp_text reference X501 (at -0.6 -1.5 180) (layer F.SilkS) hide)
    (fp_text value CON_SWD (at 0 -2.54 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 2.54 -1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2.54 1.016 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
    (pad 5 connect circle (at 1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 18 /Connectors/NRST))
    (pad 3 connect circle (at 0 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 connect circle (at -1.27 0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 6 connect circle (at 1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 connect circle (at -1.27 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 26 /Connectors/SWCLK))
    (pad 4 connect circle (at 0 -0.635 180) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 25 /Connectors/SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0 180) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask F.SilkS))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C55)
    (at 51.5 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TX (at -1.8 0 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(U201-Pad30)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C68)
    (at 54 86)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference RX (at 2 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 "Net-(U201-Pad31)"))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 573486BA)
    (at 43.5 77)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 2.6 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5734841B)
    (at 76.5 93.2)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5734893D)
    (at 76 76.5)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -2.7 -1.1) (layer F.SilkS) hide)
    (fp_text value Dummy_FIDUCIAL_Passermarke_Type1_RevE_Date16Nov2011 (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 573489D1)
    (at 64.9 84.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C208 (at 0 0) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /Connectors/NRST))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228D02)
    (at 52.5 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCL (at -0.55 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 13 "Net-(R201-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228CEF)
    (at 55 92)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SDA (at 0.7 -1.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 14 "Net-(R202-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BF4)
    (at 54 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference CS (at 1.95 0.55) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 19 "Net-(U201-Pad25)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228BE4)
    (at 51.5 80.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference SCK (at -2.35 0.6) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "Net-(U201-Pad26)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C15)
    (at 51.5 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MISO (at -2.55 0.1 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 21 "Net-(U201-Pad27)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 57228C24)
    (at 54 83)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference MOSI (at 2.75 0.05 180) (layer B.SilkS))
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "Net-(U201-Pad28)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228AA1)
    (at 48.15 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W301 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 5 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Big (layer B.Cu) (tedit 57228A9D)
    (at 44.3 78.5)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference W302 (at 0 3) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -3) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 3 3) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 573489E0)
    (at 71.65 85.5 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R402 (at 0 0 270) (layer F.Fab))
    (fp_text value dnp (at 0 -0.01 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAN/CAN_H))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /CAN/CAN_L))
  )
  (module subd9:DB9M_CI (layer F.Cu) (tedit 57348D2E)
    (at 79 85 270)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference X502 (at 0 1.05 270) (layer F.Fab))
    (fp_text value SUB-D9 (at 0 -3.048 270) (layer F.Fab) hide)
    (pad 2 connect rect (at 2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 17 /CAN/CAN_L))
    (pad 3 connect rect (at 0 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect rect (at -2.794 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 5 connect rect (at -5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 1 connect rect (at 5.588 2.667 270) (size 1.778 5.08) (layers F.Cu F.Mask))
    (pad 9 connect rect (at -4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 8 connect rect (at -1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 1.397 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 16 /CAN/CAN_H))
    (pad 6 connect rect (at 4.191 2.667 270) (size 1.778 5.08) (layers B.Cu B.Mask))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (gr_text T (at 71.7 85.5 90) (layer F.SilkS))
  (gr_text B (at 57.6 92.9 90) (layer F.SilkS))
  (dimension 19.95 (width 0.25) (layer Dwgs.User)
    (gr_text "19,950 mm" (at 37.65 84.975 270) (layer Dwgs.User))
    (feature1 (pts (xy 41.4 94.95) (xy 36.65 94.95)))
    (feature2 (pts (xy 41.4 75) (xy 36.65 75)))
    (crossbar (pts (xy 38.65 75) (xy 38.65 94.95)))
    (arrow1a (pts (xy 38.65 94.95) (xy 38.063579 93.823496)))
    (arrow1b (pts (xy 38.65 94.95) (xy 39.236421 93.823496)))
    (arrow2a (pts (xy 38.65 75) (xy 38.063579 76.126504)))
    (arrow2b (pts (xy 38.65 75) (xy 39.236421 76.126504)))
  )
  (dimension 37.65 (width 0.25) (layer Dwgs.User)
    (gr_text "37,650 mm" (at 60.275 71.300001) (layer Dwgs.User))
    (feature1 (pts (xy 41.45 75) (xy 41.45 70.300001)))
    (feature2 (pts (xy 79.1 75) (xy 79.1 70.300001)))
    (crossbar (pts (xy 79.1 72.300001) (xy 41.45 72.300001)))
    (arrow1a (pts (xy 41.45 72.300001) (xy 42.576504 71.71358)))
    (arrow1b (pts (xy 41.45 72.300001) (xy 42.576504 72.886422)))
    (arrow2a (pts (xy 79.1 72.300001) (xy 77.973496 71.71358)))
    (arrow2b (pts (xy 79.1 72.300001) (xy 77.973496 72.886422)))
  )
  (gr_text PWR (at 54 75.9) (layer F.SilkS))
  (gr_text RX (at 60.35 75.9) (layer F.SilkS))
  (gr_text TX (at 57.15 75.9) (layer F.SilkS))
  (gr_text "candleLight v1.1" (at 69.1 77.3) (layer B.SilkS))
  (gr_text http://bytewerk.org (at 70.55 93.6) (layer B.SilkS))
  (gr_text CAN_H (at 71.2 86.5) (layer B.SilkS))
  (gr_text +5V (at 48.6 76.1) (layer B.SilkS))
  (gr_text GND (at 44.25 76.1) (layer B.SilkS))
  (gr_line (start 41.4 75) (end 41.4 81.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 75) (end 79.1 95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 47 81.9) (end 47 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 81.1) (end 46.2 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 81.9) (end 46.2 81.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 46.2 88.1) (end 47 88.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 88.9) (end 46.2 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 95) (end 41.4 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.1 95) (end 41.4 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 41.4 75) (end 79.1 75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 74) (xy 80 74) (xy 80 96) (xy 40.5 96) (xy 40.5 74)
        (xy 40.5 74)
      )
    )
  )
  (zone (net 4) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2) (smoothing fillet))
    (polygon
      (pts
        (xy 40 73.5) (xy 80.5 73.5) (xy 80.5 96.5) (xy 40 96.5)
      )
    )
  )
)
