(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 23)
    (no_connects 0)
    (area 92.887 85.268999 148.259 112.343001)
    (thickness 1.6)
    (drawings 13)
    (tracks 46)
    (zones 0)
    (modules 13)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 3)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /R1_EN)
  (net 2 GND)
  (net 3 /R2_EN)
  (net 4 /BATT_POS)
  (net 5 /R2_FET)
  (net 6 /R1_FET)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BATT_POS)
    (add_net /R1_EN)
    (add_net /R1_FET)
    (add_net /R2_EN)
    (add_net /R2_FET)
    (add_net GND)
  )
  (net_class Bigger ""
    (clearance 0.1524)
    (trace_width 1)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Small ""
    (clearance 0.16)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59D7973F)
    (at 108.331 99.949 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /R1_EN))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59D79744)
    (at 122.936 99.314 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /R2_EN))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Philmore_TB132_02x5mm_Straight (layer F.Cu) (tedit 59D7970D)
    (at 99.822 93.98 90)
    (descr "2-way 5.0mm pitch terminal block, http://www.philmore-datak.com/mc/Page%20197.pdf")
    (tags "screw terminal block")
    (fp_text reference "" (at 2.5 -6 90) (layer F.SilkS))
    (fp_text value "" (at 2.5 6.9 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0.3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 4 /BATT_POS))
    (model ${KISYS3DMOD}/Connectors_Terminal_Blocks.3dshapes/TerminalBlock_Philmore_TB132_02x5mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Philmore_TB133_03x5mm_Straight (layer F.Cu) (tedit 59D79722)
    (at 141.224 92.456 270)
    (descr "3-way 5.0mm pitch terminal block, http://www.philmore-datak.com/mc/Page%20197.pdf")
    (tags "screw terminal block")
    (fp_text reference J2 (at 5 -6 270) (layer F.SilkS))
    (fp_text value "" (at 5 6.9 270) (layer F.Fab))
    (fp_text user %R (at 5 0.3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 1 /R1_EN))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 3 /R2_EN))
    (pad 3 thru_hole circle (at 10 0 270) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_Terminal_Blocks.3dshapes/TerminalBlock_Philmore_TB133_03x5mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Philmore_TB132_02x5mm_Straight (layer F.Cu) (tedit 59D79705)
    (at 99.822 107.95 90)
    (descr "2-way 5.0mm pitch terminal block, http://www.philmore-datak.com/mc/Page%20197.pdf")
    (tags "screw terminal block")
    (fp_text reference "" (at 2.5 -6 90) (layer F.SilkS))
    (fp_text value "" (at 2.5 6.9 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0.3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 4 /BATT_POS))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_Terminal_Blocks.3dshapes/TerminalBlock_Philmore_TB132_02x5mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer F.Cu) (tedit 59D7974E)
    (at 113.538 92.964 270)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R1 (at -0.0254 0 270) (layer F.SilkS))
    (fp_text value "" (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /BATT_POS))
    (pad 2 smd rect (at 3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /R1_FET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer F.Cu) (tedit 59D79755)
    (at 118.11 92.964 270)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R2 (at 0 -0.1524 270) (layer F.SilkS))
    (fp_text value "" (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /BATT_POS))
    (pad 2 smd rect (at 3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /R1_FET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer F.Cu) (tedit 59D79759)
    (at 127.762 92.964 270)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R3 (at 0 -0.2286 270) (layer F.SilkS))
    (fp_text value "" (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /BATT_POS))
    (pad 2 smd rect (at 3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /R2_FET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer F.Cu) (tedit 59D79760)
    (at 132.334 92.964 270)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference R4 (at 0 -0.1016 270) (layer F.SilkS))
    (fp_text value "" (at 0 2.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /BATT_POS))
    (pad 2 smd rect (at 3.95 0 270) (size 2.7 3.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /R2_FET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D7974C)
    (at 108.331 97.409 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /R1_EN))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 59D79749)
    (at 122.936 97.282 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.0508 1.27 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /R2_EN))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Batter-Measurement-Tool:DPAK369C (layer F.Cu) (tedit 59D7976C)
    (at 109.728 101.854 270)
    (fp_text reference Q1 (at 2.8448 -1.2192 270) (layer F.SilkS))
    (fp_text value "" (at 2.794 4.064 270) (layer F.Fab))
    (pad 3 smd rect (at 5.334 1.524 270) (size 1.6 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.762 1.524 270) (size 1.6 3) (layers F.Cu F.Paste F.Mask)
      (net 1 /R1_EN))
    (pad 1 smd rect (at 3.048 -5.969 270) (size 5.8 6.8) (layers F.Cu F.Paste F.Mask)
      (net 6 /R1_FET))
  )
  (module Batter-Measurement-Tool:DPAK369C (layer F.Cu) (tedit 59D79767)
    (at 124.206 101.854 270)
    (fp_text reference Q2 (at 3.048 -1.2192 270) (layer F.SilkS))
    (fp_text value "" (at 2.794 4.064 270) (layer F.Fab))
    (pad 3 smd rect (at 5.334 1.524 270) (size 1.6 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.762 1.524 270) (size 1.6 3) (layers F.Cu F.Paste F.Mask)
      (net 3 /R2_EN))
    (pad 1 smd rect (at 3.048 -5.969 270) (size 5.8 6.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /R2_FET))
  )
  (gr_text "CONT.\nG 2 1" (at 142.0368 108.5088 90) (layer F.SilkS))
  (gr_text "+ MEAS." (at 110.617 110.363) (layer F.SilkS))
  (gr_text - (at 107.6452 93.9546) (layer F.SilkS))
  (gr_text + (at 107.8992 88.8238) (layer F.SilkS))
  (gr_text BATT. (at 107.95 91.4146) (layer F.SilkS))
  (gr_line (start 95.758 85.344) (end 144.78 85.344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.726 110.236) (end 93.726 87.376) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 112.268) (end 95.758 112.268) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.812 87.376) (end 146.812 110.236) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95.758 87.376) (end 93.726 87.376) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 95.758 110.236) (end 95.758 112.268) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 110.236) (end 146.812 110.236) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 144.78 87.376) (end 144.78 85.344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.472 85.344) (xy 146.812 85.344) (xy 146.812 112.268) (xy 93.472 112.268)
      )
    )
  )
  (zone (net 4) (net_name /BATT_POS) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.366 90.932) (xy 98.298 90.932) (xy 98.298 87.376) (xy 134.366 87.376)
      )
    )
  )
  (zone (net 6) (net_name /R1_FET) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.142 98.298) (xy 119.38 99.06) (xy 119.38 108.458) (xy 111.506 108.458) (xy 111.506 94.742)
        (xy 120.142 94.742)
      )
    )
  )
  (zone (net 5) (net_name /R2_FET) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.366 108.204) (xy 125.73 108.204) (xy 125.73 94.996) (xy 134.366 94.996)
      )
    )
  )
)
