(kicad_pcb (version 20171130) (host pcbnew 6.0.0-rc1-unknown-968ea98~66~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 642)
    (zones 0)
    (modules 39)
    (nets 92)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.127)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.6096 0.254)
    (uvia_size 0.254)
    (uvia_drill 0.1016)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.1016)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(J6-Pad3)")
  (net 4 "Net-(J6-Pad4)")
  (net 5 "Net-(S1-Pad1)")
  (net 6 "Net-(Y1-Pad1)")
  (net 7 "Net-(U1-Pad62)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J1-Pad3)")
  (net 10 "Net-(J1-Pad7)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 "Net-(J1-Pad8)")
  (net 14 "Net-(J2-Pad1)")
  (net 15 "Net-(J2-Pad3)")
  (net 16 "Net-(J2-Pad7)")
  (net 17 "Net-(J2-Pad2)")
  (net 18 "Net-(J2-Pad4)")
  (net 19 "Net-(J2-Pad8)")
  (net 20 "Net-(J3-Pad8)")
  (net 21 "Net-(J3-Pad4)")
  (net 22 "Net-(J3-Pad2)")
  (net 23 "Net-(J3-Pad7)")
  (net 24 "Net-(J3-Pad3)")
  (net 25 "Net-(J3-Pad1)")
  (net 26 "Net-(J4-Pad8)")
  (net 27 "Net-(J4-Pad4)")
  (net 28 "Net-(J4-Pad2)")
  (net 29 "Net-(J4-Pad7)")
  (net 30 "Net-(J4-Pad3)")
  (net 31 "Net-(J4-Pad1)")
  (net 32 "Net-(J5-Pad1)")
  (net 33 "Net-(J5-Pad3)")
  (net 34 "Net-(J5-Pad7)")
  (net 35 "Net-(J5-Pad2)")
  (net 36 "Net-(J5-Pad4)")
  (net 37 "Net-(J5-Pad8)")
  (net 38 "Net-(J7-Pad2)")
  (net 39 "Net-(J7-Pad3)")
  (net 40 "Net-(J7-Pad4)")
  (net 41 "Net-(J7-Pad6)")
  (net 42 "Net-(U1-Pad14)")
  (net 43 "Net-(U1-Pad15)")
  (net 44 "Net-(U1-Pad18)")
  (net 45 "Net-(U1-Pad19)")
  (net 46 "Net-(U1-Pad61)")
  (net 47 "Net-(U1-Pad63)")
  (net 48 "Net-(U1-Pad64)")
  (net 49 "Net-(U1-Pad65)")
  (net 50 "Net-(U1-Pad82)")
  (net 51 "Net-(U1-Pad83)")
  (net 52 "Net-(U1-Pad84)")
  (net 53 "Net-(U1-Pad89)")
  (net 54 "Net-(J1-Pad5)")
  (net 55 "Net-(J1-Pad6)")
  (net 56 "Net-(J2-Pad5)")
  (net 57 "Net-(J2-Pad6)")
  (net 58 "Net-(J3-Pad6)")
  (net 59 "Net-(J3-Pad5)")
  (net 60 "Net-(J4-Pad6)")
  (net 61 "Net-(J4-Pad5)")
  (net 62 "Net-(J5-Pad5)")
  (net 63 "Net-(J5-Pad6)")
  (net 64 "Net-(D1-Pad2)")
  (net 65 "Net-(D1-Pad1)")
  (net 66 "Net-(D2-Pad1)")
  (net 67 "Net-(D2-Pad2)")
  (net 68 "Net-(D5-Pad2)")
  (net 69 "Net-(D5-Pad1)")
  (net 70 "Net-(D6-Pad1)")
  (net 71 "Net-(D6-Pad2)")
  (net 72 "Net-(D7-Pad1)")
  (net 73 "Net-(D7-Pad2)")
  (net 74 "Net-(D8-Pad2)")
  (net 75 "Net-(D8-Pad1)")
  (net 76 "Net-(D9-Pad1)")
  (net 77 "Net-(D9-Pad2)")
  (net 78 "Net-(D10-Pad2)")
  (net 79 "Net-(D10-Pad1)")
  (net 80 "Net-(U1-Pad29)")
  (net 81 "Net-(U1-Pad30)")
  (net 82 "Net-(U1-Pad36)")
  (net 83 "Net-(U1-Pad37)")
  (net 84 "Net-(S2-PadA)")
  (net 85 "Net-(S2-PadB)")
  (net 86 "Net-(S2-PadC)")
  (net 87 "Net-(S2-PadCTR)")
  (net 88 "Net-(S2-PadD)")
  (net 89 "Net-(D3-Pad2)")
  (net 90 "Net-(D3-Pad1)")
  (net 91 "Net-(D4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.254)
    (uvia_drill 0.1016)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad4)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S2-PadA)")
    (add_net "Net-(S2-PadB)")
    (add_net "Net-(S2-PadC)")
    (add_net "Net-(S2-PadCTR)")
    (add_net "Net-(S2-PadD)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad61)")
    (add_net "Net-(U1-Pad62)")
    (add_net "Net-(U1-Pad63)")
    (add_net "Net-(U1-Pad64)")
    (add_net "Net-(U1-Pad65)")
    (add_net "Net-(U1-Pad82)")
    (add_net "Net-(U1-Pad83)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad89)")
    (add_net "Net-(Y1-Pad1)")
  )
  (module Connectors:1X04_1MM_RA (layer F.Cu) (tedit 200000)
    (at 133.35 68.58 180)
    (descr "SMD- 4 PIN RIGHT ANGLE")
    (tags "SMD- 4 PIN RIGHT ANGLE")
    (attr smd)
    (fp_text reference J6 (at 2.794 -0.635) (layer F.SilkS))
    (fp_text value QWIIC_CONNECTORJS-1MM (at 8.255 6.35) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.4986 0 180) (size 0.59944 1.34874) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -0.49784 0 180) (size 0.59944 1.34874) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0.49784 0 180) (size 0.59944 1.34874) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J6-Pad3)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 1.4986 0 180) (size 0.59944 1.34874) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J6-Pad4)") (solder_mask_margin 0.1016))
    (pad NC1 smd rect (at 2.79908 3.67284 180) (size 1.19888 1.99898) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
    (pad NC2 smd rect (at -2.79908 3.67284 180) (size 1.19888 1.99898) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Switches:TACTILE_SWITCH_SMD_4.6X2.8MM (layer F.Cu) (tedit 200000)
    (at 140.335 67.31 270)
    (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 4.6 X 2.8MM")
    (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 4.6 X 2.8MM")
    (attr smd)
    (fp_text reference S1 (at 0 0) (layer F.SilkS))
    (fp_text value MOMENTARY-SWITCH-SPST-SMD-4.6X2.8MM (at -6.35 -1.905) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.04978 0.79756 270) (size 0.89916 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(S1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 2.04978 0.79756 270) (size 0.89916 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(S1-Pad1)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 2.04978 -0.79756 270) (size 0.89916 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -2.04978 -0.79756 270) (size 0.89916 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module Clocks:OSCILLATOR-SMD-5X3.2 (layer F.Cu) (tedit 59628541)
    (at 146.685 82.55 180)
    (descr "5.0X3.2 MM 4-SMD OSCILLATOR (POLARIZED)")
    (tags "5.0X3.2 MM 4-SMD OSCILLATOR (POLARIZED)")
    (attr smd)
    (fp_text reference Y1 (at -1.27 2.54 180) (layer F.SilkS))
    (fp_text value OSCILLATOR-33MHZ (at -6.985 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.27 1.09982 180) (size 1.397 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(Y1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 1.27 1.09982 180) (size 1.397 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 1.27 -1.09982 180) (size 1.397 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad62)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -1.27 -1.09982 180) (size 1.397 1.1938) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3) (solder_mask_margin 0.1016))
  )
  (module Connector_Samtec_HLE_SMD:Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5B5713AB)
    (at 133.35 97.79)
    (descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-106-02-xxx-DV-BE, 6 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xxx-dv-xx-xx-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-dv-footprint.pdf), generated with kicad-footprint-generator")
    (tags "connector Samtec HLE top entry")
    (attr smd)
    (fp_text reference J1 (at 0 -4.76) (layer F.SilkS))
    (fp_text value Conn_02x06_Top_Bottom (at 0 4.76) (layer F.Fab))
    (fp_text user %R (at 0 1.84) (layer F.Fab))
    (pad "" np_thru_hole circle (at -6.35 -1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.35 1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 -1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 -1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 -1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 -1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 1.27) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -6.35 -2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -3.81 -2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at -1.27 -2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J1-Pad5)"))
    (pad 7 smd rect (at 1.27 -2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 9 smd rect (at 3.81 -2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 6.35 -2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -6.35 2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -3.81 2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at -1.27 2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J1-Pad6)"))
    (pad 8 smd rect (at 1.27 2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad8)"))
    (pad 10 smd rect (at 3.81 2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 6.35 2.72) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_Samtec_HLE_SMD.3dshapes/Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Samtec_HLE_SMD:Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5B5713AB)
    (at 118.11 71.12 90)
    (descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-106-02-xxx-DV-BE, 6 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xxx-dv-xx-xx-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-dv-footprint.pdf), generated with kicad-footprint-generator")
    (tags "connector Samtec HLE top entry")
    (attr smd)
    (fp_text reference J2 (at -8.89 0 180) (layer F.SilkS))
    (fp_text value Conn_02x06_Top_Bottom (at 0 4.76 90) (layer F.Fab))
    (fp_text user %R (at 0 1.84 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -6.35 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.35 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -6.35 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (pad 3 smd rect (at -3.81 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad3)"))
    (pad 5 smd rect (at -1.27 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J2-Pad5)"))
    (pad 7 smd rect (at 1.27 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad7)"))
    (pad 9 smd rect (at 3.81 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 6.35 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -6.35 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad2)"))
    (pad 4 smd rect (at -3.81 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 6 smd rect (at -1.27 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J2-Pad6)"))
    (pad 8 smd rect (at 1.27 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad8)"))
    (pad 10 smd rect (at 3.81 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 6.35 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_Samtec_HLE_SMD.3dshapes/Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Samtec_HLE_SMD:Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5B5713AB)
    (at 118.11 93.98 90)
    (descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-106-02-xxx-DV-BE, 6 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xxx-dv-xx-xx-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-dv-footprint.pdf), generated with kicad-footprint-generator")
    (tags "connector Samtec HLE top entry")
    (attr smd)
    (fp_text reference J3 (at 8.89 0 180) (layer F.SilkS))
    (fp_text value Conn_02x06_Top_Bottom (at 0 4.76 90) (layer F.Fab))
    (fp_text user %R (at 0 1.84 90) (layer F.Fab))
    (pad 12 smd rect (at 6.35 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at 3.81 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 1.27 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad8)"))
    (pad 6 smd rect (at -1.27 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J3-Pad6)"))
    (pad 4 smd rect (at -3.81 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad4)"))
    (pad 2 smd rect (at -6.35 2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad2)"))
    (pad 11 smd rect (at 6.35 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 9 smd rect (at 3.81 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 1.27 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad7)"))
    (pad 5 smd rect (at -1.27 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J3-Pad5)"))
    (pad 3 smd rect (at -3.81 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad3)"))
    (pad 1 smd rect (at -6.35 -2.72 90) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad1)"))
    (pad "" np_thru_hole circle (at 6.35 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.35 1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.35 -1.27 90) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Samtec_HLE_SMD.3dshapes/Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Samtec_HLE_SMD:Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5B5713AB)
    (at 148.59 71.12 270)
    (descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-106-02-xxx-DV-BE, 6 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xxx-dv-xx-xx-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-dv-footprint.pdf), generated with kicad-footprint-generator")
    (tags "connector Samtec HLE top entry")
    (attr smd)
    (fp_text reference J4 (at 8.89 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x06_Top_Bottom (at 0 4.76 270) (layer F.Fab))
    (fp_text user %R (at 0 1.84 270) (layer F.Fab))
    (pad 12 smd rect (at 6.35 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at 3.81 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 1.27 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J4-Pad8)"))
    (pad 6 smd rect (at -1.27 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J4-Pad6)"))
    (pad 4 smd rect (at -3.81 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad4)"))
    (pad 2 smd rect (at -6.35 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J4-Pad2)"))
    (pad 11 smd rect (at 6.35 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 9 smd rect (at 3.81 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 1.27 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J4-Pad7)"))
    (pad 5 smd rect (at -1.27 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J4-Pad5)"))
    (pad 3 smd rect (at -3.81 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J4-Pad3)"))
    (pad 1 smd rect (at -6.35 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad1)"))
    (pad "" np_thru_hole circle (at 6.35 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.35 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.35 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Samtec_HLE_SMD.3dshapes/Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Samtec_HLE_SMD:Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5B5713AB)
    (at 148.59 93.98 270)
    (descr "Samtec HLE .100\" Tiger Beam Cost-effective Single Beam Socket Strip, HLE-106-02-xxx-DV-BE, 6 Pins per row (http://suddendocs.samtec.com/prints/hle-1xx-02-xxx-dv-xx-xx-xx-mkt.pdf, http://suddendocs.samtec.com/prints/hle-dv-footprint.pdf), generated with kicad-footprint-generator")
    (tags "connector Samtec HLE top entry")
    (attr smd)
    (fp_text reference J5 (at -8.89 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x06_Top_Bottom (at 0 4.76 270) (layer F.Fab))
    (fp_text user %R (at 0 1.84 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at -6.35 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.35 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.81 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.27 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.81 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 -1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.35 1.27 270) (size 0.97 0.97) (drill 0.97) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -6.35 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J5-Pad1)"))
    (pad 3 smd rect (at -3.81 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J5-Pad3)"))
    (pad 5 smd rect (at -1.27 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J5-Pad5)"))
    (pad 7 smd rect (at 1.27 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J5-Pad7)"))
    (pad 9 smd rect (at 3.81 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 6.35 -2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -6.35 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J5-Pad2)"))
    (pad 4 smd rect (at -3.81 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J5-Pad4)"))
    (pad 6 smd rect (at -1.27 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J5-Pad6)"))
    (pad 8 smd rect (at 1.27 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J5-Pad8)"))
    (pad 10 smd rect (at 3.81 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 6.35 2.72 270) (size 1.27 1.68) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_Samtec_HLE_SMD.3dshapes/Samtec_HLE-106-02-xxx-DV-BE_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical (layer F.Cu) (tedit 5A29CEA9)
    (at 126.365 67.945 270)
    (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
    (tags "tag connect programming header pogo pins")
    (attr virtual)
    (fp_text reference J7 (at -3.175 1.905) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 0 -2.3 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (fp_text user KEEPOUT (at 0 0 270) (layer Cmts.User))
    (pad "" np_thru_hole circle (at 2.54 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 connect circle (at -1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 2 connect circle (at -1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 38 "Net-(J7-Pad2)"))
    (pad 3 connect circle (at 0 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 39 "Net-(J7-Pad3)"))
    (pad 4 connect circle (at 0 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 40 "Net-(J7-Pad4)"))
    (pad 5 connect circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 6 connect circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 41 "Net-(J7-Pad6)"))
  )
  (module Package_QFP:LQFP-100_14x14mm_P0.5mm (layer F.Cu) (tedit 5A02F146)
    (at 133.35 82.55)
    (descr "LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at -9.525 -7.62) (layer F.SilkS))
    (fp_text value LCMXO2-TQ100 (at 0 9.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -7.9 -6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad8)"))
    (pad 2 smd rect (at -7.9 -5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J2-Pad6)"))
    (pad 3 smd rect (at -7.9 -5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 4 smd rect (at -7.9 -4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad2)"))
    (pad 5 smd rect (at -7.9 -4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at -7.9 -3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -7.9 -3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at -7.9 -2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J2-Pad5)"))
    (pad 9 smd rect (at -7.9 -2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad3)"))
    (pad 10 smd rect (at -7.9 -1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (pad 11 smd rect (at -7.9 -1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 12 smd rect (at -7.9 -0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad7)"))
    (pad 13 smd rect (at -7.9 0) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J3-Pad5)"))
    (pad 14 smd rect (at -7.9 0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -7.9 1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -7.9 1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad3)"))
    (pad 17 smd rect (at -7.9 2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad1)"))
    (pad 18 smd rect (at -7.9 2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at -7.9 3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at -7.9 3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad8)"))
    (pad 21 smd rect (at -7.9 4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J3-Pad6)"))
    (pad 22 smd rect (at -7.9 4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at -7.9 5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 24 smd rect (at -7.9 5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J3-Pad4)"))
    (pad 25 smd rect (at -7.9 6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J3-Pad2)"))
    (pad 26 smd rect (at -6 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 27 smd rect (at -5.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 28 smd rect (at -5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 29 smd rect (at -4.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at -4 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at -3.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 32 smd rect (at -3 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J1-Pad5)"))
    (pad 33 smd rect (at -2.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 34 smd rect (at -2 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(D1-Pad1)"))
    (pad 35 smd rect (at -1.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(D2-Pad1)"))
    (pad 36 smd rect (at -1 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U1-Pad36)"))
    (pad 37 smd rect (at -0.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 0 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D5-Pad1)"))
    (pad 39 smd rect (at 0.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D6-Pad1)"))
    (pad 40 smd rect (at 1 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(D7-Pad1)"))
    (pad 41 smd rect (at 1.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(D8-Pad1)"))
    (pad 42 smd rect (at 2 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D9-Pad1)"))
    (pad 43 smd rect (at 2.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(D10-Pad1)"))
    (pad 44 smd rect (at 3 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 45 smd rect (at 3.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J1-Pad6)"))
    (pad 46 smd rect (at 4 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 47 smd rect (at 4.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad8)"))
    (pad 48 smd rect (at 5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 49 smd rect (at 5.5 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 50 smd rect (at 6 7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 51 smd rect (at 7.9 6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J5-Pad8)"))
    (pad 52 smd rect (at 7.9 5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(J5-Pad6)"))
    (pad 53 smd rect (at 7.9 5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J5-Pad4)"))
    (pad 54 smd rect (at 7.9 4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J5-Pad2)"))
    (pad 55 smd rect (at 7.9 4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 56 smd rect (at 7.9 3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 57 smd rect (at 7.9 3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J5-Pad7)"))
    (pad 58 smd rect (at 7.9 2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(J5-Pad5)"))
    (pad 59 smd rect (at 7.9 2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J5-Pad3)"))
    (pad 60 smd rect (at 7.9 1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J5-Pad1)"))
    (pad 61 smd rect (at 7.9 1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad61)"))
    (pad 62 smd rect (at 7.9 0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad62)"))
    (pad 63 smd rect (at 7.9 0) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad63)"))
    (pad 64 smd rect (at 7.9 -0.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad64)"))
    (pad 65 smd rect (at 7.9 -1) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad65)"))
    (pad 66 smd rect (at 7.9 -1.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J4-Pad7)"))
    (pad 67 smd rect (at 7.9 -2) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J4-Pad5)"))
    (pad 68 smd rect (at 7.9 -2.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J4-Pad3)"))
    (pad 69 smd rect (at 7.9 -3) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad1)"))
    (pad 70 smd rect (at 7.9 -3.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J4-Pad8)"))
    (pad 71 smd rect (at 7.9 -4) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J4-Pad6)"))
    (pad 72 smd rect (at 7.9 -4.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 73 smd rect (at 7.9 -5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 74 smd rect (at 7.9 -5.5) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad4)"))
    (pad 75 smd rect (at 7.9 -6) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J4-Pad2)"))
    (pad 76 smd rect (at 6 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D4-Pad2)"))
    (pad 77 smd rect (at 5.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(D3-Pad1)"))
    (pad 78 smd rect (at 5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(S2-PadCTR)"))
    (pad 79 smd rect (at 4.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 80 smd rect (at 4 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 81 smd rect (at 3.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(S1-Pad1)"))
    (pad 82 smd rect (at 3 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad82)"))
    (pad 83 smd rect (at 2.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad83)"))
    (pad 84 smd rect (at 2 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-Pad84)"))
    (pad 85 smd rect (at 1.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J6-Pad3)"))
    (pad 86 smd rect (at 1 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J6-Pad4)"))
    (pad 87 smd rect (at 0.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J6-Pad4)"))
    (pad 88 smd rect (at 0 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J6-Pad3)"))
    (pad 89 smd rect (at -0.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad89)"))
    (pad 90 smd rect (at -1 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J7-Pad2)"))
    (pad 91 smd rect (at -1.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J7-Pad4)"))
    (pad 92 smd rect (at -2 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 93 smd rect (at -2.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 94 smd rect (at -3 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J7-Pad3)"))
    (pad 95 smd rect (at -3.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J7-Pad6)"))
    (pad 96 smd rect (at -4 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(S2-PadC)"))
    (pad 97 smd rect (at -4.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(S2-PadB)"))
    (pad 98 smd rect (at -5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(S2-PadD)"))
    (pad 99 smd rect (at -5.5 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(S2-PadA)"))
    (pad 100 smd rect (at -6 -7.9 90) (size 1.5 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-100_14x14mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 128.905 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 130.175 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 131.445 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D5 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 132.715 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D6 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D6-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 133.985 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D7 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D7-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 135.255 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D8 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 136.525 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D9 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(D9-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137.795 87.00739 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D10 (at -2.52761 0 90) (layer B.SilkS))
    (fp_text value LED_Small_ALT (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 128.905 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.175 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(D2-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.445 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 132.715 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D6-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 133.985 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 135.255 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(D8-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 136.525 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 137.795 84.46739 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 3.3K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(D10-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.35 70.485 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 3.3K (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.445 70.485)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 1.27) (layer F.SilkS))
    (fp_text value 3.3K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J6-Pad4)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.73 74.295 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.73 90.805 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.17 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 140.97 90.805)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.27) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 140.97 74.295)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.032 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.495 82.55 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switches:JOYSTICK_MINI (layer B.Cu) (tedit 596297CE)
    (at 133.35 78.105 225)
    (descr "SMALL TACTILE JOYSTICK W/ SELECT SWITCH")
    (tags "SMALL TACTILE JOYSTICK W/ SELECT SWITCH")
    (attr smd)
    (fp_text reference S2 (at -3.683 3.429 180) (layer B.SilkS))
    (fp_text value JOYSTICK_MINI (at 3.683 -3.683 180) (layer B.SilkS) hide)
    (fp_text user UP (at -1.778 2.921 45) (layer B.SilkS))
    (fp_text user UP (at -2.54 2.54 180) (layer Dwgs.User))
    (pad A smd rect (at -3.32486 1.39954 225) (size 1.84912 1.09982) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(S2-PadA)") (solder_mask_margin 0.1016))
    (pad B smd rect (at 3.32486 1.39954 225) (size 1.84912 1.09982) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(S2-PadB)") (solder_mask_margin 0.1016))
    (pad C smd rect (at -3.32486 -1.39954 225) (size 1.84912 1.09982) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(S2-PadC)") (solder_mask_margin 0.1016))
    (pad CTR smd rect (at -3.32486 0 225) (size 1.84912 1.09982) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(S2-PadCTR)") (solder_mask_margin 0.1016))
    (pad D smd rect (at 3.32486 -1.39954 225) (size 1.84912 1.09982) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(S2-PadD)") (solder_mask_margin 0.1016))
    (pad GND smd rect (at 3.32486 0 225) (size 1.84912 1.09982) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad NC smd rect (at 0 4.1275 225) (size 1.89992 1.99898) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
    (pad NC@0 smd rect (at 0 -4.1275 225) (size 1.89992 1.99898) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
    (pad "" np_thru_hole circle (at 0 1.89992 225) (size 0.7493 0.7493) (drill 0.7493) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad "" np_thru_hole circle (at 0 -1.89992 225) (size 1.04902 1.04902) (drill 1.04902) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.255 70.485)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 1.27) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.43 71.755 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at 1.905 -0.127 90) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 90 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 140.97 71.755 90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D4 (at 0.127 2.921 90) (layer F.SilkS) hide)
    (fp_text value LED_Small_ALT (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 137.16 71.755 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.413 -0.127 90) (layer F.SilkS) hide)
    (fp_text value 3.3K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 89 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 139.7 71.755 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0.635 2.794 90) (layer F.SilkS) hide)
    (fp_text value 3.3K (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 91 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PROGRAM (at 140.335 64.135) (layer F.SilkS))
  (gr_text "\nDONE" (at 141.605 71.755 90) (layer F.SilkS))
  (gr_text INIT (at 137.795 69.342 90) (layer F.SilkS))
  (gr_text "Developer\nEnabling\nInnovations\nby Steiert Solutions" (at 137.795 65.405 90) (layer B.SilkS))
  (gr_text "XO2 QWIIC PMOD" (at 123.19 82.55 90) (layer B.SilkS))
  (gr_line (start 152.4 101.6) (end 114.3 101.6) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 152.4 63.5) (end 152.4 101.6) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 114.3 63.5) (end 152.4 63.5) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 114.3 101.6) (end 114.3 63.5) (layer Edge.Cuts) (width 0.254))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.205 66.675) (xy 150.495 66.675) (xy 150.495 99.695) (xy 116.205 99.695) (xy 116.205 83.185)
      )
    )
  )
  (zone (net 1) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 73.66) (xy 142.24 73.66) (xy 142.24 91.44) (xy 124.46 91.44)
      )
    )
  )
)
