(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "SiPMMountV2/")
		)
	)
	(net 0 "")
	(net 1 "/K")
	(net 2 "/A")
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.85 94.15 180)
		(descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.77 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 0 5.31 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "SiPMMountV2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.975 6.275 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/A")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/K")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:SiPMPad_12mm12mm_WirebondPad_10mm0p5mm-NoSolderMask"
		(layer "F.Cu")
		(at 120 95.875)
		(property "Reference" "D1"
			(at 0 -12 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at -11.5 -3.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "SiPMMountV2.kicad_sch")
		(attr smd)
		(fp_text user "Wirebond Pad"
			(at 0 8.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 -3)
			(size 12 12)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.15)
			(net 1 "/K")
			(pinfunction "K")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 0 4)
			(size 10 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 2 "/A")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 103 102)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H2"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "SiPMMountV2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 120 83.6)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H3"
			(at -4.94 0.13 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 10 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "SiPMMountV2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 110.75 96.5)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H4"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -2.75 -6.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "SiPMMountV2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 129.25 96.5)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H5"
			(at 0.15 -4.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 2.75 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "SiPMMountV2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 103 82.95)
		(descr "Mounting Hole 3mm, no annular")
		(tags "mounting hole 3mm no annular")
		(property "Reference" "H1"
			(at 5.1 0.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "SiPMMountV2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 100 80)
		(end 140 105)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "SiPM carrier board v2\nA.G. & B.L."
		(at 124.7 103.75 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
