(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 300)
    (zones 0)
    (modules 20)
    (nets 25)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.2)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.1016)
    (pad_size 1 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFBFFF)
    (pcbplotparams
      (layerselection 0x010a8_7fffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory "output"))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 DIO0)
  (net 4 UPDI)
  (net 5 RESET)
  (net 6 DIO5)
  (net 7 DIO4)
  (net 8 DIO3)
  (net 9 DIO2)
  (net 10 DIO1)
  (net 11 BME_CS)
  (net 12 "Net-(ANT1-Pad1)")
  (net 13 MOSI_R)
  (net 14 SCK_R)
  (net 15 MISO_R)
  (net 16 CLK32K)
  (net 17 SCK)
  (net 18 MISO)
  (net 19 MOSI)
  (net 20 LORA_CS)
  (net 21 BAT_IN)
  (net 22 BAT_EN)
  (net 23 "Net-(Q1-Pad3)")
  (net 24 V_BAT)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net BAT_EN)
    (add_net BAT_IN)
    (add_net BME_CS)
    (add_net CLK32K)
    (add_net DIO0)
    (add_net DIO1)
    (add_net DIO2)
    (add_net DIO3)
    (add_net DIO4)
    (add_net DIO5)
    (add_net GND)
    (add_net LORA_CS)
    (add_net MISO)
    (add_net MISO_R)
    (add_net MOSI)
    (add_net MOSI_R)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net RESET)
    (add_net SCK)
    (add_net SCK_R)
    (add_net UPDI)
    (add_net VDD)
    (add_net V_BAT)
  )
  (module lora_node:DSC6083MI2A (layer F.Cu) (tedit 5D4A4AE6)
    (at 116.205 90.932 90)
    (attr smd)
    (fp_text reference U5 (at 0.762 1.7145 90) (layer F.SilkS))
    (fp_text value DSC6083 (at 0 2.794 90) (layer F.Fab))
    (pad 4 smd rect (at -0.775 -0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 0.775 -0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.775 0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.775 0.475 90) (size 0.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 CLK32K))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 134.366 88.011)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.413 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.682 107.442 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.143 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 V_BAT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.73 104.267)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.143 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.787501 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.787501 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal (layer B.Cu) (tedit 5B7745C6)
    (at 119.507 102.616 180)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J2 (at 1 1.397 180) (layer B.SilkS))
    (fp_text value "S2B-PH-K-S(LF)(SN)" (at 1 -7.45 180) (layer B.Fab))
    (fp_text user %R (at 1 -2.5 180) (layer B.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 V_BAT))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 125.984 106.553)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U4 (at 1.397 1.3335 90) (layer F.SilkS))
    (fp_text value MCP1812A (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 V_BAT))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 113.538 100.076 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.397 -1.143 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GSD (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 BAT_EN))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 V_BAT))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.919 96.139 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value 26.7k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 BAT_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.919 97.409)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.032 0) (layer F.SilkS))
    (fp_text value 11.3k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(Q1-Pad3)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 BAT_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lora_node:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5CF5BD77)
    (at 119.888 97.028 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value ATtiny814 (at 0 5.375 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 SCK))
    (pad 12 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 MISO))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 MOSI))
    (pad 10 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 UPDI))
    (pad 9 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 BAT_IN))
    (pad 8 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 BME_CS))
    (pad 7 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 BAT_EN))
    (pad 6 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 CLK32K))
    (pad 5 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 DIO5))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 DIO0))
    (pad 3 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 RESET))
    (pad 2 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 LORA_CS))
    (pad 1 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lora_node:0915AT43A0026 (layer F.Cu) (tedit 5CF5BB60)
    (at 150.125 93.625)
    (attr smd)
    (fp_text reference ANT1 (at 0 -2) (layer F.SilkS))
    (fp_text value 0915AT43A0026 (at 0 7.25) (layer F.Fab))
    (pad "" smd rect (at -2.85 4.5) (size 0.5 2) (layers F.Cu F.Mask))
    (pad "" smd rect (at 0.45 5.75 90) (size 0.5 7.1) (layers F.Cu F.Mask))
    (pad "" smd rect (at 3.75 3.2) (size 0.5 4.6) (layers F.Cu F.Mask))
    (pad 2 smd rect (at 3.5 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -3.5 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(ANT1-Pad1)"))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.238 96.774 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -1.016 -3.302 270) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 MISO_R))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 MISO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.238 94.996 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -5.08 270) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 MOSI))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 MOSI_R))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.238 98.552 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 1.016 -1.524 270) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 SCK_R))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 SCK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.6175 107.315 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0.0635 -1.143 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.698 91.465501 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.025501 1.397 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.787501 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.787501 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x12_P2.54mm_Vertical (layer F.Cu) (tedit 5C81E5A4)
    (at 112.776 83.312 90)
    (descr "Through hole straight socket strip, 2x12, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x12 2.54mm double row")
    (fp_text reference J1 (at -1.151 6.393 180) (layer F.SilkS) hide)
    (fp_text value Conn_02x12_Odd_Even (at -1.27 30.71 90) (layer F.Fab))
    (fp_text user %R (at -1.27 13.97 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 UPDI))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 RESET))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 BME_CS))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 V_BAT))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 DIO2))
    (pad 14 thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 DIO1))
    (pad 16 thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 MISO_R))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 DIO0))
    (pad 18 thru_hole oval (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 MOSI_R))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 DIO4))
    (pad 20 thru_hole oval (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 SCK_R))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 DIO3))
    (pad 22 thru_hole oval (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 LORA_CS))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 24 thru_hole oval (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 DIO5))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lora_node:BME280 (layer F.Cu) (tedit 5B2F0E9C)
    (at 114.15 104.938 90)
    (fp_text reference U3 (at 0 -2.136 90) (layer F.SilkS))
    (fp_text value BME280 (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at 1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 BME_CS))
    (pad 3 smd rect (at 1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 13 MOSI_R))
    (pad 4 smd rect (at 1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 14 SCK_R))
    (pad 5 smd rect (at -1.025 0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 15 MISO_R))
    (pad 6 smd rect (at -1.025 0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 7 smd rect (at -1.025 -0.325 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -1.025 -0.975 90) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
  )
  (module lora_node:RFM95W locked (layer F.Cu) (tedit 58C0EDBF)
    (at 136.15 98.35)
    (fp_text reference U2 (at -8.896 -8.942 180) (layer F.SilkS))
    (fp_text value RFM95W-915S2 (at 0 0) (layer F.Fab))
    (pad 16 smd rect (at -7 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 9 DIO2))
    (pad 1 smd rect (at -7 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at -5 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 10 DIO1))
    (pad 2 smd rect (at -5 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 15 MISO_R))
    (pad 14 smd rect (at -3 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 3 DIO0))
    (pad 3 smd rect (at -3 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 13 MOSI_R))
    (pad 13 smd rect (at -1 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 4 smd rect (at -1 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 14 SCK_R))
    (pad 12 smd rect (at 1 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 7 DIO4))
    (pad 5 smd rect (at 1 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 20 LORA_CS))
    (pad 11 smd rect (at 3 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 8 DIO3))
    (pad 6 smd rect (at 3 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 5 RESET))
    (pad 10 smd rect (at 5 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 5 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 DIO5))
    (pad 9 smd rect (at 7 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(ANT1-Pad1)"))
    (pad 8 smd rect (at 7 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.3 90.932 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.143 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.787501 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
    (pad 2 smd roundrect (at 0.787501 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "LoRaAtmo v0.46" (at 144.018 107.188) (layer B.SilkS))
  (gr_line (start 155.5 109) (end 111 109) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 155.5 81.5) (end 111 81.5) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 111 109) (end 111 81.5) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 155.5 81.5) (end 155.5 109) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.255) (thermal_bridge_width 0.255) (smoothing fillet))
    (polygon
      (pts
        (xy 121.372 81.534) (xy 144.907 81.534) (xy 144.907 108.966) (xy 111.028 108.966) (xy 111.028 81.534)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.673 103.1875) (xy 115.673 103.1875) (xy 115.673 106.934) (xy 112.673 106.934)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.255) (thermal_bridge_width 0.255) (smoothing fillet))
    (polygon
      (pts
        (xy 144.907 81.534) (xy 144.907 108.966) (xy 140.716 108.966) (xy 140.716 81.534)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.524 88.646) (xy 139.954 88.646) (xy 139.954 108.966) (xy 128.524 108.966)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.189 92.1385) (xy 115.189 89.7255) (xy 117.221 89.7255) (xy 117.221 92.1385)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.063 95.631) (xy 123.063 92.837) (xy 124.46 92.837) (xy 124.46 95.631)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer F.Cu) (hatch none 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.255) (thermal_bridge_width 0.255) (smoothing fillet))
    (polygon
      (pts
        (xy 139.957 81.534) (xy 139.954 108.966) (xy 110.998 108.966) (xy 110.998 81.534)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.524 100.584) (xy 126.746 100.584) (xy 123.825 103.632) (xy 123.825 108.712) (xy 128.524 108.712)
        (xy 128.524 104.648)
      )
    )
  )
)
