(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 2)
    (tracks 23)
    (zones 0)
    (modules 1)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 134.49 85.34)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Crazy_Circuits:Adafruit-Trinket-M0 (layer F.Cu) (tedit 5C573FED)
    (at 110.49 53.34)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference M0 (at 13 25 90) (layer F.SilkS) hide)
    (fp_text value "Adafruit Trinket" (at 11 25 90) (layer F.Fab) hide)
    (fp_text user Bat (at 19.447 40.3005) (layer F.SilkS))
    (fp_text user 4 (at 20.336 24.0445) (layer F.SilkS))
    (fp_text user Gnd (at 18.92 32) (layer F.SilkS))
    (fp_text user 3 (at 20.209 16.0435) (layer F.SilkS))
    (fp_text user Rst (at 19.574 7.9155) (layer F.SilkS))
    (fp_text user USB (at 4.842 40.3005) (layer F.SilkS))
    (fp_arc (start 24 40) (end 27.9 40) (angle 90) (layer Edge.Cuts) (width 0.04064))
    (fp_arc (start 24 8) (end 24 4.1) (angle 89.89999678) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start 27.9 40) (end 27.899994 7.993193) (layer Edge.Cuts) (width 0.04064))
    (fp_arc (start 0 8) (end -3.9 8) (angle 90) (layer Edge.Cuts) (width 0.04064))
    (fp_arc (start 0.001 40) (end 0.001 43.9) (angle 89.89999678) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start -3.9 8) (end -3.898994 40.006807) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start 24 4.1) (end 0 4.1) (layer Edge.Cuts) (width 0.04064))
    (fp_line (start 0.001 43.9) (end 24 43.9) (layer Edge.Cuts) (width 0.04064))
    (fp_text user 1 (at 3.572 23.94) (layer F.SilkS))
    (fp_text user 0 (at 3.572 32.19) (layer F.SilkS))
    (fp_text user 3V (at 4 7.94) (layer F.SilkS))
    (fp_text user 2 (at 3.572 16.1705) (layer F.SilkS))
    (fp_text user USB (at 11.748 38.735) (layer F.SilkS))
    (pad Bat thru_hole circle (at 24 40 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad Gnd thru_hole circle (at 24 32 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 24 24 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 24 16 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad Rst thru_hole circle (at 24 8 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0.001 24 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad USB thru_hole circle (at 0.001 40 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 0 thru_hole circle (at 0.001 32 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0.001 16 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 3V thru_hole circle (at 0 8 90) (size 6 6) (drill 4.98) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5.477 21.2505 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad USB thru_hole circle (at 5.477 28.8705 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3V thru_hole circle (at 5.477 18.7105 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 5.477 26.3305 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 5.477 23.7905 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad Rst thru_hole circle (at 18.177 18.7105 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 18.177 21.2505 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 18.177 23.7905 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad Gnd thru_hole circle (at 18.177 26.3305 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad Bat thru_hole circle (at 18.177 28.8705 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "Adafruit Trinket M0" (at 121.79 77.72 90) (layer F.SilkS))
)
