(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 30)
    (no_connects 0)
    (area 140.894999 98.730999 160.603001 120.471001)
    (thickness 1.6)
    (drawings 21)
    (tracks 278)
    (zones 0)
    (modules 16)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /INP)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 /OUT)
  (net 9 /ENA)
  (net 10 "Net-(Q1-Pad3)")
  (net 11 "Net-(R2-Pad2)")
  (net 12 "Net-(R4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ENA)
    (add_net /INP)
    (add_net /OUT)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R4-Pad2)")
  )
  (module Choke_SMD:Choke_SMD_12x12mm_h8mm (layer F.Cu) (tedit 58A0B0CF)
    (at 148.59 105.41)
    (descr "Choke, SMD, 12x12mm 8mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L1 (at 0 -8.89) (layer F.SilkS) hide)
    (fp_text value 22u (at 0 8.89) (layer F.Fab) hide)
    (pad 1 smd rect (at -5.05046 0) (size 3.10068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 1 /INP))
    (pad 2 smd rect (at 5.05046 0) (size 3.10068 5.40004) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Choke_SMD.3dshapes/Choke_SMD_12x12mm_h8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58A0B11B)
    (at 149.352 104.648 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1 180) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /INP))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58A0B100)
    (at 148.082 110.236 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 10n (at 0 -1.9 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58A0B107)
    (at 145.288 110.17 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 2n2 (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58A0B0ED)
    (at 156.21 109.982 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 2.1 90) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58A0B09C)
    (at 157.48 107.696 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 -2.85 90) (layer F.SilkS) hide)
    (fp_text value 3A (at 0.05 4.4 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/D_SMA_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_4pol (layer F.Cu) (tedit 58A0B0B3)
    (at 144.13 115.57)
    (descr "4-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference P1 (at 5.25 -4.3) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 5.25 6) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /INP))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /OUT))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /ENA))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_4pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58A0B0D8)
    (at 158.308 115.57 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.5 90) (layer B.SilkS) hide)
    (fp_text value IRLML2502 (at 0 -2.5 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 /ENA))
    (pad 2 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(Q1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58A0B0DA)
    (at 158.242 115.57 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5 270) (layer F.SilkS) hide)
    (fp_text value AO3407 (at 0 2.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /OUT))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58A0B0BA)
    (at 145.796 117.856 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 100k (at 0 -1.9 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /ENA))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58A0B0F3)
    (at 153.924 108.882 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 100k (at 0 -1.9 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /INP))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58A0B10C)
    (at 143.764 110.49 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.9 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58A0B0F0)
    (at 152.23 111.76 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 100k (at 0 -1.9 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58A0B0FA)
    (at 148.166 111.76 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.9 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58A0B0E2)
    (at 158.242 110.49 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.9 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer B.Cu) (tedit 58A0B117)
    (at 149.52 107.625)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 2.6) (layer B.SilkS) hide)
    (fp_text value MP1542 (at 0 -2.6) (layer B.Fab) hide)
    (pad 1 smd rect (at -2.2 0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at -2.2 0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R4-Pad2)"))
    (pad 3 smd rect (at -2.2 -0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 /ENA))
    (pad 4 smd rect (at -2.2 -0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.2 -0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 6 smd rect (at 2.2 -0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 /INP))
    (pad 7 smd rect (at 2.2 0.325) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R2-Pad2)"))
    (pad 8 smd rect (at 2.2 0.975) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text OUT (at 154.559 117.729) (layer F.SilkS))
  (gr_text INP (at 151.13 117.729) (layer F.SilkS))
  (gr_text ENA (at 147.701 117.729) (layer F.SilkS))
  (gr_text GND (at 144.145 117.729) (layer F.SilkS))
  (gr_text 170212 (at 149.225 113.284) (layer F.SilkS))
  (gr_text "Boost 13.75V 1.5A" (at 151.003 101.092) (layer B.SilkS))
  (gr_text OUT (at 154.559 113.411) (layer B.SilkS))
  (gr_text INP (at 151.003 113.411) (layer B.SilkS))
  (gr_text ENA (at 147.701 113.411) (layer B.SilkS))
  (gr_text GND (at 144.145 113.411) (layer B.SilkS))
  (gr_line (start 140.97 119.38) (end 141.986 120.396) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 99.822) (end 141.986 98.806) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.512 98.806) (end 160.528 99.822) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.512 120.396) (end 160.528 119.38) (layer Edge.Cuts) (width 0.15))
  (dimension 19.558 (width 0.3) (layer Dwgs.User)
    (gr_text "19.558 mm" (at 150.749 93.646) (layer Dwgs.User))
    (feature1 (pts (xy 160.528 98.298) (xy 160.528 92.296)))
    (feature2 (pts (xy 140.97 98.298) (xy 140.97 92.296)))
    (crossbar (pts (xy 140.97 94.996) (xy 160.528 94.996)))
    (arrow1a (pts (xy 160.528 94.996) (xy 159.401496 95.582421)))
    (arrow1b (pts (xy 160.528 94.996) (xy 159.401496 94.409579)))
    (arrow2a (pts (xy 140.97 94.996) (xy 142.096504 95.582421)))
    (arrow2b (pts (xy 140.97 94.996) (xy 142.096504 94.409579)))
  )
  (dimension 21.59 (width 0.3) (layer Dwgs.User)
    (gr_text "21.590 mm" (at 166.196 109.601 90) (layer Dwgs.User))
    (feature1 (pts (xy 161.036 98.806) (xy 167.546 98.806)))
    (feature2 (pts (xy 161.036 120.396) (xy 167.546 120.396)))
    (crossbar (pts (xy 164.846 120.396) (xy 164.846 98.806)))
    (arrow1a (pts (xy 164.846 98.806) (xy 165.432421 99.932504)))
    (arrow1b (pts (xy 164.846 98.806) (xy 164.259579 99.932504)))
    (arrow2a (pts (xy 164.846 120.396) (xy 165.432421 119.269496)))
    (arrow2b (pts (xy 164.846 120.396) (xy 164.259579 119.269496)))
  )
  (gr_line (start 141.986 120.396) (end 142.24 120.396) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 99.822) (end 140.97 119.38) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.512 98.806) (end 141.986 98.806) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.528 119.38) (end 160.528 99.822) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 120.396) (end 159.512 120.396) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.986 120.396) (xy 159.512 120.396) (xy 160.528 119.38) (xy 160.528 99.822) (xy 159.512 98.806)
        (xy 141.986 98.806) (xy 140.97 99.822) (xy 140.97 119.38)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.986 120.396) (xy 159.512 120.396) (xy 160.528 119.38) (xy 160.528 99.822) (xy 159.512 98.806)
        (xy 141.986 98.806) (xy 140.97 99.822) (xy 140.97 119.38)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.923 106.68) (xy 142.494 106.68) (xy 142.494 104.394) (xy 145.923 104.394)
      )
    )
  )
)
