(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 29)
    (no_connects 1)
    (area 141.465299 59.347099 163.334701 77.812901)
    (thickness 1.6002)
    (drawings 15)
    (tracks 77)
    (zones 0)
    (modules 13)
    (nets 10)
  )
  (page A4)
  (title_block
    (title "ISL12022M RTC Breakout v1.0")
    (date 2017-02-01)
    (rev A)
    (company "Rene van der Meer / rene@golemparts.com / @GolemParts")
    (comment 2 https://creativecommons.org/licenses/by-sa/4.0/.)
    (comment 3 "License. To view a copy of this license, visit")
    (comment 4 "This work is licensed under the Creative Commons Attribution-ShareAlike 4.0 International")
  )
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.508 1.27)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0762)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BT1-Pad1)")
  (net 3 VDD)
  (net 4 "Net-(R1-Pad1)")
  (net 5 /IRQ)
  (net 6 /SDA)
  (net 7 /SCL)
  (net 8 /VBAT)
  (net 9 "Net-(R2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /IRQ)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /VBAT)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net VDD)
  )
  (module Golemparts:VIA-0.6mm (layer Top) (tedit 586C277E)
    (at 143.256 76.708 180)
    (fp_text reference REF** (at 0 1.27 180) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Golemparts:VIA-0.6mm (layer Top) (tedit 586C277E)
    (at 161.544 76.708 180)
    (fp_text reference REF** (at 0 1.27 180) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Bottom) (tedit 588E89EC)
    (at 145.876 73.5838 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.4732 180) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Bottom B.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Bottom B.Mask)
      (net 6 /SDA))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 588E89AA)
    (at 144.526 70.4523 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.7505 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Mask)
      (net 8 /VBAT))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 588E89C0)
    (at 160.274 70.4523 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.7505 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer Top) (tedit 588E89C8)
    (at 144.526 64.135 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 2.77495 0 180) (layer F.SilkS))
    (fp_text value BAT43 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers Top F.Mask)
      (net 8 /VBAT))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers Top F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Bottom) (tedit 588E89F4)
    (at 152.4 73.5838)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.4732) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Bottom B.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Bottom B.Mask)
      (net 7 /SCL))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Bottom) (tedit 588E89DF)
    (at 158.924 73.5838 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.4732 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Bottom B.Mask)
      (net 3 VDD))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Bottom B.Mask)
      (net 5 /IRQ))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer Top) (tedit 588E89B1)
    (at 152.4 67.31)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -7.5) (layer F.SilkS) hide)
    (fp_text value ISL12022M (at 0 7.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers Top F.Mask))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers Top F.Mask))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers Top F.Mask))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers Top F.Mask))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers Top F.Mask))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers Top F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers Top F.Mask)
      (net 8 /VBAT))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers Top F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers Top F.Mask))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers Top F.Mask))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers Top F.Mask)
      (net 6 /SDA))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers Top F.Mask)
      (net 7 /SCL))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers Top F.Mask)
      (net 5 /IRQ))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers Top F.Mask)
      (net 3 VDD))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers Top F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers Top F.Mask))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers Top F.Mask))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers Top F.Mask))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers Top F.Mask))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers Top F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Golemparts:Pin_Header_Straight_1x05_Pitch2.54mm (layer Top) (tedit 588E89A5)
    (at 157.48 76.454 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 270) (layer F.SilkS) hide)
    (fp_text value "Breakout header" (at 0 12.55 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VDD))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /IRQ))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SDA))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SCL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Golemparts:VIA-0.6mm (layer Top) (tedit 586C277E)
    (at 152.4 69.596 180)
    (fp_text reference REF** (at 0 1.27 180) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.27 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 0.6858 0.6858) (drill 0.3302) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Golemparts:3000 (layer Bottom) (tedit 588E89D8)
    (at 152.4 65.5574 180)
    (descr "Keystone 3000 CR1225")
    (tags "Keystone Battery Holder 3000 CR1225 BR1225 CR1220 CR1216")
    (fp_text reference BT1 (at 0 -7.62 180) (layer B.SilkS) hide)
    (fp_text value CR1225 (at 0 6.09 180) (layer B.Fab) hide)
    (fp_text user CR1225 (at 0 4.66 180) (layer B.SilkS))
    (pad 2 smd rect (at 0 0 180) (size 3.96 3.96) (layers Bottom B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -7.87 0 180) (size 3.18 3.18) (layers Bottom B.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at 7.87 0 180) (size 3.18 3.18) (layers Bottom B.Mask)
      (net 2 "Net-(BT1-Pad1)"))
  )
  (module Golemparts:Solder_Jumper_Dual_NO_SMD (layer Bottom) (tedit 58922A93)
    (at 160.274 69.85 270)
    (descr "Solder bridge jumper oval NO")
    (tags "solder bridge jumper oval NO normally open")
    (attr smd)
    (fp_text reference SJ1 (at 0 1.905 270) (layer B.SilkS) hide)
    (fp_text value Solder_Jumper_NO_Dual (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -0.6 0 270) (size 0.4064 1.27) (layers Bottom B.Mask)
      (net 4 "Net-(R1-Pad1)") (solder_mask_margin 0.0254))
    (pad 3 smd rect (at 0.6 0 270) (size 0.4064 1.27) (layers Bottom B.Mask)
      (net 9 "Net-(R2-Pad1)") (solder_mask_margin 0.0254))
    (pad 3 smd oval (at 0.8 0 270) (size 0.508 1.27) (layers Bottom B.Mask)
      (net 9 "Net-(R2-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd oval (at -0.8 0 90) (size 0.508 1.27) (layers Bottom B.Mask)
      (net 4 "Net-(R1-Pad1)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.73 0 270) (size 0.3556 1.016) (layers Bottom B.Mask)
      (net 4 "Net-(R1-Pad1)") (solder_mask_margin 0.0254))
    (pad 3 smd rect (at 0.73 0 270) (size 0.3556 1.016) (layers Bottom B.Mask)
      (net 9 "Net-(R2-Pad1)") (solder_mask_margin 0.0254))
    (pad 2 smd rect (at 0 0 270) (size 0.4572 1.27) (layers Bottom B.Mask)
      (net 3 VDD) (solder_mask_margin 0.0254))
  )
  (gr_text "ISL12022M RTC Breakout v1.0 A\nRene van der Meer\nCC BY-SA 4.0\n@GolemParts" (at 160.8328 59.817 270) (layer F.SilkS))
  (gr_text Pull-ups (at 162.1282 69.85 270) (layer B.SilkS))
  (gr_text SDA (at 149.86 74.7268) (layer F.SilkS))
  (gr_text SCL (at 147.32 74.7268) (layer F.SilkS))
  (gr_text IRQ (at 152.4 74.7268) (layer F.SilkS))
  (gr_text VDD (at 154.94 74.7268) (layer F.SilkS))
  (gr_text GND (at 157.48 74.7268) (layer F.SilkS))
  (gr_arc (start 162.052 60.6298) (end 162.052 59.3598) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 142.748 60.6298) (end 141.478 60.6298) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 142.748 76.5302) (end 142.748 77.8002) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 162.052 76.5302) (end 163.322 76.5302) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 163.322 76.5302) (end 163.322 60.6298) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 142.748 77.8002) (end 162.052 77.8002) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 141.478 60.6298) (end 141.478 76.5302) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 162.052 59.3598) (end 142.748 59.3598) (layer Edge.Cuts) (width 0.0254))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.3728 77.9018) (xy 163.3728 59.3598) (xy 141.478 59.3598) (xy 141.4272 77.8764)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.3728 77.9018) (xy 163.3728 59.3598) (xy 141.478 59.3598) (xy 141.4272 77.8764)
      )
    )
  )
)
