(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 105)
    (zones 0)
    (modules 6)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 8.128 8.128)
    (pad_drill 1.524)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
  )
  (module touch:TestPoint_Pad_4.0x4.0mm (layer B.Cu) (tedit 5E4F1F96)
    (at 180.29682 95.63862)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J2 (at 0 2.898) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -3.1) (layer B.Fab) hide)
    (fp_text user %R (at 0 2.9) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 8.128 8.128) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module touch:TestPoint_Pad_4.0x4.0mm (layer B.Cu) (tedit 5E4F1ECC)
    (at 124.61494 95.65132)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J1 (at 0 2.898) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -3.1) (layer B.Fab) hide)
    (fp_text user %R (at 0 2.9) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at -0.24384 -0.06604) (size 8.128 8.128) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 +3V3))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5E4C6FEF)
    (at 165.97884 95.77832 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5E4C3259)
    (at 152.34412 96.57842 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.43 270) (layer F.SilkS) hide)
    (fp_text value LED (at 2.35588 3.76428 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_14.6x12mm_SilkScreen (layer B.Cu) (tedit 5E487EEC)
    (at 152.3111 96.34474 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbol:OSHW-Logo2_14.6x12mm_SilkScreen (layer F.Cu) (tedit 5E487BD2)
    (at 152.31364 96.33204)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (gr_text "Open Hardware Summit" (at 152.3873 99.78644) (layer F.Mask))
  (gr_text + (at 152.32126 98.35388) (layer F.Cu))
  (gr_text "github.com/\noshpark/\nflextester" (at 139.03706 95.52432) (layer B.SilkS))
  (gr_text "Flex\nbattery \ntester" (at 165.5318 95.74784) (layer B.SilkS))
  (gr_text "March 13, 2020" (at 166.02964 92.3036) (layer F.Cu))
  (gr_text "New York City" (at 138.61034 92.32646) (layer F.Cu))
  (gr_text "Open Hardware Summit" (at 152.38476 99.7839) (layer F.Mask))
  (gr_text "Open Hardware Summit" (at 152.3873 99.78644) (layer F.Cu))
  (gr_line (start 186.038754 91.545674) (end 186.015894 99.972866) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.824746 91.545674) (end 118.801886 99.972866) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 120.1166 99.972866) (end 120.1166 101.28758) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 184.70118 99.972866) (end 184.70118 101.28758) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 184.70118 101.28758) (end 120.9421 101.28758) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.9421 101.28758) (end 120.1166 101.28758) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183.89854 90.23096) (end 184.72404 90.23096) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 184.72404 91.545674) (end 184.72404 90.23096) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.13946 90.23096) (end 183.89854 90.23096) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 120.13946 91.545674) (end 120.13946 90.23096) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text + (at 130.46202 91.18346) (layer B.SilkS))
  (zone (net 3) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.189174 95.578996) (xy 153.129692 95.57688) (xy 153.072194 95.570616) (xy 153.016677 95.560203) (xy 152.963143 95.545642)
        (xy 152.911591 95.526932) (xy 152.862021 95.504073) (xy 152.814433 95.477065) (xy 152.768828 95.445909) (xy 152.725204 95.410605)
        (xy 152.683564 95.371152) (xy 152.106621 95.703259) (xy 152.683111 96.03615) (xy 152.724805 95.996753) (xy 152.768476 95.961508)
        (xy 152.814124 95.930414) (xy 152.861749 95.903471) (xy 152.91135 95.88068) (xy 152.962927 95.86204) (xy 153.016482 95.847552)
        (xy 153.072012 95.837215) (xy 153.12952 95.831029) (xy 153.189004 95.828995)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.684004 94.787411) (xy 166.651062 94.783523) (xy 166.617303 94.775681) (xy 166.582726 94.763882) (xy 166.54733 94.748128)
        (xy 166.511117 94.728419) (xy 166.474085 94.704753) (xy 166.436235 94.677132) (xy 166.397567 94.645556) (xy 166.358081 94.610023)
        (xy 166.317778 94.570536) (xy 165.741341 94.903519) (xy 166.318337 95.235534) (xy 166.358574 95.196172) (xy 166.398001 95.161154)
        (xy 166.436616 95.130481) (xy 166.474421 95.104152) (xy 166.511414 95.082168) (xy 166.547596 95.064527) (xy 166.582967 95.051231)
        (xy 166.617527 95.04228) (xy 166.651276 95.037672) (xy 166.684214 95.03741)
      )
    )
  )
  (zone (net 2) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.172708 95.585356) (xy 133.341693 95.534184) (xy 132.542017 95.431152) (xy 131.773679 95.276259) (xy 131.036681 95.069504)
        (xy 130.331021 94.810888) (xy 129.656699 94.500411) (xy 129.013716 94.138073) (xy 128.402072 93.723874) (xy 127.821766 93.257814)
        (xy 127.2728 92.739893) (xy 122.339101 95.585691) (xy 127.273952 98.429492) (xy 127.822709 97.913889) (xy 128.402827 97.455217)
        (xy 129.014306 97.053476) (xy 129.657146 96.708666) (xy 130.331346 96.420787) (xy 131.036907 96.189839) (xy 131.773829 96.015822)
        (xy 132.542111 95.898735) (xy 133.341754 95.838579) (xy 134.172758 95.835355)
      )
    )
  )
  (zone (net 2) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.498685 97.57523) (xy 151.558159 97.577529) (xy 151.615638 97.583971) (xy 151.671122 97.594555) (xy 151.724611 97.609282)
        (xy 151.776105 97.628152) (xy 151.825604 97.651164) (xy 151.873108 97.678318) (xy 151.918617 97.709615) (xy 151.962131 97.745055)
        (xy 152.00365 97.784637) (xy 152.581618 97.454316) (xy 152.00616 97.119643) (xy 151.964343 97.15891) (xy 151.920563 97.19402)
        (xy 151.874819 97.224973) (xy 151.827112 97.251768) (xy 151.777441 97.274405) (xy 151.725805 97.292885) (xy 151.672207 97.307208)
        (xy 151.616644 97.317373) (xy 151.559118 97.323381) (xy 151.499628 97.325232)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.133911 96.778596) (xy 165.193394 96.780651) (xy 165.250899 96.786857) (xy 165.306426 96.797214) (xy 165.359976 96.811722)
        (xy 165.411547 96.83038) (xy 165.46114 96.853189) (xy 165.508755 96.880148) (xy 165.554392 96.911258) (xy 165.598051 96.946519)
        (xy 165.639732 96.985931) (xy 166.216339 96.653243) (xy 165.639514 96.320932) (xy 165.597859 96.36037) (xy 165.554223 96.395659)
        (xy 165.508606 96.426799) (xy 165.461009 96.45379) (xy 165.411431 96.476631) (xy 165.359872 96.495323) (xy 165.306333 96.509865)
        (xy 165.250812 96.520258) (xy 165.193311 96.526502) (xy 165.13383 96.528597)
      )
    )
  )
  (zone (net 3) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.188969 95.577609) (xy 153.129484 95.575591) (xy 153.071975 95.569421) (xy 153.016441 95.559099) (xy 152.962883 95.544625)
        (xy 152.9113 95.526) (xy 152.861693 95.503223) (xy 152.814061 95.476293) (xy 152.768404 95.445212) (xy 152.724723 95.409979)
        (xy 152.683018 95.370595) (xy 152.106621 95.703648) (xy 152.683657 96.035594) (xy 152.725286 95.996128) (xy 152.7689 95.960811)
        (xy 152.814496 95.929642) (xy 152.862077 95.902622) (xy 152.91164 95.879749) (xy 152.963187 95.861024) (xy 153.016717 95.846448)
        (xy 153.072231 95.83602) (xy 153.129728 95.82974) (xy 153.189209 95.827608)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 100)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.521007 95.136654) (xy 171.496046 95.318592) (xy 172.346591 95.541962) (xy 173.02226 95.7961) (xy 173.699552 96.040243)
        (xy 174.405212 96.298859) (xy 175.079534 96.609336) (xy 175.722517 96.971674) (xy 176.334161 97.385873) (xy 176.914467 97.851933)
        (xy 177.463433 98.369854) (xy 182.397132 95.524056) (xy 177.462281 92.680255) (xy 176.913524 93.195858) (xy 176.333406 93.65453)
        (xy 175.721927 94.056271) (xy 175.079087 94.401081) (xy 174.404887 94.68896) (xy 173.699326 94.919908) (xy 172.962404 95.093925)
        (xy 172.194122 95.211012) (xy 171.382838 95.161037) (xy 170.590358 95.054357)
      )
    )
  )
)
