(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Purple") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (color "FR4 natural") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Purple") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.1)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 90 82.5)
    (grid_origin 90 82.5)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "PulseCoil2")
  (net 3 "Filtered+12v")
  (net 4 "PulseCoil1")
  (net 5 "T1-")
  (net 6 "+12V")
  (net 7 "T2-")
  (net 8 "Net-(D1-K)")
  (net 9 "Net-(D3-A)")
  (net 10 "Net-(D2-K)")
  (net 11 "Net-(D4-A)")
  (net 12 "Net-(D6-K)")
  (net 13 "Net-(D7-K)")
  (net 14 "Net-(Q3-C)")
  (net 15 "Net-(Q4-C)")
  (net 16 "/T1_Inverting")
  (net 17 "/T1_Non-Inverting")
  (net 18 "Net-(Q1-B)")
  (net 19 "Net-(Q2-B)")
  (net 20 "Net-(Q3-B)")
  (net 21 "Net-(Q4-B)")
  (net 22 "Q3{slash}4_Supply")
  (net 23 "/T2_Inverting")
  (net 24 "/T2_Non-Inverting")
  (net 25 "/T1_Out")
  (net 26 "/T2_Out")
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 159.38 121)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R21" (at -2.63 1.75) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "/T1_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 123.13 121)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.87 1.75) (layer "F.SilkS"))
    (fp_text value "82k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 127.25 127.75)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "MFG#" "UBW1H100MPD")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "50v")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 5.25 -4.25) (layer "F.SilkS"))
    (fp_text value "10u" (at 1.75 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 159.38 127.75)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R18" (at -2.63 0) (layer "F.SilkS"))
    (fp_text value "13k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D6-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 16 "/T1_Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 137.79 132.75 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "MFG#" "KSC945CYTA")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "NPN transistor, emitter/collector/base")
    (property "ki_keywords" "transistor NPN")
    (attr through_hole)
    (fp_text reference "Q3" (at -0.96 -2.5) (layer "F.SilkS"))
    (fp_text value "KSC945" (at 2.54 2.79) (layer "F.Fab"))
    (fp_text user "C" (at 5.04 -2.75 180) (layer "B.SilkS"))
    (fp_text user "E" (at 0 -2.75 180) (layer "B.SilkS"))
    (fp_text user "B" (at 2.54 -2.75 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(Q3-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q3-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 159.38 92.75)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R25" (at -2.63 0) (layer "F.SilkS"))
    (fp_text value "13k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 23 "/T2_Inverting") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D7-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 167 124.25 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R17" (at 10.25 -0.5) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 16 "/T1_Inverting") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 127.25 92.25)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "MFG#" "UBW1H100MPD")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "50v")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 5.25 4.25) (layer "F.SilkS"))
    (fp_text value "10u" (at 1.75 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D4-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (at 135.25 118.25 -90)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D6" (at 0 2 -270) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 5.08 2.47 -270) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 -270) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 5.47 0 -270) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D6-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (thermal_bridge_angle 45))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (at 135.25 91.59 -90)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D7" (at 0 -2.25 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 5.08 2.47 -270) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 -270) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 5.47 0 -270) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 -270) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D7-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (thermal_bridge_angle 45))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-2_Horizontal_TabDown" (layer "F.Cu")
    (at 122 130.5 90)
    (descr "TO-220-2, Horizontal, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF")
    (tags "TO-220-2 Horizontal RM 5.08mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "NPN transistor, base/collector/emitter, collector connected to mounting plane")
    (property "ki_keywords" "transistor NPN")
    (attr through_hole)
    (fp_text reference "Q1" (at 2.5 -1.75 90) (layer "F.SilkS"))
    (fp_text value "BDX53BG" (at 2.54 -4 90) (layer "F.SilkS"))
    (fp_text user "B" (at 0 -2.25 unlocked) (layer "B.SilkS"))
    (fp_text user "C" (at 2.7 -10.75 unlocked) (layer "B.SilkS"))
    (fp_text user "E" (at 5 -2.25 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 -19.5 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(Q1-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive") (thermal_bridge_width 1.2) (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.67 -15.25 90) (size 6 6) (drill 3.6) (layers "*.Cu" "*.Mask")
      (net 5 "T1-") (pinfunction "C") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.SilkS") (name "Heatsink") (hatch edge 0.5)
      (connect_pads (clearance 0))
      (min_thickness 0.25) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints not_allowed))
      (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
      (polygon
        (pts
          (xy 103.4 119.8)
          (xy 103.4 122.6)
          (xy 119.5 122.6)
          (xy 119.5 119.8)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.SilkS") (name "Heatsink") (hatch edge 0.5)
      (connect_pads (clearance 0))
      (min_thickness 0.25) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints not_allowed))
      (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
      (polygon
        (pts
          (xy 103.4 133.1)
          (xy 103.4 135.8)
          (xy 119.5 135.8)
          (xy 119.5 133.1)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-2_Horizontal_TabDown.wrl"
      (offset (xyz 0 -1.08 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:L_Axial_L11.0mm_D4mm_P15.24mm_Horizontal_Fastron_MECC_with_symbol" (layer "F.Cu")
    (at 142.5 133.75)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4mm Fastron MECC")
    (property "MFG#" "77F560J-TR-RC")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L2" (at 12.5 -3) (layer "F.SilkS"))
    (fp_text value "56u" (at 7.5 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q3-C)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "Q3{slash}4_Supply") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 117.5 106.88 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at -1.88 0 -180) (layer "F.SilkS"))
    (fp_text value "3k" (at 3.8 0 -270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 -270) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "PulseCoil1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 96.75)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R19" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "15k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 24 "/T2_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 126.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R22" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "75k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 25 "/T1_Out") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "/T1_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (at 106.25 102.5)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D2" (at -2.25 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "PulseCoil2") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 123.75)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R23" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "15k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "/T1_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 162 117.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "MFG#" "R82EC2100AA50J")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at -2.5 1) (layer "F.SilkS"))
    (fp_text value "10n" (at 2.5 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/T1_Inverting") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/T1_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (at 137.79 87.25 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "MFG#" "KSC945CYTA")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "NPN transistor, emitter/collector/base")
    (property "ki_keywords" "transistor NPN")
    (attr through_hole)
    (fp_text reference "Q4" (at -0.71 2.5) (layer "F.SilkS"))
    (fp_text value "KSC945" (at 2.54 2.79) (layer "F.Fab"))
    (fp_text user "E" (at 0.04 1.75 180) (layer "B.SilkS"))
    (fp_text user "C" (at 5.04 1.75 180) (layer "B.SilkS"))
    (fp_text user "B" (at 2.54 1.75 180) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(Q4-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(Q4-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 106.25 112.75)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "MFG#" "R82EC2150AA50J")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at -2.5 0) (layer "F.SilkS"))
    (fp_text value "15n" (at 2.5 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "PulseCoil1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-2_Horizontal_TabDown" (layer "F.Cu")
    (at 122.05 95 90)
    (descr "TO-220-2, Horizontal, RM 5.08mm, see https://www.centralsemi.com/PDFS/CASE/TO-220-2PD.PDF")
    (tags "TO-220-2 Horizontal RM 5.08mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "NPN transistor, base/collector/emitter, collector connected to mounting plane")
    (property "ki_keywords" "transistor NPN")
    (attr through_hole)
    (fp_text reference "Q2" (at 2.5 -1.8 90) (layer "F.SilkS"))
    (fp_text value "BDX53BG" (at 2.54 -4 90) (layer "F.SilkS"))
    (fp_text user "C" (at 2.7 -10.75 unlocked) (layer "B.SilkS"))
    (fp_text user "E" (at 5 -2.25 unlocked) (layer "B.SilkS"))
    (fp_text user "B" (at 0 -2.25 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.54 -19.5 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Q2-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "E") (pintype "passive") (thermal_bridge_width 1.2) (thermal_bridge_angle 45))
    (pad "4" thru_hole circle (at 2.67 -15.25 90) (size 6 6) (drill 3.6) (layers "*.Cu" "*.Mask")
      (net 7 "T2-") (pinfunction "C") (pintype "passive"))
    (zone (net 0) (net_name "") (layer "F.SilkS") (name "Heatsink") (hatch edge 0.5)
      (connect_pads (clearance 0))
      (min_thickness 0.25) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints not_allowed))
      (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
      (polygon
        (pts
          (xy 103.45 84.3)
          (xy 103.45 87.1)
          (xy 119.55 87.1)
          (xy 119.55 84.3)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.SilkS") (name "Heatsink") (hatch edge 0.5)
      (connect_pads (clearance 0))
      (min_thickness 0.25) (filled_areas_thickness no)
      (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints not_allowed))
      (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
      (polygon
        (pts
          (xy 103.45 97.6)
          (xy 103.45 100.3)
          (xy 119.55 100.3)
          (xy 119.55 97.6)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-2_Horizontal_TabDown.wrl"
      (offset (xyz 0 -1.08 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 162 102.75)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "MFG#" "R82EC2100AA50J")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "10n" (at 2.5 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/T2_Inverting") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/T2_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 145.847349 105.25)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "MFG#" "UBW1H470MPD")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "50v")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 5.652651 -3.5) (layer "F.SilkS"))
    (fp_text value "47u" (at 1.75 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 22 "Q3{slash}4_Supply") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 130.75 114.5 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 9.5 0) (layer "F.SilkS"))
    (fp_text value "3k" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D6-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (at 120.59 102.5)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D4" (at 0.41 -2.25) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9) (layer "F.SilkS") hide)
    (fp_text user "K" (at 0 -1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "PulseCoil2") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (at 145.847349 114.75)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "MFG#" "UBW1J220MPD1TD")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "16v")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 5.5 3.75) (layer "F.SilkS"))
    (fp_text value "22u" (at 1.75 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal" (layer "F.Cu")
    (at 155 99.84 -90)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "Wattage" "2")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 10.16 3.25 90) (layer "F.SilkS"))
    (fp_text value "120" (at 10.16 0 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 6 "+12V") (pintype "passive"))
    (pad "2" thru_hole oval (at 20.32 0 270) (size 2.4 2.4) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 22 "Q3{slash}4_Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.7mm" (layer "F.Cu")
    (at 164 88)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.6) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 159.3 113.8 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual Operational Amplifiers, DIP-8/SOIC-8/TSSOP-8/VSSOP-8")
    (property "ki_keywords" "dual opamp")
    (attr through_hole)
    (fp_text reference "U1" (at -2.2 -0.05 90) (layer "F.SilkS"))
    (fp_text value "LM2904" (at 3.8 3.7 180) (layer "F.SilkS"))
    (fp_text user "V+" (at 6.4 0 90 unlocked) (layer "B.SilkS"))
    (fp_text user "V-" (at 3.2 7.5 90 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "/T1_Out") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/T1_Inverting") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/T1_Non-Inverting") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "V-") (pintype "power_in") (thermal_bridge_angle 45))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 24 "/T2_Non-Inverting") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "/T2_Inverting") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "/T2_Out") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 123.13 98.75)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at -2.13 0) (layer "F.SilkS"))
    (fp_text value "82k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D4-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 127.5 114.5 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R11" (at 9.5 0) (layer "F.SilkS"))
    (fp_text value "5.6k" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive") (thermal_bridge_angle 45))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.7mm" (layer "F.Cu")
    (at 95.5 131.5)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.6) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (at 135.25 104.92 -90)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "MFG#" "BZX85C15")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Zener diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D5" (at 5.08 2.25 90) (layer "F.SilkS"))
    (fp_text value "15 V" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (thermal_bridge_angle 45))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 129.62 85.75 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 3.87 -1.75) (layer "F.SilkS"))
    (fp_text value "20" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(Q4-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 159.38 96.25)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R15" (at -2.63 -0.5) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 23 "/T2_Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 124.25 114.5 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R16" (at 9.5 0 180) (layer "F.SilkS"))
    (fp_text value "3k" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D4-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D7-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (at 106.25 117.75)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D1" (at -2.25 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -3) (layer "F.SilkS") hide)
    (fp_text user "K" (at 0 -1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "PulseCoil1") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:L_Axial_L11.0mm_D4mm_P15.24mm_Horizontal_Fastron_MECC_with_symbol" (layer "F.Cu")
    (at 140 117.625 90)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4mm Fastron MECC")
    (property "Label" "221J")
    (property "MFG#" "77F220K-RC")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L1" (at 7.625 3 90) (layer "F.SilkS"))
    (fp_text value "22u" (at 7.5 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.5 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "+12V") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 159.38 99.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R14" (at -2.63 -2) (layer "F.SilkS"))
    (fp_text value "100k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 24 "/T2_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 120.75 114.5 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R12" (at 9.5 0 180) (layer "F.SilkS"))
    (fp_text value "5.6k" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D4-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive") (thermal_bridge_angle 45))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 99.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R13" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "6.2k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 26 "/T2_Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:L_Axial_L11.0mm_D4mm_P15.24mm_Horizontal_Fastron_MECC_with_symbol" (layer "F.Cu")
    (at 142.5 87)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=11*4mm^2, Fastron, MECC, http://www.fastrongroup.com/image-show/21/MECC.pdf?type=Complete-DataSheet&productType=series")
    (tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 11mm diameter 4mm Fastron MECC")
    (property "MFG#" "77F560J-TR-RC")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L3" (at 12.25 3) (layer "F.SilkS"))
    (fp_text value "56u" (at 7.5 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(Q4-C)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "Q3{slash}4_Supply") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L11.0mm_D4.5mm_P15.24mm_Horizontal_Fastron_MECC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x11_P2.54mm_Vertical" (layer "F.Cu")
    (at 100 130)
    (descr "Through hole straight socket strip, 1x11, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x11 2.54mm single row")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x11, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 3.75) (layer "F.SilkS"))
    (fp_text value "SIP Header" (at 3.5 -20 90) (layer "F.Fab"))
    (fp_text user "Or/W" (at 2.75 -32 unlocked) (layer "B.SilkS"))
    (fp_text user "W/Bl" (at 2.75 -20 unlocked) (layer "B.SilkS"))
    (fp_text user "Pnk" (at 2.75 -15.25 unlocked) (layer "B.SilkS"))
    (fp_text user "Wht" (at 0 3.75 unlocked) (layer "B.SilkS"))
    (fp_text user "Bk/Y" (at 0 -43.5 unlocked) (layer "B.SilkS"))
    (fp_text user "Bk/W" (at -2 -9 unlocked) (layer "B.SilkS"))
    (fp_text user "Yel" (at 2.75 -29.5 unlocked) (layer "B.SilkS"))
    (fp_text user "Gr/W" (at 2.75 -25 unlocked) (layer "B.SilkS"))
    (fp_text user "+12V" (at -4 -36.25 90 unlocked) (layer "F.SilkS"))
    (fp_text user "T2" (at -4 -40 90 unlocked) (layer "F.SilkS"))
    (fp_text user "GND" (at -4 -13 90 unlocked) (layer "F.SilkS"))
    (fp_text user "T1" (at -4 -2.25 90 unlocked) (layer "F.SilkS"))
    (fp_text user "P2" (at -4 -26 90 unlocked) (layer "F.SilkS"))
    (fp_text user "P1" (at -4 -18 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5 -20 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 4.3 4.3) (drill 2.1) (layers "*.Cu" "*.Mask")
      (net 5 "T1-") (pinfunction "Pin_1") (pintype "passive"))
    (pad "4" thru_hole roundrect (at 0 -12 180) (size 4 3.1) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive") (thermal_bridge_width 2) (thermal_bridge_angle 45))
    (pad "5" thru_hole roundrect (at 0 -16 180) (size 4 3.1) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 4 "PulseCoil1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole roundrect (at 0 -20 180) (size 4 3.1) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive") (thermal_bridge_width 2) (thermal_bridge_angle 45))
    (pad "7" thru_hole roundrect (at 0 -24 180) (size 4 3.1) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive") (thermal_bridge_width 2) (thermal_bridge_angle 45))
    (pad "8" thru_hole roundrect (at 0 -28 180) (size 4 3.1) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 2 "PulseCoil2") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole roundrect (at 0 -32 180) (size 4 3.1) (drill 1.4) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 6 "+12V") (pinfunction "Pin_9") (pintype "passive"))
    (pad "11" thru_hole circle (at 0 -40 180) (size 4.3 4.3) (drill 2.1) (layers "*.Cu" "*.Mask")
      (net 7 "T2-") (pinfunction "Pin_11") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x11_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 106.25 107.25)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "MFG#" "R82EC2150AA50J")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at -2.5 0) (layer "F.SilkS"))
    (fp_text value "15n" (at 2.5 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "PulseCoil2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 114.25 106.88 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at -1.94 0 -180) (layer "F.SilkS"))
    (fp_text value "3k" (at 3.8 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "PulseCoil2") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive") (thermal_bridge_angle 45))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (at 120.59 117.75)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D3" (at 0.16 2.5) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0.062651 -3) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "PulseCoil1") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 91.25)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at -2.25 0) (layer "F.SilkS"))
    (fp_text value "6.2k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(Q4-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 26 "/T2_Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 122 134.25)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "5")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 3.5 -1.75) (layer "F.SilkS"))
    (fp_text value "20" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(Q1-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q3-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 94)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R24" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "75k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 26 "/T2_Out") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 24 "/T2_Non-Inverting") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 121)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R20" (at -2.75 0) (layer "F.SilkS"))
    (fp_text value "6.2k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Filtered+12v") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 25 "/T1_Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal_with_symbol" (layer "F.Cu")
    (at 142.5 129.25)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Denso 21119-2120 Reproduction.kicad_sch")
    (property "Sheetname" "")
    (property "Tolerance" "2")
    (property "Wattage" "1/8")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at -2.25 0) (layer "F.SilkS"))
    (fp_text value "6.2k" (at 3.8 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(Q3-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 25 "/T1_Out") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 93 137.5) (end 167 137.5)
    (layer "Edge.Cuts"))
  (gr_line (start 93 82.5) (end 90 85.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 94.5 120) (mid 94.207107 120.707107) (end 93.5 121)
    (layer "Edge.Cuts"))
  (gr_line (start 90 134.5) (end 93 137.5)
    (layer "Edge.Cuts"))
  (gr_line (start 93.5 121) (end 90 121)
    (layer "Edge.Cuts"))
  (gr_line (start 90 121) (end 90 134.5)
    (layer "Edge.Cuts"))
  (gr_line (start 93.5 99) (end 90 99)
    (layer "Edge.Cuts"))
  (gr_arc (start 93.5 99) (mid 94.207107 99.292893) (end 94.5 100)
    (layer "Edge.Cuts"))
  (gr_line (start 170 134.5) (end 170 85.5)
    (layer "Edge.Cuts"))
  (gr_line (start 167 82.5) (end 93 82.5)
    (layer "Edge.Cuts"))
  (gr_line (start 90 85.5) (end 90 99)
    (layer "Edge.Cuts"))
  (gr_line (start 94.5 120) (end 94.5 100)
    (layer "Edge.Cuts"))
  (gr_line (start 167 82.5) (end 170 85.5)
    (layer "Edge.Cuts"))
  (gr_line (start 170 134.5) (end 167 137.5)
    (layer "Edge.Cuts"))
  (gr_text "Denso Ignition Module\n21119-2120\n131800-0130\n12V  TNCK02" (at 119 89.25) (layer "B.SilkS"))
  (gr_text "Reproduction\nv1 2023-04-27" (at 118.75 97) (layer "B.SilkS"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 90 82.5) (xy 170 82.5))
    (height -3)
    (gr_text "80.0000 mm" (at 130 78.35) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 90 82.5) (xy 170 82.5))
    (height -7)
    (gr_text "3.1496 in" (at 130 74.35) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 90 82.5) (xy 90 137.5))
    (height 4.25)
    (gr_text "55.0000 mm" (at 84.6 110 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 90 82.5) (xy 90 137.5))
    (height 8.25)
    (gr_text "2.1654 in" (at 80.6 110 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 7) (net_name "T2-") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 1))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 2) (smoothing fillet) (radius 5))
    (polygon
      (pts
        (xy 111.75 97.25)
        (xy 101 97.25)
        (xy 96 92.25)
        (xy 96 86)
        (xy 101.75 86)
        (xy 103 87.25)
        (xy 111.75 87.25)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers "F&B.Cu") (name "GND") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 88.75 81.25)
        (xy 88.75 138.75)
        (xy 171.25 138.75)
        (xy 171.25 81.25)
      )
    )
  )
  (zone (net 5) (net_name "T1-") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 1))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 2) (smoothing fillet) (radius 5))
    (polygon
      (pts
        (xy 111.75 122.75)
        (xy 101 122.75)
        (xy 96 127.75)
        (xy 96 134)
        (xy 101.75 134)
        (xy 103 132.75)
        (xy 111.75 132.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "*.SilkS") (name "Case Slot") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads not_allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 92.4 84)
        (xy 168.5 84)
        (xy 168.5 136)
        (xy 92.2 136)
        (xy 92.2 84.2)
        (xy 89.8 82.5)
        (xy 89.8 137.7)
        (xy 170.2 137.7)
        (xy 170.2 82.3)
        (xy 90 82.3)
      )
    )
  )
)
