<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="32.385" y1="19.3775" x2="32.385" y2="3.175" width="0.1524" layer="20"/>
<wire x1="32.385" y1="3.175" x2="34.925" y2="0.635" width="0.1524" layer="20" curve="90"/>
<wire x1="34.925" y1="0.635" x2="53.3275" y2="0.635" width="0.1524" layer="20"/>
<wire x1="53.3275" y1="0.635" x2="55.8675" y2="3.175" width="0.1524" layer="20" curve="90"/>
<wire x1="55.8675" y1="3.175" x2="55.8675" y2="19.3775" width="0.1524" layer="20"/>
<wire x1="55.8675" y1="19.3775" x2="53.3275" y2="21.9175" width="0.1524" layer="20" curve="90"/>
<wire x1="53.3275" y1="21.9175" x2="34.925" y2="21.9175" width="0.1524" layer="20"/>
<wire x1="34.925" y1="21.9175" x2="32.385" y2="19.3775" width="0.1524" layer="20" curve="90"/>
</plain>
<libraries>
<library name="supply pins">
<packages>
<package name="IO.2">
</package>
</packages>
</library>
<library name="resistors">
<packages>
<package name="0.2&quot;">
<description>0.2"  (5mm) lead spacing, 1/8W (flat), 1/4W (standing)</description>
</package>
</packages>
</library>
<library name="jacks">
<packages>
<package name="DC_TS">
</package>
<package name="2PADS">
</package>
</packages>
</library>
<library name="switches">
<packages>
<package name="3PDT.LUGS">
<description>&lt;b&gt; Latching Footswitch, Solder Lugs&lt;/b&gt;
&lt;br&gt;&lt;a href="http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt/"&gt;http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt/&lt;/a&gt;
&lt;p&gt;
&lt;b&gt;Momentary Footswitch, Solder Lugs&lt;/b&gt;
&lt;br&gt;&lt;a href="http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt-momentary/"&gt;http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt-momentary/&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BYP.1" library="supply pins" package="IO.2" value="BYP.2"/>
<element name="CLR" library="resistors" package="0.2&quot;" value=""/>
<element name="DC1" library="jacks" package="DC_TS" value="DC_TS"/>
<element name="DC2" library="jacks" package="DC_TS" value="DC_TS"/>
<element name="INPUT" library="jacks" package="2PADS" value=""/>
<element name="OUTPUT" library="jacks" package="2PADS" value=""/>
<element name="3PDT" library="switches" package="3PDT.LUGS" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="INPUT" pad="S"/>
<contactref element="OUTPUT" pad="S"/>
<contactref element="DC1" pad="GND"/>
<contactref element="DC2" pad="GND"/>
<contactref element="3PDT" pad="B3"/>
<contactref element="3PDT" pad="A2"/>
<contactref element="BYP.1" pad="G"/>
<contactref element="3PDT" pad="A3"/>
</signal>
<signal name="N$1">
<contactref element="3PDT" pad="B2"/>
<contactref element="BYP.1" pad="IN"/>
</signal>
<signal name="N$2">
<contactref element="BYP.1" pad="OUT"/>
<contactref element="3PDT" pad="C1"/>
</signal>
<signal name="N$3">
<contactref element="OUTPUT" pad="T"/>
<contactref element="3PDT" pad="C2"/>
</signal>
<signal name="N$4">
<contactref element="INPUT" pad="T"/>
<contactref element="3PDT" pad="C3"/>
<contactref element="3PDT" pad="B1"/>
</signal>
<signal name="N$5">
<contactref element="DC1" pad="PWR"/>
<contactref element="CLR" pad="2"/>
<contactref element="DC2" pad="PWR"/>
</signal>
<signal name="N$7">
<contactref element="CLR" pad="1"/>
<contactref element="BYP.1" pad="+"/>
</signal>
<signal name="N$8">
<contactref element="BYP.1" pad="-"/>
<contactref element="3PDT" pad="A1"/>
<contactref element="BYP.1" pad="SW"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
