<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="73.66" y1="48.26" x2="11.43" y2="48.26" width="0.1016" layer="20"/>
<wire x1="8.89" y1="34.29" x2="10.16" y2="35.56" width="0.1016" layer="20" curve="90"/>
<wire x1="10.16" y1="35.56" x2="10.16" y2="46.99" width="0.1016" layer="20"/>
<wire x1="10.16" y1="46.99" x2="11.43" y2="48.26" width="0.1016" layer="20" curve="-90"/>
<wire x1="8.89" y1="34.29" x2="1.27" y2="34.29" width="0.1016" layer="20"/>
<wire x1="1.27" y1="34.29" x2="0" y2="33.02" width="0.1016" layer="20" curve="90"/>
<wire x1="0" y1="33.02" x2="0" y2="1.27" width="0.1016" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0.1016" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="86.36" y2="0" width="0.1016" layer="20"/>
<wire x1="86.36" y1="0" x2="87.63" y2="1.27" width="0.1016" layer="20" curve="90"/>
<wire x1="87.63" y1="1.27" x2="87.63" y2="31.115" width="0.1016" layer="20"/>
<wire x1="87.63" y1="31.115" x2="86.36" y2="32.385" width="0.1016" layer="20" curve="90"/>
<wire x1="86.36" y1="32.385" x2="76.2" y2="32.385" width="0.1016" layer="20"/>
<wire x1="76.2" y1="32.385" x2="74.93" y2="33.655" width="0.1016" layer="20" curve="-90"/>
<wire x1="74.93" y1="33.655" x2="74.93" y2="46.99" width="0.1016" layer="20"/>
<wire x1="74.93" y1="46.99" x2="73.66" y2="48.26" width="0.1016" layer="20" curve="90"/>
<text>Quasar Tiny Amp</text>
<text>GFE Hand Made</text>
<text>gnd   in</text>
<text>Test</text>
<text>Point</text>
<text>SP-</text>
<text>SP+</text>
<text>+18V</text>
<text>gnd</text>
<text>Designed and fully manufactured</text>
<text>in Italy by GFE Hand Made</text>
<text>Please rock it loud!</text>
</plain>
<libraries>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
<package name="1003">
</package>
</packages>
</library>
<library name="gm-caps-ceramic">
<description>&lt;b&gt;Capacitors, Ceramic&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;very small capacitances: 1 - 1000pF
&lt;/ul&gt;</description>
<packages>
<package name="050X030_050_1">
</package>
<package name="050X030_025">
<description>&lt;b&gt;5mm x 3mm, 2.5mm lead spacing
&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
<package name="063_025">
<description>&lt;b&gt;6.3mm diameter, 2.5 mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="gm-pots">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;chassis-mount (e.g., Alpha 16mm) pots&lt;/li&gt;
&lt;li&gt;board-mount trim pots (1/4" and 3/8")&lt;/li&gt;
&lt;li&gt; all pot values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="B25P">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;&lt;p&gt;
1/4" on-board trim potentiometer</description>
</package>
<package name="16MM-PCB-MOUNT">
<description>&lt;b&gt;PCB Mount 16mm Alpha Potentiometer&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="tubes">
<description>Tubes devices</description>
<packages>
<package name="NOVAL">
</package>
</packages>
</library>
<library name="gm-caps-film-chicklet">
<description>&lt;b&gt;Capacitors, Film, Chicklet&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;100pF - 0.1uF (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors
&lt;li&gt;available from smallbearelec.com as Panasonic ECQ-B capacitors
&lt;li&gt;these become quite large for values near 1uF
&lt;/ul&gt;</description>
<packages>
<package name="070X030">
<description>&lt;b&gt;7mm x 3mm, 5mm lead spacing&lt;/b&gt;
&lt;p&gt;Panasonic ECQ-B</description>
</package>
<package name="075X035">
<description>&lt;b&gt;7.5mm x 3.5mm, 5mm lead spacing&lt;/b&gt;

&lt;p&gt;Panasonic ECQ-B</description>
</package>
<package name="080X050">
<description>&lt;b&gt;8mm x 5mm, 5mm lead spacing&lt;/b&gt;
&lt;p&gt;Panasonic ECQ-B</description>
</package>
</packages>
</library>
<library name="GFE LOGO">
<packages>
<package name="LOGO-GRANDE">
<description>Logo Grande GFE Hand Made senza scritta</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="REG" library="linear" package="SOT223" value="317EMP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="gm-resistors" package="R0207/3" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="gm-caps-ceramic" package="050X030_050_1" value="100n - cer">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="gm-caps-electro-pol" package="050_020_1" value="47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="gm-diodes" package="DO41-3" value="schottky">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+18V1" library="gm-supply" package="SQUARE" value="+18V(T)">
<attribute name="NAME"/>
</element>
<element name="GND1" library="gm-supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="ADJ" library="gm-pots" package="B25P" value="200R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="gm-caps-electro-pol" package="050_020_1" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TL072" library="gm-ics" package="DIL08" value="TL072P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DIRT" library="gm-pots" package="16MM-PCB-MOUNT" value="1M - A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MASTER" library="gm-pots" package="16MM-PCB-MOUNT" value="250K - A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PREAMP" library="gm-pots" package="16MM-PCB-MOUNT" value="1M -A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V2" library="tubes" package="NOVAL" value=""/>
<element name="R2" library="gm-resistors" package="R0207/3" value="270R - 0.5W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="gm-caps-film-chicklet" package="070X030" value="150n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="gm-resistors" package="R0207/3" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="gm-resistors" package="R0207/3" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="gm-caps-electro-pol" package="050_020_1" value="47u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="gm-resistors" package="R0207/3" value="2M2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="gm-resistors" package="R0207/3" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="gm-caps-ceramic" package="050X030_025" value="27p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="gm-resistors" package="R0207/3" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="gm-resistors" package="R0207/3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="gm-resistors" package="R0207/3" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="gm-caps-film-chicklet" package="075X035" value="470n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="gm-resistors" package="R0207/3" value="220k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="gm-caps-film-chicklet" package="070X030" value="27n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="gm-resistors" package="R0207/3" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="gm-resistors" package="R0207/3" value="2.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="gm-caps-film-chicklet" package="075X035" value="680n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TL071" library="gm-ics" package="DIL08" value="TL071P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LM386" library="gm-ics" package="DIL08" value="LM386">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="gm-caps-film-chicklet" package="070X030" value="27n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="gm-resistors" package="R0207/3" value="470K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="gm-caps-film-chicklet" package="070X030" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="gm-caps-ceramic" package="050X030_025" value="470p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="gm-caps-film-chicklet" package="080X050" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="gm-resistors" package="R0207/3" value="2M2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="gm-resistors" package="R0207/3" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="gm-caps-film-chicklet" package="080X050" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="gm-caps-film-chicklet" package="080X050" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="gm-resistors" package="R0207/3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="gm-resistors" package="R0207/3" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="gm-caps-film-chicklet" package="070X030" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="gm-caps-electro-pol" package="063_025" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="gm-caps-film-chicklet" package="070X030" value="47n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="gm-resistors" package="1003" value="8.2R - 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND7" library="gm-supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="GND8" library="gm-supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="C6" library="gm-caps-film-chicklet" package="080X050" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="gm-resistors" package="1003" value="8.2R - 1W">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TESTPOINT" library="gm-supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="SPKR" library="gm-supply" package="SQUARE" value="OUT(T)">
<attribute name="NAME"/>
</element>
<element name="IN" library="gm-supply" package="SQUARE" value="IN(T)">
<attribute name="NAME"/>
</element>
<element name="U$1" library="GFE LOGO" package="LOGO-GRANDE" value=""/>
</elements>
<signals>
<signal name="+18V">
<contactref element="+18V1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="R3" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="-"/>
<contactref element="GND1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="ADJ" pad="1"/>
<contactref element="ADJ" pad="2"/>
<contactref element="C3" pad="-"/>
<contactref element="V2" pad="4"/>
<contactref element="V2" pad="5"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="MASTER" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="TL072" pad="4"/>
<contactref element="PREAMP" pad="1"/>
<contactref element="TL071" pad="4"/>
<contactref element="R15" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="LM386" pad="2"/>
<contactref element="LM386" pad="4"/>
<contactref element="R18" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="GND7" pad="1"/>
<contactref element="C5" pad="-"/>
<contactref element="GND8" pad="1"/>
</signal>
<signal name="VA">
<contactref element="D1" pad="C"/>
<contactref element="C2" pad="+"/>
<contactref element="C1" pad="2"/>
<contactref element="REG" pad="3"/>
<contactref element="TL072" pad="8"/>
<contactref element="TL071" pad="7"/>
<contactref element="LM386" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="REG" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="ADJ" pad="3"/>
</signal>
<signal name="VR">
<contactref element="REG" pad="4"/>
<contactref element="C3" pad="+"/>
<contactref element="R2" pad="1"/>
<contactref element="V2" pad="9"/>
<contactref element="TESTPOINT" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="TL072" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VB">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C5" pad="+"/>
<contactref element="R5" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="TL072" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="TL072" pad="2"/>
<contactref element="TL072" pad="1"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="TL072" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="C7" pad="2"/>
<contactref element="DIRT" pad="1"/>
<contactref element="TL072" pad="7"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="DIRT" pad="3"/>
<contactref element="R7" pad="2"/>
<contactref element="DIRT" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R8" pad="1"/>
<contactref element="V2" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="V2" pad="3"/>
<contactref element="R9" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="V2" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="C10" pad="2"/>
<contactref element="MASTER" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="V2" pad="7"/>
<contactref element="PREAMP" pad="2"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R12" pad="1"/>
<contactref element="V2" pad="6"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R13" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="V2" pad="8"/>
</signal>
<signal name="N$18">
<contactref element="C14" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R14" pad="1"/>
<contactref element="PREAMP" pad="3"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="MASTER" pad="2"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="TL071" pad="2"/>
<contactref element="TL071" pad="6"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R11" pad="1"/>
<contactref element="TL071" pad="3"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="C12" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="C17" pad="2"/>
</signal>
<signal name="PWR_AMP">
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="LM386" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="C19" pad="1"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="LM386" pad="5"/>
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="-"/>
</signal>
<signal name="OUT">
<contactref element="C18" pad="+"/>
<contactref element="SPKR" pad="1"/>
</signal>
<signal name="IN">
<contactref element="C4" pad="1"/>
<contactref element="IN" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
