(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 488)
    (no_connects 0)
    (area 95.174999 69.774999 139.775001 133.425001)
    (thickness 1.6)
    (drawings 10)
    (tracks 0)
    (zones 0)
    (modules 14)
    (nets 155)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.7)
    (user_trace_width 1.7)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 101.6 101.6)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(P2-Pad1)")
  (net 10 "Net-(P2-Pad2)")
  (net 11 "Net-(P2-Pad3)")
  (net 12 "Net-(P2-Pad4)")
  (net 13 "Net-(P2-Pad5)")
  (net 14 "Net-(P2-Pad6)")
  (net 15 "Net-(P2-Pad7)")
  (net 16 "Net-(P2-Pad8)")
  (net 17 "Net-(P2-Pad9)")
  (net 18 "Net-(P2-Pad10)")
  (net 19 "Net-(P2-Pad11)")
  (net 20 "Net-(P2-Pad12)")
  (net 21 "Net-(P2-Pad13)")
  (net 22 "Net-(P2-Pad14)")
  (net 23 "Net-(P2-Pad15)")
  (net 24 "Net-(P2-Pad16)")
  (net 25 "Net-(P2-Pad17)")
  (net 26 "Net-(P2-Pad18)")
  (net 27 "Net-(P2-Pad19)")
  (net 28 "Net-(P2-Pad20)")
  (net 29 "Net-(P2-Pad21)")
  (net 30 "Net-(P2-Pad22)")
  (net 31 "Net-(P2-Pad23)")
  (net 32 "Net-(P2-Pad24)")
  (net 33 "Net-(P3-Pad1)")
  (net 34 "Net-(P3-Pad2)")
  (net 35 "Net-(P3-Pad3)")
  (net 36 "Net-(P3-Pad4)")
  (net 37 "Net-(P3-Pad5)")
  (net 38 "Net-(P3-Pad6)")
  (net 39 "Net-(P3-Pad7)")
  (net 40 "Net-(P3-Pad8)")
  (net 41 "Net-(P3-Pad9)")
  (net 42 "Net-(P3-Pad10)")
  (net 43 "Net-(P3-Pad11)")
  (net 44 "Net-(P3-Pad12)")
  (net 45 "Net-(P3-Pad13)")
  (net 46 "Net-(P3-Pad14)")
  (net 47 "Net-(P3-Pad15)")
  (net 48 "Net-(P3-Pad16)")
  (net 49 "Net-(P3-Pad17)")
  (net 50 "Net-(P3-Pad18)")
  (net 51 "Net-(P3-Pad19)")
  (net 52 "Net-(P3-Pad20)")
  (net 53 "Net-(P3-Pad21)")
  (net 54 "Net-(P3-Pad22)")
  (net 55 "Net-(P3-Pad23)")
  (net 56 "Net-(P3-Pad24)")
  (net 57 "Net-(P4-Pad1)")
  (net 58 "Net-(P4-Pad2)")
  (net 59 "Net-(P4-Pad3)")
  (net 60 "Net-(P4-Pad4)")
  (net 61 "Net-(P4-Pad5)")
  (net 62 "Net-(P4-Pad6)")
  (net 63 "Net-(P4-Pad7)")
  (net 64 "Net-(P4-Pad8)")
  (net 65 "Net-(P4-Pad9)")
  (net 66 "Net-(P4-Pad10)")
  (net 67 "Net-(P4-Pad11)")
  (net 68 "Net-(P4-Pad12)")
  (net 69 "Net-(P4-Pad13)")
  (net 70 "Net-(P4-Pad14)")
  (net 71 "Net-(P4-Pad15)")
  (net 72 "Net-(P4-Pad16)")
  (net 73 "Net-(P4-Pad17)")
  (net 74 "Net-(P4-Pad18)")
  (net 75 "Net-(P4-Pad19)")
  (net 76 "Net-(P4-Pad20)")
  (net 77 "Net-(P4-Pad21)")
  (net 78 "Net-(P4-Pad22)")
  (net 79 "Net-(P4-Pad23)")
  (net 80 "Net-(P4-Pad24)")
  (net 81 "Net-(P5-Pad1)")
  (net 82 "Net-(P6-Pad1)")
  (net 83 "Net-(P6-Pad2)")
  (net 84 "Net-(P6-Pad3)")
  (net 85 "Net-(P6-Pad4)")
  (net 86 "Net-(P6-Pad5)")
  (net 87 "Net-(P6-Pad6)")
  (net 88 "Net-(P6-Pad7)")
  (net 89 "Net-(P6-Pad8)")
  (net 90 "Net-(P6-Pad9)")
  (net 91 "Net-(P6-Pad10)")
  (net 92 "Net-(P6-Pad11)")
  (net 93 "Net-(P6-Pad12)")
  (net 94 "Net-(P6-Pad13)")
  (net 95 "Net-(P6-Pad14)")
  (net 96 "Net-(P6-Pad15)")
  (net 97 "Net-(P6-Pad16)")
  (net 98 "Net-(P6-Pad17)")
  (net 99 "Net-(P6-Pad18)")
  (net 100 "Net-(P6-Pad19)")
  (net 101 "Net-(P6-Pad20)")
  (net 102 "Net-(P6-Pad21)")
  (net 103 "Net-(P6-Pad22)")
  (net 104 "Net-(P6-Pad23)")
  (net 105 "Net-(P6-Pad24)")
  (net 106 "Net-(P7-Pad1)")
  (net 107 "Net-(P7-Pad2)")
  (net 108 "Net-(P7-Pad3)")
  (net 109 "Net-(P7-Pad4)")
  (net 110 "Net-(P7-Pad5)")
  (net 111 "Net-(P7-Pad6)")
  (net 112 "Net-(P7-Pad7)")
  (net 113 "Net-(P7-Pad8)")
  (net 114 "Net-(P7-Pad9)")
  (net 115 "Net-(P7-Pad10)")
  (net 116 "Net-(P7-Pad11)")
  (net 117 "Net-(P7-Pad12)")
  (net 118 "Net-(P7-Pad13)")
  (net 119 "Net-(P7-Pad14)")
  (net 120 "Net-(P7-Pad15)")
  (net 121 "Net-(P7-Pad16)")
  (net 122 "Net-(P7-Pad17)")
  (net 123 "Net-(P7-Pad18)")
  (net 124 "Net-(P7-Pad19)")
  (net 125 "Net-(P7-Pad20)")
  (net 126 "Net-(P7-Pad21)")
  (net 127 "Net-(P7-Pad22)")
  (net 128 "Net-(P7-Pad23)")
  (net 129 "Net-(P7-Pad24)")
  (net 130 "Net-(P8-Pad1)")
  (net 131 "Net-(P8-Pad2)")
  (net 132 "Net-(P8-Pad3)")
  (net 133 "Net-(P8-Pad4)")
  (net 134 "Net-(P8-Pad5)")
  (net 135 "Net-(P8-Pad6)")
  (net 136 "Net-(P8-Pad7)")
  (net 137 "Net-(P8-Pad8)")
  (net 138 "Net-(P8-Pad9)")
  (net 139 "Net-(P8-Pad10)")
  (net 140 "Net-(P8-Pad11)")
  (net 141 "Net-(P8-Pad12)")
  (net 142 "Net-(P8-Pad13)")
  (net 143 "Net-(P8-Pad14)")
  (net 144 "Net-(P8-Pad15)")
  (net 145 "Net-(P8-Pad16)")
  (net 146 "Net-(P8-Pad17)")
  (net 147 "Net-(P8-Pad18)")
  (net 148 "Net-(P8-Pad19)")
  (net 149 "Net-(P8-Pad20)")
  (net 150 "Net-(P8-Pad21)")
  (net 151 "Net-(P8-Pad22)")
  (net 152 "Net-(P8-Pad23)")
  (net 153 "Net-(P8-Pad24)")
  (net 154 "Net-(P9-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad11)")
    (add_net "Net-(P2-Pad12)")
    (add_net "Net-(P2-Pad13)")
    (add_net "Net-(P2-Pad14)")
    (add_net "Net-(P2-Pad15)")
    (add_net "Net-(P2-Pad16)")
    (add_net "Net-(P2-Pad17)")
    (add_net "Net-(P2-Pad18)")
    (add_net "Net-(P2-Pad19)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad20)")
    (add_net "Net-(P2-Pad21)")
    (add_net "Net-(P2-Pad22)")
    (add_net "Net-(P2-Pad23)")
    (add_net "Net-(P2-Pad24)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P2-Pad9)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad11)")
    (add_net "Net-(P3-Pad12)")
    (add_net "Net-(P3-Pad13)")
    (add_net "Net-(P3-Pad14)")
    (add_net "Net-(P3-Pad15)")
    (add_net "Net-(P3-Pad16)")
    (add_net "Net-(P3-Pad17)")
    (add_net "Net-(P3-Pad18)")
    (add_net "Net-(P3-Pad19)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad20)")
    (add_net "Net-(P3-Pad21)")
    (add_net "Net-(P3-Pad22)")
    (add_net "Net-(P3-Pad23)")
    (add_net "Net-(P3-Pad24)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad10)")
    (add_net "Net-(P4-Pad11)")
    (add_net "Net-(P4-Pad12)")
    (add_net "Net-(P4-Pad13)")
    (add_net "Net-(P4-Pad14)")
    (add_net "Net-(P4-Pad15)")
    (add_net "Net-(P4-Pad16)")
    (add_net "Net-(P4-Pad17)")
    (add_net "Net-(P4-Pad18)")
    (add_net "Net-(P4-Pad19)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad20)")
    (add_net "Net-(P4-Pad21)")
    (add_net "Net-(P4-Pad22)")
    (add_net "Net-(P4-Pad23)")
    (add_net "Net-(P4-Pad24)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P4-Pad9)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad10)")
    (add_net "Net-(P6-Pad11)")
    (add_net "Net-(P6-Pad12)")
    (add_net "Net-(P6-Pad13)")
    (add_net "Net-(P6-Pad14)")
    (add_net "Net-(P6-Pad15)")
    (add_net "Net-(P6-Pad16)")
    (add_net "Net-(P6-Pad17)")
    (add_net "Net-(P6-Pad18)")
    (add_net "Net-(P6-Pad19)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad20)")
    (add_net "Net-(P6-Pad21)")
    (add_net "Net-(P6-Pad22)")
    (add_net "Net-(P6-Pad23)")
    (add_net "Net-(P6-Pad24)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad5)")
    (add_net "Net-(P6-Pad6)")
    (add_net "Net-(P6-Pad7)")
    (add_net "Net-(P6-Pad8)")
    (add_net "Net-(P6-Pad9)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad10)")
    (add_net "Net-(P7-Pad11)")
    (add_net "Net-(P7-Pad12)")
    (add_net "Net-(P7-Pad13)")
    (add_net "Net-(P7-Pad14)")
    (add_net "Net-(P7-Pad15)")
    (add_net "Net-(P7-Pad16)")
    (add_net "Net-(P7-Pad17)")
    (add_net "Net-(P7-Pad18)")
    (add_net "Net-(P7-Pad19)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad20)")
    (add_net "Net-(P7-Pad21)")
    (add_net "Net-(P7-Pad22)")
    (add_net "Net-(P7-Pad23)")
    (add_net "Net-(P7-Pad24)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P7-Pad5)")
    (add_net "Net-(P7-Pad6)")
    (add_net "Net-(P7-Pad7)")
    (add_net "Net-(P7-Pad8)")
    (add_net "Net-(P7-Pad9)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad10)")
    (add_net "Net-(P8-Pad11)")
    (add_net "Net-(P8-Pad12)")
    (add_net "Net-(P8-Pad13)")
    (add_net "Net-(P8-Pad14)")
    (add_net "Net-(P8-Pad15)")
    (add_net "Net-(P8-Pad16)")
    (add_net "Net-(P8-Pad17)")
    (add_net "Net-(P8-Pad18)")
    (add_net "Net-(P8-Pad19)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P8-Pad20)")
    (add_net "Net-(P8-Pad21)")
    (add_net "Net-(P8-Pad22)")
    (add_net "Net-(P8-Pad23)")
    (add_net "Net-(P8-Pad24)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(P8-Pad5)")
    (add_net "Net-(P8-Pad6)")
    (add_net "Net-(P8-Pad7)")
    (add_net "Net-(P8-Pad8)")
    (add_net "Net-(P8-Pad9)")
    (add_net "Net-(P9-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 589BEA09)
    (at 135.89 80.01)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (fp_text reference P9 (at 0 -2.39) (layer F.SilkS) hide)
    (fp_text value CONN_01X18 (at 0 45.57) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (pad 18 thru_hole rect (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(P9-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x18_Pitch2.54mm.wrl
      (at (xyz 0 -0.85 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x24_Pitch2.54mm (layer F.Cu) (tedit 589BE9D6)
    (at 120.65 72.39)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (fp_text reference P5 (at 0 -2.39) (layer F.SilkS) hide)
    (fp_text value CONN_01X24 (at 0 60.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 21 thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 22 thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 23 thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (pad 24 thru_hole rect (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P5-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x24_Pitch2.54mm.wrl
      (at (xyz 0 -1.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 589BE973)
    (at 105.41 120.65 180)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X16 (at 0 40.49 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole rect (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 589B8379)
    (at 135.89 129.54)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference H (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 589B8373)
    (at 99.06 129.54)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference H (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 589B8366)
    (at 135.89 73.66)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference H (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 589B836B)
    (at 99.06 73.66)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference H (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBVA-G_08x5.00mm_Vertical (layer F.Cu) (tedit 589B8831)
    (at 99.1 119.1 90)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBVA-G; number of pins: 08; pin pitch: 5.00mm; Vertical || order number: 1755574 12A || order number: 1924253 16A (HC)")
    (tags "phoenix_contact connector MSTBVA_01x08_G_5.00mm")
    (fp_text reference J1 (at 17.5 -6 90) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_1x08 (at 17.5 5.3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 5 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 10 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 15 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 20 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 25 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 30 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 35 0 90) (size 2.1 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (model Connectors_Phoenix.3dshapes/PhoenixContact_MSTBVA-G_08x5.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PerfProto:Socket_Strip_Straight_1x24_Pitch2.54mm (layer F.Cu) (tedit 589B90CF)
    (at 110.49 72.39)
    (descr "Through hole straight socket strip, 1x24, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x24 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X24 (at 0 60.75) (layer F.Fab))
    (pad 3 thru_hole trapezoid (at 0 5.08 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P2-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P2-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P2-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P2-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P2-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P2-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P2-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P2-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P2-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P2-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad24)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P2-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P2-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P2-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P2-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P2-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P2-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P2-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P2-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P2-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P2-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad3)"))
    (pad 24 thru_hole trapezoid (at 0 58.42) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P2-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P2-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P2-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P2-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P2-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P2-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P2-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P2-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P2-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P2-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad3)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 1 thru_hole trapezoid (at 0 0) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P2-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P2-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P2-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P2-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P2-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P2-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P2-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P2-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P2-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P2-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P2-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P2-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P2-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P2-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P2-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad24)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x24_Pitch2.54mm.wrl
      (at (xyz 0 -1.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module PerfProto:Socket_Strip_Straight_1x24_Pitch2.54mm (layer F.Cu) (tedit 589B90CF)
    (at 113.03 72.39)
    (descr "Through hole straight socket strip, 1x24, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x24 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X24 (at 0 60.75) (layer F.Fab))
    (pad 3 thru_hole trapezoid (at 0 5.08 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P3-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P3-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P3-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P3-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P3-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P3-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P3-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P3-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P3-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P3-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P3-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P3-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P3-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P3-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P3-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P3-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P3-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P3-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P3-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P3-Pad24)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P3-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P3-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P3-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P3-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P3-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P3-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P3-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P3-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P3-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P3-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P3-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P3-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P3-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P3-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P3-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P3-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P3-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P3-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P3-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P3-Pad3)"))
    (pad 24 thru_hole trapezoid (at 0 58.42) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P3-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P3-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P3-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P3-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P3-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P3-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P3-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P3-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P3-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P3-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P3-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P3-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P3-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P3-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P3-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P3-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P3-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P3-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P3-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P3-Pad3)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P3-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P3-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P3-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P3-Pad2)"))
    (pad 1 thru_hole trapezoid (at 0 0) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P3-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P3-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P3-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P3-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P3-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P3-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P3-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P3-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P3-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P3-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P3-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P3-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P3-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P3-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P3-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P3-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P3-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P3-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P3-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P3-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P3-Pad24)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x24_Pitch2.54mm.wrl
      (at (xyz 0 -1.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module PerfProto:Socket_Strip_Straight_1x24_Pitch2.54mm (layer F.Cu) (tedit 589B90CF)
    (at 115.57 72.39)
    (descr "Through hole straight socket strip, 1x24, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x24 2.54mm single row")
    (fp_text reference P4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X24 (at 0 60.75) (layer F.Fab))
    (pad 3 thru_hole trapezoid (at 0 5.08 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P4-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P4-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(P4-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(P4-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(P4-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(P4-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(P4-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(P4-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(P4-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(P4-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(P4-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(P4-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(P4-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(P4-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(P4-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(P4-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(P4-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(P4-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(P4-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(P4-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(P4-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(P4-Pad24)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(P4-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(P4-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(P4-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(P4-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(P4-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(P4-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(P4-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(P4-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(P4-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(P4-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(P4-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(P4-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(P4-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(P4-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(P4-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(P4-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(P4-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(P4-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(P4-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(P4-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P4-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P4-Pad3)"))
    (pad 24 thru_hole trapezoid (at 0 58.42) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(P4-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(P4-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(P4-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(P4-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(P4-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(P4-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(P4-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(P4-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(P4-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(P4-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(P4-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(P4-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(P4-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(P4-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(P4-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(P4-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(P4-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(P4-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(P4-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(P4-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P4-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P4-Pad3)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P4-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P4-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P4-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P4-Pad2)"))
    (pad 1 thru_hole trapezoid (at 0 0) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P4-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P4-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P4-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P4-Pad1)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P4-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P4-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(P4-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(P4-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(P4-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(P4-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(P4-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(P4-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(P4-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(P4-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(P4-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(P4-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(P4-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(P4-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(P4-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(P4-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(P4-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(P4-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(P4-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(P4-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(P4-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(P4-Pad24)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x24_Pitch2.54mm.wrl
      (at (xyz 0 -1.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module PerfProto:Socket_Strip_Straight_1x24_Pitch2.54mm (layer F.Cu) (tedit 589B90CF)
    (at 125.73 72.39)
    (descr "Through hole straight socket strip, 1x24, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x24 2.54mm single row")
    (fp_text reference P6 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X24 (at 0 60.75) (layer F.Fab))
    (pad 3 thru_hole trapezoid (at 0 5.08 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(P6-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(P6-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(P6-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(P6-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(P6-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(P6-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P6-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P6-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P6-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P6-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(P6-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(P6-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(P6-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(P6-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(P6-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(P6-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(P6-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(P6-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(P6-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(P6-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(P6-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(P6-Pad24)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(P6-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(P6-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(P6-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(P6-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(P6-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(P6-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(P6-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(P6-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(P6-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(P6-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(P6-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(P6-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P6-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P6-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P6-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P6-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(P6-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(P6-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(P6-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(P6-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(P6-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(P6-Pad3)"))
    (pad 24 thru_hole trapezoid (at 0 58.42) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(P6-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(P6-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(P6-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(P6-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(P6-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(P6-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(P6-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(P6-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(P6-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(P6-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(P6-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(P6-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P6-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P6-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P6-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P6-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(P6-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(P6-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(P6-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(P6-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(P6-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(P6-Pad3)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(P6-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(P6-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(P6-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(P6-Pad2)"))
    (pad 1 thru_hole trapezoid (at 0 0) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(P6-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(P6-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(P6-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(P6-Pad1)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(P6-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(P6-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(P6-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(P6-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(P6-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(P6-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(P6-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(P6-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(P6-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(P6-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(P6-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(P6-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(P6-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(P6-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(P6-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(P6-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(P6-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(P6-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(P6-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(P6-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(P6-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(P6-Pad24)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x24_Pitch2.54mm.wrl
      (at (xyz 0 -1.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module PerfProto:Socket_Strip_Straight_1x24_Pitch2.54mm (layer F.Cu) (tedit 589B90CF)
    (at 128.27 72.39)
    (descr "Through hole straight socket strip, 1x24, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x24 2.54mm single row")
    (fp_text reference P7 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X24 (at 0 60.75) (layer F.Fab))
    (pad 3 thru_hole trapezoid (at 0 5.08 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(P7-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(P7-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(P7-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(P7-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(P7-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(P7-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(P7-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(P7-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(P7-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(P7-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(P7-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(P7-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(P7-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(P7-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(P7-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(P7-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(P7-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(P7-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(P7-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(P7-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(P7-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(P7-Pad24)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(P7-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(P7-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(P7-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(P7-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(P7-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(P7-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(P7-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(P7-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(P7-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(P7-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(P7-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(P7-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(P7-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(P7-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(P7-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(P7-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(P7-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(P7-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(P7-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(P7-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(P7-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(P7-Pad3)"))
    (pad 24 thru_hole trapezoid (at 0 58.42) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(P7-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(P7-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(P7-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(P7-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(P7-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(P7-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(P7-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(P7-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(P7-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(P7-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(P7-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(P7-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(P7-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(P7-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(P7-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(P7-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(P7-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(P7-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(P7-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(P7-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(P7-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(P7-Pad3)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(P7-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(P7-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(P7-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(P7-Pad2)"))
    (pad 1 thru_hole trapezoid (at 0 0) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(P7-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(P7-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(P7-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(P7-Pad1)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(P7-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(P7-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(P7-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(P7-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(P7-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(P7-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(P7-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(P7-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(P7-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(P7-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(P7-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(P7-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(P7-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(P7-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(P7-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(P7-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(P7-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(P7-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(P7-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(P7-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(P7-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(P7-Pad24)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x24_Pitch2.54mm.wrl
      (at (xyz 0 -1.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module PerfProto:Socket_Strip_Straight_1x24_Pitch2.54mm (layer F.Cu) (tedit 589B90CF)
    (at 130.81 72.39)
    (descr "Through hole straight socket strip, 1x24, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x24 2.54mm single row")
    (fp_text reference P8 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X24 (at 0 60.75) (layer F.Fab))
    (pad 3 thru_hole trapezoid (at 0 5.08 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(P8-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(P8-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(P8-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(P8-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(P8-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(P8-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(P8-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(P8-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(P8-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(P8-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(P8-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(P8-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(P8-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(P8-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(P8-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(P8-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(P8-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(P8-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(P8-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(P8-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 152 "Net-(P8-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 153 "Net-(P8-Pad24)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 153 "Net-(P8-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 152 "Net-(P8-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(P8-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(P8-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(P8-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(P8-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(P8-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(P8-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(P8-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(P8-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(P8-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(P8-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(P8-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(P8-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(P8-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(P8-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(P8-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(P8-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(P8-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(P8-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(P8-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(P8-Pad3)"))
    (pad 24 thru_hole trapezoid (at 0 58.42) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 153 "Net-(P8-Pad24)"))
    (pad 23 thru_hole trapezoid (at 0 55.88) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 152 "Net-(P8-Pad23)"))
    (pad 22 thru_hole trapezoid (at 0 53.34) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(P8-Pad22)"))
    (pad 21 thru_hole trapezoid (at 0 50.8) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(P8-Pad21)"))
    (pad 20 thru_hole trapezoid (at 0 48.26) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(P8-Pad20)"))
    (pad 19 thru_hole trapezoid (at 0 45.72) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(P8-Pad19)"))
    (pad 18 thru_hole trapezoid (at 0 43.18) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(P8-Pad18)"))
    (pad 17 thru_hole trapezoid (at 0 40.64) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(P8-Pad17)"))
    (pad 16 thru_hole trapezoid (at 0 38.1) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(P8-Pad16)"))
    (pad 15 thru_hole trapezoid (at 0 35.56) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(P8-Pad15)"))
    (pad 14 thru_hole trapezoid (at 0 33.02) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(P8-Pad14)"))
    (pad 13 thru_hole trapezoid (at 0 30.48) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(P8-Pad13)"))
    (pad 12 thru_hole trapezoid (at 0 27.94) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(P8-Pad12)"))
    (pad 11 thru_hole trapezoid (at 0 25.4) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(P8-Pad11)"))
    (pad 10 thru_hole trapezoid (at 0 22.86) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(P8-Pad10)"))
    (pad 9 thru_hole trapezoid (at 0 20.32) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(P8-Pad9)"))
    (pad 8 thru_hole trapezoid (at 0 17.78) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(P8-Pad8)"))
    (pad 7 thru_hole trapezoid (at 0 15.24) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(P8-Pad7)"))
    (pad 6 thru_hole trapezoid (at 0 12.7) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(P8-Pad6)"))
    (pad 5 thru_hole trapezoid (at 0 10.16) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(P8-Pad5)"))
    (pad 4 thru_hole trapezoid (at 0 7.62) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(P8-Pad4)"))
    (pad 3 thru_hole trapezoid (at 0 5.08) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(P8-Pad3)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(P8-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(P8-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(P8-Pad2)"))
    (pad 2 thru_hole trapezoid (at 0 2.54) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(P8-Pad2)"))
    (pad 1 thru_hole trapezoid (at 0 0) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(P8-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 180) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(P8-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 90) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(P8-Pad1)"))
    (pad 1 thru_hole trapezoid (at 0 0 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(P8-Pad1)"))
    (pad 3 thru_hole trapezoid (at 0 5.08 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(P8-Pad3)"))
    (pad 4 thru_hole trapezoid (at 0 7.62 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(P8-Pad4)"))
    (pad 5 thru_hole trapezoid (at 0 10.16 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(P8-Pad5)"))
    (pad 6 thru_hole trapezoid (at 0 12.7 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(P8-Pad6)"))
    (pad 7 thru_hole trapezoid (at 0 15.24 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(P8-Pad7)"))
    (pad 8 thru_hole trapezoid (at 0 17.78 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(P8-Pad8)"))
    (pad 9 thru_hole trapezoid (at 0 20.32 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(P8-Pad9)"))
    (pad 10 thru_hole trapezoid (at 0 22.86 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(P8-Pad10)"))
    (pad 11 thru_hole trapezoid (at 0 25.4 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(P8-Pad11)"))
    (pad 12 thru_hole trapezoid (at 0 27.94 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(P8-Pad12)"))
    (pad 13 thru_hole trapezoid (at 0 30.48 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(P8-Pad13)"))
    (pad 14 thru_hole trapezoid (at 0 33.02 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(P8-Pad14)"))
    (pad 15 thru_hole trapezoid (at 0 35.56 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(P8-Pad15)"))
    (pad 16 thru_hole trapezoid (at 0 38.1 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(P8-Pad16)"))
    (pad 17 thru_hole trapezoid (at 0 40.64 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(P8-Pad17)"))
    (pad 18 thru_hole trapezoid (at 0 43.18 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(P8-Pad18)"))
    (pad 19 thru_hole trapezoid (at 0 45.72 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(P8-Pad19)"))
    (pad 20 thru_hole trapezoid (at 0 48.26 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(P8-Pad20)"))
    (pad 21 thru_hole trapezoid (at 0 50.8 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(P8-Pad21)"))
    (pad 22 thru_hole trapezoid (at 0 53.34 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(P8-Pad22)"))
    (pad 23 thru_hole trapezoid (at 0 55.88 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 152 "Net-(P8-Pad23)"))
    (pad 24 thru_hole trapezoid (at 0 58.42 270) (size 1.016 2.286) (rect_delta 0 0.508 ) (drill 1) (layers *.Cu *.Mask)
      (net 153 "Net-(P8-Pad24)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x24_Pitch2.54mm.wrl
      (at (xyz 0 -1.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_line (start 95.25 72.39) (end 95.25 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 69.85) (end 137.16 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 130.81) (end 139.7 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 133.35) (end 137.16 133.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.79 130.81) (end 97.79 133.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.16 130.81) (end 139.7 130.81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 63.5 (width 0.3) (layer Cmts.User)
    (gr_text "2.5000 in" (at 144.86 101.6 270) (layer Cmts.User))
    (feature1 (pts (xy 138.43 133.35) (xy 146.21 133.35)))
    (feature2 (pts (xy 138.43 69.85) (xy 146.21 69.85)))
    (crossbar (pts (xy 143.51 69.85) (xy 143.51 133.35)))
    (arrow1a (pts (xy 143.51 133.35) (xy 142.923579 132.223496)))
    (arrow1b (pts (xy 143.51 133.35) (xy 144.096421 132.223496)))
    (arrow2a (pts (xy 143.51 69.85) (xy 142.923579 70.976504)))
    (arrow2b (pts (xy 143.51 69.85) (xy 144.096421 70.976504)))
  )
  (dimension 44.45 (width 0.3) (layer Cmts.User)
    (gr_text "1.7500 in" (at 117.475 63.42) (layer Cmts.User))
    (feature1 (pts (xy 139.7 71.12) (xy 139.7 62.07)))
    (feature2 (pts (xy 95.25 71.12) (xy 95.25 62.07)))
    (crossbar (pts (xy 95.25 64.77) (xy 139.7 64.77)))
    (arrow1a (pts (xy 139.7 64.77) (xy 138.573496 65.356421)))
    (arrow1b (pts (xy 139.7 64.77) (xy 138.573496 64.183579)))
    (arrow2a (pts (xy 95.25 64.77) (xy 96.376504 65.356421)))
    (arrow2b (pts (xy 95.25 64.77) (xy 96.376504 64.183579)))
  )
  (gr_arc (start 137.16 72.39) (end 137.16 69.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.79 72.39) (end 95.25 72.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 117.094) (xy 97.028 117.094) (xy 97.028 121.158) (xy 97.028 121.412) (xy 97.028 121.666)
        (xy 106.426 121.666)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 117.094) (xy 97.028 117.094) (xy 97.028 121.158) (xy 97.028 121.412) (xy 97.028 121.666)
        (xy 106.426 121.666)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 112.014) (xy 97.028 112.014) (xy 97.028 116.078) (xy 97.028 116.332) (xy 97.028 116.586)
        (xy 106.426 116.586)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 112.014) (xy 97.028 112.014) (xy 97.028 116.078) (xy 97.028 116.332) (xy 97.028 116.586)
        (xy 106.426 116.586)
      )
    )
  )
  (zone (net 81) (net_name "Net-(P5-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 123.19 70.612) (xy 118.11 70.612) (xy 118.11 132.588) (xy 123.19 132.588)
      )
    )
  )
  (zone (net 81) (net_name "Net-(P5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 123.19 70.612) (xy 118.11 70.612) (xy 118.11 132.588) (xy 123.19 132.588)
      )
    )
  )
  (zone (net 154) (net_name "Net-(P9-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 133.35 125.222) (xy 138.43 125.222) (xy 138.43 77.978) (xy 133.35 77.978)
      )
    )
  )
  (zone (net 154) (net_name "Net-(P9-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 133.35 125.222) (xy 138.43 125.222) (xy 138.43 77.978) (xy 133.35 77.978)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pad3)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 111.506) (xy 106.426 106.934) (xy 97.028 106.934) (xy 97.028 111.506)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pad3)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 111.506) (xy 106.426 106.934) (xy 97.028 106.934) (xy 97.028 111.506)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 106.426) (xy 106.426 106.426) (xy 106.426 101.854) (xy 97.028 101.854)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad5)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 101.346) (xy 106.426 101.346) (xy 106.426 96.774) (xy 97.028 96.774)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad6)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 96.266) (xy 106.426 96.266) (xy 106.426 91.694) (xy 97.028 91.694)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pad7)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 91.186) (xy 106.426 91.186) (xy 106.426 86.614) (xy 97.028 86.614)
      )
    )
  )
  (zone (net 8) (net_name "Net-(J1-Pad8)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 86.106) (xy 106.426 81.534) (xy 97.028 81.534) (xy 97.028 86.106)
      )
    )
  )
  (zone (net 8) (net_name "Net-(J1-Pad8)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 106.426 86.106) (xy 106.426 81.534) (xy 97.028 81.534) (xy 97.028 86.106)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pad7)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 91.186) (xy 106.426 91.186) (xy 106.426 86.614) (xy 97.028 86.614)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad6)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 96.266) (xy 106.426 96.266) (xy 106.426 91.694) (xy 97.028 91.694)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad5)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 101.346) (xy 106.426 101.346) (xy 106.426 96.774) (xy 97.028 96.774)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 97.028 106.426) (xy 106.426 106.426) (xy 106.426 101.854) (xy 97.028 101.854)
      )
    )
  )
)
