(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 61)
    (zones 0)
    (modules 8)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /nRESET)
  (net 2 /GND)
  (net 3 "Net-(J1-Pad8)")
  (net 4 "Net-(J1-Pad7)")
  (net 5 /SWO)
  (net 6 /SWDCLK)
  (net 7 /SWDIO)
  (net 8 /VTREF)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /VTREF)
    (add_net /nRESET)
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 144.78 99.06)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference J1 (at 1.778 -1.778) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0.635 6.775) (layer F.Fab))
    (fp_text user %R (at 0.635 2.54 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 1.27 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 /nRESET))
    (pad 9 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 8 thru_hole oval (at 1.27 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 1.27 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 /SWO))
    (pad 5 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 4 thru_hole oval (at 1.27 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /SWDCLK))
    (pad 3 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 /SWDIO))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /VTREF))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 127 99.06)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 2.286 -2.54) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /nRESET))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SWO))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SWDIO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SWDCLK))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VTREF))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 139.7 105.41)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value TestPoint_Probe (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 /GND))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 105.41)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP5 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value TestPoint_Probe (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /nRESET))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 97.79)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.778) (layer F.SilkS) hide)
    (fp_text value TestPoint_Probe (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /VTREF))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 139.7 101.6)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP3 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value TestPoint_Probe (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SWO))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 139.7 97.79)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value TestPoint_Probe (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SWDCLK))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 101.6)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value TestPoint_Probe (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SWDIO))
  )
  (gr_arc (start 147.955 95.885) (end 148.59 95.885) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.59 107.315) (end 148.59 107.188) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 147.955 107.315) (end 147.955 107.95) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.59 95.885) (end 148.59 107.188) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.955 107.95) (end 125.095 107.95) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 125.095 107.315) (end 124.46 107.315) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 125.095 95.885) (end 125.095 95.25) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.46 95.885) (end 124.46 107.315) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.095 95.25) (end 147.955 95.25) (layer Edge.Cuts) (width 0.05))
  (gr_text "Sid Price\n2020" (at 145.288 96.774) (layer B.SilkS))
  (gr_text JLINK (at 145.288 106.426) (layer F.SilkS))
  (gr_text EDT (at 128.524 106.426) (layer F.SilkS))
  (gr_text 1 (at 144.018 97.282) (layer F.SilkS))
  (gr_text 1 (at 125.984 96.52) (layer F.SilkS))
  (gr_text GND (at 139.7 103.632) (layer F.SilkS))
  (gr_text nRESET (at 134.874 103.632) (layer F.SilkS))
  (gr_text SWO (at 139.7 99.822) (layer F.SilkS))
  (gr_text SWDIO (at 134.874 99.822) (layer F.SilkS))
  (gr_text SWDCLK (at 139.7 96.012) (layer F.SilkS))
  (gr_text VTREF (at 134.62 96.012) (layer F.SilkS))
  (dimension 12.7 (width 0.15) (layer Dwgs.User)
    (gr_text "0.5000 in" (at 154.97 101.6 270) (layer Dwgs.User))
    (feature1 (pts (xy 148.59 107.95) (xy 154.256421 107.95)))
    (feature2 (pts (xy 148.59 95.25) (xy 154.256421 95.25)))
    (crossbar (pts (xy 153.67 95.25) (xy 153.67 107.95)))
    (arrow1a (pts (xy 153.67 107.95) (xy 153.083579 106.823496)))
    (arrow1b (pts (xy 153.67 107.95) (xy 154.256421 106.823496)))
    (arrow2a (pts (xy 153.67 95.25) (xy 153.083579 96.376504)))
    (arrow2b (pts (xy 153.67 95.25) (xy 154.256421 96.376504)))
  )
  (dimension 24.13 (width 0.15) (layer Dwgs.User)
    (gr_text "0.9500 in" (at 136.525 90.14) (layer Dwgs.User))
    (feature1 (pts (xy 148.59 95.25) (xy 148.59 90.853579)))
    (feature2 (pts (xy 124.46 95.25) (xy 124.46 90.853579)))
    (crossbar (pts (xy 124.46 91.44) (xy 148.59 91.44)))
    (arrow1a (pts (xy 148.59 91.44) (xy 147.463496 92.026421)))
    (arrow1b (pts (xy 148.59 91.44) (xy 147.463496 90.853579)))
    (arrow2a (pts (xy 124.46 91.44) (xy 125.586504 92.026421)))
    (arrow2b (pts (xy 124.46 91.44) (xy 125.586504 90.853579)))
  )
  (zone (net 2) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 147.955 107.315) (xy 125.095 107.315) (xy 125.095 95.885) (xy 147.955 95.885)
      )
    )
  )
)
