(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "d25M Tally Output Adapter board")
		(date "2022-06-14")
		(rev "20220514-1")
		(company "Chibi Circuitz")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Pin1")
	(net 3 "Pin2")
	(net 4 "Pin4")
	(net 5 "Pin10")
	(net 6 "Pin9")
	(net 7 "Pin7")
	(net 8 "Pin13")
	(net 9 "Pin6")
	(net 10 "Pin11")
	(net 11 "Pin3")
	(net 12 "Pin8")
	(net 13 "Pin12")
	(net 14 "Pin5")
	(net 15 "Pin15")
	(net 16 "Pin18")
	(net 17 "Pin24")
	(net 18 "Pin19")
	(net 19 "Pin20")
	(net 20 "Pin17")
	(net 21 "Pin16")
	(net 22 "Pin25")
	(net 23 "Pin21")
	(net 24 "Pin23")
	(net 25 "Pin14")
	(net 26 "Pin22")
	(footprint "test:OSHW-Logo2"
		(layer "F.Cu")
		(at 104.013 117.602)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "LOGO2"
			(at -0.00762 3.02768 0)
			(layer "Eco1.User")
			(hide yes)
		)
		(property "Value" "Logo_Open_Hardware_Small"
			(at 0 1.475 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "test:OSHW-Logo2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Tally25-20240704.kicad_sch")
		(attr exclude_from_pos_files)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-13-3.5-H_1x13_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 148.026 105.283 180)
		(descr "Terminal Block Phoenix PT-1,5-13-3.5-H, 13 pins, pitch 3.5mm, size 45.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix PT-1,5-13-3.5-H pitch 3.5mm size 45.5x7.6mm^2 drill 1.2mm pad 2.4mm")
		(property "Reference" "J1"
			(at 19.248 2.286 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "pims 1-13"
			(at 11.755 2.286 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-13-3.5-H_1x13_P3.50mm_Horizontal"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Tally25-20240704.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.945 -2.413 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Pin1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Pin2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 7 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Pin3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 10.5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Pin4")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 14 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Pin5")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 17.5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Pin6")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 21 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Pin7")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 24.5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Pin8")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 28 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Pin9")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 31.5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Pin10")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 35 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Pin11")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 38.5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Pin12")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 42 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Pin13")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(model "/home/doug/Documents/KiCad/library/3d/PT_1-5-13-Body.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.394 0.394 0.394)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-12-3.5-H_1x12_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 109.5 117.729)
		(descr "Terminal Block Phoenix PT-1,5-12-3.5-H, 12 pins, pitch 3.5mm, size 42x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix PT-1,5-12-3.5-H pitch 3.5mm size 42x7.6mm^2 drill 1.2mm pad 2.4mm")
		(property "Reference" "J3"
			(at 39.344 -2.286 0)
			(layer "F.SilkS")
		)
		(property "Value" "pins 14-25"
			(at 25.882 2.286 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-12-3.5-H_1x12_P3.50mm_Horizontal"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Tally25-20240704.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 19.25 2.4 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Pin25")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Pin24")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 7 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Pin23")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 10.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Pin22")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 14 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Pin21")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 17.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Pin20")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 21 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Pin19")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 24.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Pin18")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 28 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Pin17")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 31.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Pin16")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 35 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Pin15")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 38.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Pin14")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(model "/home/doug/Documents/KiCad/library/3d/PT_1-5-12-Body.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.394 0.394 0.394)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles"
		(layer "B.Cu")
		(at 143.9 110.1 180)
		(descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
		(property "Reference" "J2"
			(at -2.912 -3.565 0)
			(layer "B.SilkS")
		)
		(property "Value" "DB25_Male_MountingHoles"
			(at 16.62 -8.73 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_Dsub:DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Male*")
		(sheetname "Root")
		(sheetfile "Tally25-20240704.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 16.62 -1.42 0)
			(layer "B.Fab")
		)
		(pad "0" thru_hole circle
			(at -6.93 -1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 40.17 -1.42 180)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Pin1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.77 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Pin2")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.54 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Pin3")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 8.31 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Pin4")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 11.08 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Pin5")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 13.85 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Pin6")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 16.62 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Pin7")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 19.39 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Pin8")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 22.16 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Pin9")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 24.93 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Pin10")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 27.7 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Pin11")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 30.47 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Pin12")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 33.24 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Pin13")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 1.385 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Pin14")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 4.155 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Pin15")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 6.925 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Pin16")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 9.695 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Pin17")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 12.465 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Pin18")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 15.235 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Pin19")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 18.005 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Pin20")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 20.775 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Pin21")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 23.545 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Pin22")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 26.315 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Pin23")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 29.085 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Pin24")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 31.855 -2.84 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Pin25")
			(pinfunction "P25")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Male_Vertical_P2.77x2.84mm_MountingHoles.wrl"
			(offset
				(xyz 0 0 1.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "test:OSHW-Logo2"
		(layer "B.Cu")
		(at 104.521 117.729 180)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "LOGO1"
			(at -0.00762 -3.02768 0)
			(layer "Eco1.User")
			(hide yes)
		)
		(property "Value" "Logo_Open_Hardware_Small"
			(at 0 -1.475 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "test:OSHW-Logo2"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Tally25-20240704.kicad_sch")
		(attr exclude_from_pos_files)
	)
	(gr_line
		(start 150 100.5)
		(end 104.5 100.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 100 105)
		(mid 101.318019 101.818019)
		(end 104.5 100.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 150 100.5)
		(mid 153.181981 101.818019)
		(end 154.5 105)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 154.5 118)
		(mid 153.181981 121.181981)
		(end 150 122.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100 105)
		(end 100 118)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.5 122.5)
		(mid 101.318019 121.181981)
		(end 100 118)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.5 122.5)
		(end 150 122.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.5 118)
		(end 154.5 105)
		(layer "Edge.Cuts")
	)
	(gr_text "d25M Tally Output Adapter v20220614-1\nDesigned by Chibi Circuitz   chibicircuitz.com/tally"
		(at 128.397 121 0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 146.812 109.855 0)
		(layer "F.SilkS")
	)
	(gr_text "d25M"
		(at 101.981 105.029 90)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 154.432 103.378) (xy 154.178 120.523) (xy 151.13 122.682) (xy 103.251 122.428) (xy 100.076 119.253)
				(xy 99.949 102.743) (xy 102.743 100.457) (xy 151.638 100.457)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 154.432 103.124) (xy 154.305 120.015) (xy 151.638 122.428) (xy 102.743 122.428) (xy 100 119.888)
				(xy 100.076 103.886) (xy 103.378 100.457) (xy 152.019 100.584)
			)
		)
	)
)
