<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="48.26" y1="22.86" x2="119.995" y2="22.86" width="0" layer="20"/>
<wire x1="119.995" y1="22.86" x2="119.995" y2="79.045" width="0" layer="20"/>
<wire x1="119.995" y1="79.045" x2="48.26" y2="79.045" width="0" layer="20"/>
<wire x1="48.26" y1="79.045" x2="48.26" y2="22.86" width="0" layer="20"/>
</plain>
<libraries>
<library name="Resistor">
<description>&lt;B&gt;Resistors, Potentiometers, TrimPot</description>
<packages>
<package name="RESAD724W46L381D178B">
<description>Axial Resistor, 7.24 mm pitch, 3.81 mm body length, 1.78 mm body diameter
&lt;p&gt;Axial Resistor package with 7.24 mm pitch (lead spacing), 0.46 mm lead diameter, 3.81 mm body length and 1.78 mm body diameter&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="ARDUINOR3-BPLACE">
</package>
</packages>
</library>
<library name="AM2315A">
<packages>
<package name="AM2315A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="Resistor" package="RESAD724W46L381D178B" value="10Kohm">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Resistor" package="RESAD724W46L381D178B" value="10Kohm">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="adafruit" package="ARDUINOR3-BPLACE" value="ARDUINOR3-BPLACE"/>
<element name="U$1" library="AM2315A" package="AM2315A" value="AM2315D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="GND"/>
<contactref element="U1" pad="GND2"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U1" pad="GND1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="SCL"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="SDA"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="5V"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="3V"/>
</signal>
<signal name="+9V">
<contactref element="U1" pad="VIN"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
