(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 32)
    (zones 0)
    (modules 7)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 /GPIO_17)
  (net 5 /GPIO27)
  (net 6 GND)
  (net 7 /SDA)
  (net 8 /SCL)
  (net 9 /TX_LED)
  (net 10 "Net-(J2-Pad15)")
  (net 11 "Net-(J2-Pad16)")
  (net 12 /OE)
  (net 13 /V_servo)
  (net 14 "Net-(J2-Pad13)")
  (net 15 "Net-(J2-Pad11)")
  (net 16 "Net-(J2-Pad9)")
  (net 17 "Net-(J2-Pad8)")
  (net 18 "Net-(J2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /GPIO27)
    (add_net /GPIO_17)
    (add_net /OE)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX_LED)
    (add_net /V_servo)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )
  (module LED_SMD:LED_0603_1608Metric_Castellated (layer F.Cu) (tedit 5B301BBE)
    (at 149.098 109.22 180)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (attr smd)
    (fp_text reference D1 (at -0.762 1.524) (layer F.SilkS))
    (fp_text value "5V ok" (at 0 1.38 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8125 0 180) (size 1.225 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.8125 0 180) (size 1.225 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x08_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A42B)
    (at 149.86 87.63 180)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (fp_text reference J2 (at 2.54 -18.6055 180) (layer B.SilkS))
    (fp_text value SH2-16G (at -1.27 -20.55 180) (layer B.Fab))
    (fp_text user %R (at -1.27 -8.89 90) (layer B.Fab))
    (pad 16 thru_hole oval (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIO27))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /GPIO_17))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /TX_LED))
    (pad 6 thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SCL))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 4 thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SDA))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module molex_SL:molex_sl_1X6_right_th (layer F.Cu) (tedit 5CD460E6)
    (at 144.78 96.52 270)
    (fp_text reference J4 (at 8.89 -2.794 90) (layer F.SilkS))
    (fp_text value "Molex SL 1X6 right TH" (at -2.54 -6.35 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.75 8.64 270) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.75 8.64 270) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 6.35 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 5 thru_hole circle (at 3.81 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 12 /OE))
    (pad 4 thru_hole circle (at 1.27 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 /SCL))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 7 /SDA))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole circle (at -6.35 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 13 /V_servo))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 152.654 109.22 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.762 1.524) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 147.6248 94.7674 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.5146 0.0508 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 147.6248 90.6525 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.5146 -0.0508 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module molex_SL:molex_sl_1X2_right_th (layer F.Cu) (tedit 5CD4609F)
    (at 144.78 111.76 270)
    (fp_text reference J3 (at -4.064 -2.794 270) (layer F.SilkS))
    (fp_text value "Molex SL 1X2 right TH" (at 0 -3.175 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.54 8.64 270) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 8.64 270) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.79 1.79) (drill 1.09) (layers *.Cu *.Mask)
      (net 9 /TX_LED))
  )
  (gr_text "rev 1.0" (at 151.3205 115.062) (layer B.SilkS))
  (gr_text "molex \nthis side" (at 139.954 111.76 90) (layer F.SilkS))
  (gr_text "Place PI \nheader on\nthis side" (at 153.924 109.474) (layer B.SilkS))
  (gr_text +5Vout (at 140.97 90.17) (layer B.SilkS))
  (gr_text "+3.3V " (at 140.97 92.71) (layer B.SilkS))
  (gr_text SDA (at 142.24 95.25) (layer B.SilkS))
  (gr_text SCL (at 142.24 97.79) (layer B.SilkS))
  (gr_text OE (at 142.24 100.33) (layer B.SilkS))
  (gr_text GND (at 142.24 102.87) (layer B.SilkS))
  (gr_text GND (at 142.24 113.03) (layer B.SilkS))
  (gr_text "TX LED" (at 140.97 110.49) (layer B.SilkS))
  (gr_text "ARM* PI \nbreakout" (at 148.336 87.376) (layer B.SilkS))
  (gr_text "PWR ON" (at 150.876 110.744) (layer F.SilkS))
  (gr_text "molex \nthis side" (at 139.954 96.266 90) (layer F.SilkS))
  (gr_text "ARM*\nSSPD" (at 150.876 113.792) (layer F.SilkS))
  (gr_arc (start 134.62 115.57) (end 134.62 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.62 86.36) (end 134.62 85.09) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.67 86.36) (end 154.94 86.36) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.67 115.57) (end 153.67 116.84) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.62 116.84) (end 153.67 116.84) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.35 86.36) (end 133.35 115.57) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.67 85.09) (end 134.62 85.09) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.94 115.57) (end 154.94 86.36) (layer Edge.Cuts) (width 0.2))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 85.09) (xy 133.35 116.84) (xy 154.94 116.84) (xy 154.94 85.09)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.94 106.045) (xy 133.35 106.045) (xy 133.35 85.09) (xy 154.94 85.09)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 107.315) (xy 133.35 116.84) (xy 154.94 116.84) (xy 154.94 107.315)
      )
    )
  )
)
