(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 954)
    (zones 0)
    (modules 60)
    (nets 63)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4572 0.3048)
    (user_via 0.5588 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.302 3.302)
    (pad_drill 3.302)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BT1-Pad1)")
  (net 3 VCC)
  (net 4 +5V)
  (net 5 "Net-(C6-Pad1)")
  (net 6 /XTAL2)
  (net 7 /XTAL1)
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C19-Pad2)")
  (net 10 "Net-(C20-Pad2)")
  (net 11 "Net-(C21-Pad1)")
  (net 12 "Net-(C22-Pad1)")
  (net 13 /DC_SENSE)
  (net 14 /POWER_LED)
  (net 15 "Net-(D2-Pad1)")
  (net 16 "Net-(D3-Pad2)")
  (net 17 "Net-(D3-Pad1)")
  (net 18 "Net-(D4-Pad2)")
  (net 19 "Net-(D4-Pad1)")
  (net 20 "Net-(D5-Pad2)")
  (net 21 "Net-(D5-Pad1)")
  (net 22 "Net-(D6-Pad2)")
  (net 23 "Net-(D6-Pad1)")
  (net 24 "Net-(D7-Pad2)")
  (net 25 "Net-(D7-Pad1)")
  (net 26 "Net-(D8-Pad2)")
  (net 27 "Net-(D8-Pad1)")
  (net 28 "Net-(IC1-Pad4)")
  (net 29 /MUX_STAT)
  (net 30 "Net-(IC3-Pad5)")
  (net 31 /CHARGE_STAT)
  (net 32 /SW_POWER)
  (net 33 "Net-(IC4-Pad3)")
  (net 34 "Net-(IC5-Pad24)")
  (net 35 "Net-(IC5-Pad23)")
  (net 36 /RA_PWR)
  (net 37 "Net-(IC5-Pad19)")
  (net 38 /RA_DIR)
  (net 39 /RA_STEP)
  (net 40 "Net-(IC5-Pad7)")
  (net 41 "Net-(IC5-Pad5)")
  (net 42 "Net-(IC5-Pad2)")
  (net 43 "Net-(IC6-Pad24)")
  (net 44 "Net-(IC6-Pad23)")
  (net 45 /DEC_PWR)
  (net 46 "Net-(IC6-Pad19)")
  (net 47 /DEC_DIR)
  (net 48 /DEC_STEP)
  (net 49 "Net-(IC6-Pad7)")
  (net 50 "Net-(IC6-Pad5)")
  (net 51 "Net-(IC6-Pad2)")
  (net 52 /JS_DEC)
  (net 53 /ST4_RA-)
  (net 54 /ST4_DEC-)
  (net 55 /ST4_DEC+)
  (net 56 /ST4_RA+)
  (net 57 /JS_RA)
  (net 58 /RST)
  (net 59 /GUIDE_RATE)
  (net 60 /TRACK_RATE)
  (net 61 /DIP1)
  (net 62 /DIP2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /CHARGE_STAT)
    (add_net /DC_SENSE)
    (add_net /DEC_DIR)
    (add_net /DEC_PWR)
    (add_net /DEC_STEP)
    (add_net /DIP1)
    (add_net /DIP2)
    (add_net /GUIDE_RATE)
    (add_net /JS_DEC)
    (add_net /JS_RA)
    (add_net /MUX_STAT)
    (add_net /POWER_LED)
    (add_net /RA_DIR)
    (add_net /RA_PWR)
    (add_net /RA_STEP)
    (add_net /RST)
    (add_net /ST4_DEC+)
    (add_net /ST4_DEC-)
    (add_net /ST4_RA+)
    (add_net /ST4_RA-)
    (add_net /SW_POWER)
    (add_net /TRACK_RATE)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC3-Pad5)")
    (add_net "Net-(IC4-Pad3)")
    (add_net "Net-(IC5-Pad19)")
    (add_net "Net-(IC5-Pad2)")
    (add_net "Net-(IC5-Pad23)")
    (add_net "Net-(IC5-Pad24)")
    (add_net "Net-(IC5-Pad5)")
    (add_net "Net-(IC5-Pad7)")
    (add_net "Net-(IC6-Pad19)")
    (add_net "Net-(IC6-Pad2)")
    (add_net "Net-(IC6-Pad23)")
    (add_net "Net-(IC6-Pad24)")
    (add_net "Net-(IC6-Pad5)")
    (add_net "Net-(IC6-Pad7)")
    (add_net VCC)
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 125.222 72.644 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 146.812 88.392)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 470Ω (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.496 88.392)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 470Ω (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 141.161 73.406)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 47KΩ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(IC6-Pad24)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 151.7885 73.406)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 47KΩ (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(IC5-Pad24)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 177.546 82.110099 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.608099 0 90) (layer F.SilkS))
    (fp_text value 4.7KΩ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /TRACK_RATE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 175.617501 82.110099 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.608099 -0.103501 90) (layer F.SilkS))
    (fp_text value 4.7KΩ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /TRACK_RATE))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 192.786 64.77)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 1.016 1.27) (layer F.SilkS))
    (fp_text value 2Ω (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(IC3-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 109.474 84.836 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1KΩ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D2-Pad1)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 183.388 63.9045 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 4.7KΩ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /SW_POWER))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 185.42 60.452 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -3.302 90) (layer F.SilkS))
    (fp_text value 4.7KΩ (at 0 1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /CHARGE_STAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 183.388 60.452 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -3.302 90) (layer F.SilkS))
    (fp_text value 4.7KΩ (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /CHARGE_STAT))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 187.452 69.088)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 470Ω (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(IC1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 113.284 82.296 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Prog (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /RST))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /ST4_DEC+))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /ST4_RA-))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /ST4_DEC-))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 127.762 68.242 90)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 2.794 90) (layer F.SilkS))
    (fp_text value "16 MHz" (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 -0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /XTAL2))
    (pad 2 smd rect (at 1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0.85 90) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /XTAL1))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1008_2520Metric (layer F.Cu) (tedit 5F68FEF0)
    (at 181.043 68.072)
    (descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0 -2.05) (layer F.SilkS))
    (fp_text value 2.2µH (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.075 0) (size 1.25 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1.075 0) (size 1.25 2.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(IC4-Pad3)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 191.262 73.914)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 9.398 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 112.014 69.85)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -8.89 -5.334) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 148.59 77.758 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at 2.76 0 90) (layer F.SilkS))
    (fp_text value D_TVS (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 160.274 77.724 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D_TVS (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 139.7 77.758 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D_TVS (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 152.4 77.724 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value D_TVS (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 143.7385 88.392)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D4 (at 0 -1.43) (layer F.SilkS))
    (fp_text value ERR_DEC (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 155.448 88.392)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value ERR_RA (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 109.474 81.788 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value POWER (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /POWER_LED))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer B.Cu) (tedit 5AE50EF0)
    (at 180.086 82.042 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 4.4 90) (layer B.SilkS))
    (fp_text value 47µF (at 1.25 -4.4 90) (layer B.Fab))
    (fp_text user %R (at 1.25 0 90) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm (layer F.Cu) (tedit 5DC5F6A4)
    (at 120.65 69.088 180)
    (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/8008S.pdf#page=16), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U1 (at 0 -3.3) (layer F.SilkS))
    (fp_text value ATmega328P-MMH (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd custom (at -1.95 -1.35 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 38 /RA_DIR)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 -0.0625) (xy 0.274112 -0.0625) (xy 0.3375 0.000888) (xy 0.3375 0.0625) (xy -0.3375 0.0625)
) (width 0.125))
      ))
    (pad 2 smd roundrect (at -1.95 -0.9 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /RA_PWR))
    (pad 3 smd roundrect (at -1.95 -0.45 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 4 smd roundrect (at -1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at -1.95 0.45 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /XTAL1))
    (pad 6 smd roundrect (at -1.95 0.9 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /XTAL2))
    (pad 7 smd custom (at -1.95 1.35 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 48 /DEC_STEP)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 -0.0625) (xy 0.3375 -0.0625) (xy 0.3375 -0.000888) (xy 0.274112 0.0625) (xy -0.3375 0.0625)
) (width 0.125))
      ))
    (pad 8 smd custom (at -1.35 1.95 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 47 /DEC_DIR)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.0625 -0.274112) (xy 0.000888 -0.3375) (xy 0.0625 -0.3375) (xy 0.0625 0.3375) (xy -0.0625 0.3375)
) (width 0.125))
      ))
    (pad 9 smd roundrect (at -0.9 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /DEC_PWR))
    (pad 10 smd roundrect (at -0.45 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /MUX_STAT))
    (pad 11 smd roundrect (at 0 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /POWER_LED))
    (pad 12 smd roundrect (at 0.45 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /ST4_RA+))
    (pad 13 smd roundrect (at 0.9 1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /ST4_DEC+))
    (pad 14 smd custom (at 1.35 1.95 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 54 /ST4_DEC-)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.0625 -0.3375) (xy -0.000888 -0.3375) (xy 0.0625 -0.274112) (xy 0.0625 0.3375) (xy -0.0625 0.3375)
) (width 0.125))
      ))
    (pad 15 smd custom (at 1.95 1.35 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 53 /ST4_RA-)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 -0.0625) (xy 0.3375 -0.0625) (xy 0.3375 0.0625) (xy -0.274112 0.0625) (xy -0.3375 -0.000888)
) (width 0.125))
      ))
    (pad 16 smd roundrect (at 1.95 0.9 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 17 smd roundrect (at 1.95 0.45 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 18 smd roundrect (at 1.95 0 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 19 smd roundrect (at 1.95 -0.45 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /JS_RA))
    (pad 20 smd roundrect (at 1.95 -0.9 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /JS_DEC))
    (pad 21 smd custom (at 1.95 -1.35 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 60 /TRACK_RATE)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 0.000888) (xy -0.274112 -0.0625) (xy 0.3375 -0.0625) (xy 0.3375 0.0625) (xy -0.3375 0.0625)
) (width 0.125))
      ))
    (pad 22 smd custom (at 1.35 -1.95 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 59 /GUIDE_RATE)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.0625 -0.3375) (xy 0.0625 -0.3375) (xy 0.0625 0.274112) (xy -0.000888 0.3375) (xy -0.0625 0.3375)
) (width 0.125))
      ))
    (pad 23 smd roundrect (at 0.9 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /CHARGE_STAT))
    (pad 24 smd roundrect (at 0.45 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /DC_SENSE))
    (pad 25 smd roundrect (at 0 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /RST))
    (pad 26 smd roundrect (at -0.45 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /DIP1))
    (pad 27 smd roundrect (at -0.9 -1.95 180) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /DIP2))
    (pad 28 smd custom (at -1.35 -1.95 180) (size 0.179289 0.179289) (layers F.Cu F.Paste F.Mask)
      (net 39 /RA_STEP)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.0625 -0.3375) (xy 0.0625 -0.3375) (xy 0.0625 0.3375) (xy 0.000888 0.3375) (xy -0.0625 0.274112)
) (width 0.125))
      ))
    (pad 29 smd rect (at 0 0 180) (size 2.4 2.4) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad "" smd roundrect (at -0.6 -0.6 180) (size 0.97 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.6 0.6 180) (size 0.97 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.6 -0.6 180) (size 0.97 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.6 0.6 180) (size 0.97 0.97) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-4_W7.62mm (layer B.Cu) (tedit 5A02E8C5)
    (at 131.318 80.518 270)
    (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference SW1 (at 3.81 2.33 90) (layer B.SilkS))
    (fp_text value SW_DIP_x02 (at 3.81 -4.87 90) (layer B.Fab))
    (fp_text user %R (at 3.81 -1.27 90) (layer B.Fab))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /DIP1))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 7.62 -2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /DIP2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP5 (layer B.Cu) (tedit 5A14249F)
    (at 165.608 84.328 90)
    (descr "5-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 6.35 2.4 90) (layer B.SilkS))
    (fp_text value R_Network04 (at 6.35 -2.4 90) (layer B.Fab))
    (fp_text user %R (at 5.08 0 90) (layer B.Fab))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(IC6-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(IC6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(IC5-Pad5)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(IC5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 173.228 79.502 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J5 (at 1.27 2.33) (layer B.SilkS))
    (fp_text value CHASSIS_SWITCHES (at 1.27 -9.95) (layer B.Fab))
    (fp_text user %R (at 1.27 -3.81 270) (layer B.Fab))
    (pad 8 thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /SW_POWER))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /GUIDE_RATE))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /TRACK_RATE))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Multicomp:6P4Cx2 (layer B.Cu) (tedit 5FA61512)
    (at 150.1648 84.328 180)
    (fp_text reference J2 (at 0 12.7) (layer B.SilkS))
    (fp_text value 6P4Cx2 (at 0 0.5) (layer B.Fab))
    (pad "" np_thru_hole circle (at 10.7188 2.54 180) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -10.8712 2.54 180) (size 3.302 3.302) (drill 3.302) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 7.493 5.588 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 26 "Net-(D8-Pad2)"))
    (pad 7 thru_hole circle (at 6.477 7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (pad 6 thru_hole circle (at 5.461 5.588 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 23 "Net-(D6-Pad1)"))
    (pad 5 thru_hole circle (at 4.445 7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 27 "Net-(D8-Pad1)"))
    (pad 2 thru_hole circle (at -6.604 5.588 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 21 "Net-(D5-Pad1)"))
    (pad 4 thru_hole circle (at -4.572 5.588 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 24 "Net-(D7-Pad2)"))
    (pad 3 thru_hole circle (at -5.588 7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 "Net-(D5-Pad2)"))
    (pad 1 thru_hole circle (at -7.62 7.62 180) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 25 "Net-(D7-Pad1)"))
  )
  (module Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal (layer B.Cu) (tedit 5B103613)
    (at 122.428 85.598 90)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags RJ45)
    (fp_text reference J1 (at 4.445 5 90) (layer B.SilkS))
    (fp_text value 8P8C (at 4.445 -4 90) (layer B.Fab))
    (fp_text user %R (at 4.445 -2 90) (layer B.Fab))
    (pad 8 thru_hole circle (at 8.89 2.54 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 52 /JS_DEC))
    (pad 7 thru_hole circle (at 7.62 0 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 53 /ST4_RA-))
    (pad 6 thru_hole circle (at 6.35 2.54 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 54 /ST4_DEC-))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 55 /ST4_DEC+))
    (pad 4 thru_hole circle (at 3.81 2.54 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 56 /ST4_RA+))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 2.54 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 57 /JS_RA))
    (pad "" np_thru_hole circle (at -1.27 -6.35 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 -6.35 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias (layer F.Cu) (tedit 5DC5F6A3)
    (at 145.43 72.136 90)
    (descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference IC6 (at -0.254 3.16 90) (layer F.SilkS))
    (fp_text value DRV8834 (at 0 3.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd roundrect (at 0.65 0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.65 -0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.65 0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.65 -0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad 25 smd rect (at 0 0 90) (size 2.6 2.6) (layers B.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.05 1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.05 1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.05 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.05 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.05 -1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 -1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.05 -1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 smd rect (at 0 0 90) (size 2.6 2.6) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 24 smd roundrect (at -1.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(IC6-Pad24)"))
    (pad 23 smd roundrect (at -0.75 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(IC6-Pad23)"))
    (pad 22 smd roundrect (at -0.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /DEC_PWR))
    (pad 21 smd roundrect (at 0.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(IC6-Pad19)"))
    (pad 20 smd roundrect (at 0.75 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(IC6-Pad19)"))
    (pad 19 smd roundrect (at 1.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(IC6-Pad19)"))
    (pad 18 smd roundrect (at 1.9375 -1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 17 smd roundrect (at 1.9375 -0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad1)"))
    (pad 16 smd roundrect (at 1.9375 -0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 15 smd roundrect (at 1.9375 0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 14 smd roundrect (at 1.9375 0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad2)"))
    (pad 13 smd roundrect (at 1.9375 1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D4-Pad1)"))
    (pad 12 smd roundrect (at 1.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad1)"))
    (pad 11 smd roundrect (at 0.75 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 0.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -0.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /DEC_DIR))
    (pad 8 smd roundrect (at -0.75 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /DEC_STEP))
    (pad 7 smd roundrect (at -1.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(IC6-Pad7)"))
    (pad 6 smd roundrect (at -1.9375 1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D8-Pad1)"))
    (pad 5 smd roundrect (at -1.9375 0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(IC6-Pad5)"))
    (pad 4 smd roundrect (at -1.9375 0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D8-Pad2)"))
    (pad 3 smd roundrect (at -1.9375 -0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D6-Pad2)"))
    (pad 2 smd roundrect (at -1.9375 -0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(IC6-Pad2)"))
    (pad 1 smd roundrect (at -1.9375 -1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias (layer F.Cu) (tedit 5DC5F6A3)
    (at 156.1155 72.136 90)
    (descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference IC5 (at 0 3.6505 90) (layer F.SilkS))
    (fp_text value DRV8834 (at 0 3.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd roundrect (at 0.65 0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.65 -0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.65 0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.65 -0.65 90) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad 25 smd rect (at 0 0 90) (size 2.6 2.6) (layers B.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.05 1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.05 1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.05 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.05 0 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.05 -1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 -1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.05 -1.05 90) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 smd rect (at 0 0 90) (size 2.6 2.6) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 24 smd roundrect (at -1.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(IC5-Pad24)"))
    (pad 23 smd roundrect (at -0.75 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(IC5-Pad23)"))
    (pad 22 smd roundrect (at -0.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /RA_PWR))
    (pad 21 smd roundrect (at 0.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(IC5-Pad19)"))
    (pad 20 smd roundrect (at 0.75 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(IC5-Pad19)"))
    (pad 19 smd roundrect (at 1.25 -1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(IC5-Pad19)"))
    (pad 18 smd roundrect (at 1.9375 -1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 17 smd roundrect (at 1.9375 -0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C21-Pad1)"))
    (pad 16 smd roundrect (at 1.9375 -0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 15 smd roundrect (at 1.9375 0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 14 smd roundrect (at 1.9375 0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C19-Pad2)"))
    (pad 13 smd roundrect (at 1.9375 1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D3-Pad1)"))
    (pad 12 smd roundrect (at 1.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C21-Pad1)"))
    (pad 11 smd roundrect (at 0.75 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 0.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -0.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /RA_DIR))
    (pad 8 smd roundrect (at -0.75 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /RA_STEP))
    (pad 7 smd roundrect (at -1.25 1.9375 90) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(IC5-Pad7)"))
    (pad 6 smd roundrect (at -1.9375 1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D7-Pad1)"))
    (pad 5 smd roundrect (at -1.9375 0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(IC5-Pad5)"))
    (pad 4 smd roundrect (at -1.9375 0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D7-Pad2)"))
    (pad 3 smd roundrect (at -1.9375 -0.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D5-Pad2)"))
    (pad 2 smd roundrect (at -1.9375 -0.75 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(IC5-Pad2)"))
    (pad 1 smd roundrect (at -1.9375 -1.25 90) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:Texas_S-PVSON-N10_ThermalVias (layer F.Cu) (tedit 5A8E06E8)
    (at 179.324 63.246 90)
    (descr "3x3mm Body, 0.5mm Pitch, S-PVSON-N10, DRC, http://www.ti.com/lit/ds/symlink/tps61201.pdf")
    (tags "0.5 S-PVSON-N10 DRC")
    (attr smd)
    (fp_text reference IC4 (at 2.794 -0.254 180) (layer F.SilkS))
    (fp_text value TPS61202 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 11 smd rect (at 0 0 90) (size 2.3 2.8) (layers B.Cu)
      (net 1 GND))
    (pad 11 thru_hole circle (at -0.5 0.75 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at -0.5 -0.75 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0.5 -0.75 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at 0.5 0.75 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 smd oval (at 1.475 -1 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 9 smd oval (at 1.475 -0.5 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 8 smd oval (at 1.475 0 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 7 smd rect (at 1.76 0.5 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 6 smd rect (at 1.76 1 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 32 /SW_POWER) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 5 smd oval (at -1.475 1 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 4 smd rect (at -1.76 0.5 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 3 smd oval (at -1.475 0 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC4-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 2 smd rect (at -1.76 -0.5 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 1 smd rect (at -1.76 -1 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 11 smd rect (at 0 0 90) (size 1.65 2.4) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.45 0.635 90) (size 0.68 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.45 0.635 90) (size 0.68 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.45 -0.635 90) (size 0.68 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 1.63 90) (size 0.26 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.25 1.63 90) (size 0.26 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -1.63 90) (size 0.26 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 1.55 90) (size 0.28 0.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.25 1.55 90) (size 0.28 0.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -1.55 90) (size 0.28 0.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.25 -1.63 90) (size 0.26 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.25 -1.55 90) (size 0.28 0.7) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -0.45 -0.635 90) (size 0.68 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.76 -1 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 9 smd rect (at 1.76 -0.5 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 8 smd rect (at 1.76 0 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 7 smd oval (at 1.475 0.5 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 6 smd oval (at 1.475 1 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 32 /SW_POWER) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 5 smd rect (at -1.76 1 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 4 smd oval (at -1.475 0.5 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 3 smd rect (at -1.76 0 90) (size 0.28 0.28) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC4-Pad3)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 2 smd oval (at -1.475 -0.5 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (pad 1 smd oval (at -1.475 -1 90) (size 0.85 0.28) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)") (solder_mask_margin 0.07) (solder_paste_margin -0.025))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/Texas_S-PVSON-N10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 189.06 65.786)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference IC3 (at -2.878 -2.286) (layer F.SilkS))
    (fp_text value MCP73831 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC3-Pad5)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 /CHARGE_STAT))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:Texas_S-PVSON-N8_ThermalVias (layer F.Cu) (tedit 5A4A697F)
    (at 184.912 72.136 180)
    (descr "8-Lead Plastic VSON, 3x3mm Body, 0.65mm Pitch, S-PVSON-N8, http://www.ti.com/lit/ds/symlink/opa2333.pdf")
    (tags "DFN 0.65 S-PVSON-N8")
    (attr smd)
    (fp_text reference IC1 (at -3.556 0.254) (layer F.SilkS))
    (fp_text value TPS2113A (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd oval (at 1.55 -0.975 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_paste_margin -0.05))
    (pad 7 smd oval (at 1.55 -0.325 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)") (solder_paste_margin -0.05))
    (pad 6 smd rect (at 1.75 0.325 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)") (solder_paste_margin -0.05))
    (pad 5 smd rect (at 1.75 0.975 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.05))
    (pad 4 smd rect (at -1.75 0.975 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad4)") (solder_paste_margin -0.05))
    (pad 3 smd oval (at -1.55 0.325 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.05))
    (pad 2 smd rect (at -1.75 -0.325 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.05))
    (pad 1 smd rect (at -1.75 -0.975 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /MUX_STAT) (solder_paste_margin -0.05))
    (pad 9 smd rect (at 0 0 180) (size 1.65 2.4) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.45 0.625 180) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -0.45 0.625 180) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.45 -0.625 180) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -0.45 -0.625 180) (size 0.65 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.5 0.75 180) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.5 0.75 180) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.5 -0.75 180) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.5 -0.75 180) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.25) (layers *.Cu)
      (net 1 GND))
    (pad 8 smd rect (at 1.75 -0.975 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V) (solder_paste_margin -0.05))
    (pad 7 smd rect (at 1.75 -0.325 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)") (solder_paste_margin -0.05))
    (pad 6 smd oval (at 1.55 0.325 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)") (solder_paste_margin -0.05))
    (pad 5 smd oval (at 1.55 0.975 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.05))
    (pad 4 smd oval (at -1.55 0.975 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad4)") (solder_paste_margin -0.05))
    (pad 3 smd rect (at -1.75 0.325 180) (size 0.3 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.05))
    (pad 2 smd oval (at -1.55 -0.325 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_paste_margin -0.05))
    (pad 1 smd oval (at -1.55 -0.975 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /MUX_STAT) (solder_paste_margin -0.05))
    (pad 9 smd rect (at 0 0 180) (size 1.65 2.4) (layers B.Cu)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/Texas_S-PVSON-N8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer B.Cu) (tedit 5A1DBF6A)
    (at 186.69 82.296 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at -8.45 -5.75) (layer B.SilkS))
    (fp_text value BARREL_JACK (at -6.2 5.5) (layer B.Fab))
    (fp_text user %R (at -3 2.95) (layer B.Fab))
    (pad 3 thru_hole roundrect (at -3 -4.7 180) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 13 /DC_SENSE))
    (pad 2 thru_hole roundrect (at -6 0 180) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 149.86 69.85)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 2.2µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C22-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 162.293 69.088)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 2.2µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C21-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 146.304 68.072 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C20-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 157.988 67.056 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C19-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 144.005 68.326 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 3.035 0) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 155.448 66.294 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 2.794 0) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 144.005 66.802 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 3.035 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 155.435 67.818 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 2.781 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 173.228 67.043 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 3.061 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 174.752 67.056 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 176.276 67.056 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 175.514 64.77 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.778) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 125.222 69.596 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /XTAL1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 125.222 66.548 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /XTAL2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 186.182 66.04 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.594 70.866 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.286 0) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.594 72.39 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.286 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 183.896 68.58 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 184.15 74.93)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.524) (layer F.SilkS))
    (fp_text value 1µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 192.024 67.564 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 4.7µF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 116.573 68.072 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery:Battery_Clip_21700 (layer B.Cu) (tedit 5F98F533)
    (at 151.5618 61.468 180)
    (fp_text reference BT1 (at 0.4318 0) (layer B.SilkS))
    (fp_text value "LiIon 18650" (at 0 0.5) (layer B.Fab))
    (pad 2 thru_hole rect (at 38.9636 0.254 180) (size 5.207 3.302) (drill 1.8542) (layers *.Cu *.Mask B.Paste)
      (net 1 GND))
    (pad 1 thru_hole rect (at -38.9636 0 180) (size 5.207 3.302) (drill 1.8542) (layers *.Cu *.Mask B.Paste)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole rect (at 18.9738 0 180) (size 4.572 5.207) (drill 1.8542) (layers *.Cu *.Mask B.Paste)
      (net 1 GND))
    (pad 1 thru_hole rect (at -18.9738 0 180) (size 4.572 5.207) (drill 1.8542) (layers *.Cu *.Mask B.Paste)
      (net 2 "Net-(BT1-Pad1)"))
  )
  (gr_text "Texas Two Step rev. 0\nαLyraen Astronomy" (at 178.816 73.914) (layer B.SilkS))
  (gr_text - (at 141.732 61.468) (layer B.SilkS))
  (gr_text + (at 160.274 61.468) (layer B.SilkS))
  (gr_line (start 136.398 57.658) (end 166.878 57.658) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.458 57.658) (end 136.398 57.658) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 194.818 89.408) (end 108.458 89.408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 194.818 57.658) (end 194.818 89.408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.878 57.658) (end 194.818 57.658) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.458 89.408) (end 108.458 57.658) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.652 57.404) (xy 143.764 57.404) (xy 159.512 57.404) (xy 166.624 57.404) (xy 195.072 57.404)
        (xy 195.072 89.662) (xy 107.696 89.662) (xy 107.696 57.404)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.652 57.404) (xy 143.764 57.404) (xy 159.512 57.404) (xy 166.624 57.404) (xy 176.784 57.404)
        (xy 176.784 89.662) (xy 107.696 89.662) (xy 107.696 57.404)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.174 68.834) (xy 121.92 68.834) (xy 121.92 67.818) (xy 120.904 67.818) (xy 120.904 67.564)
        (xy 122.174 67.564)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.396 67.818) (xy 119.38 67.818) (xy 119.38 68.834) (xy 119.126 68.834) (xy 119.126 67.564)
        (xy 120.396 67.564)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.38 70.358) (xy 120.396 70.358) (xy 120.396 70.612) (xy 119.126 70.612) (xy 119.126 69.342)
        (xy 119.38 69.342)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.174 70.612) (xy 120.904 70.612) (xy 120.904 70.358) (xy 121.92 70.358) (xy 121.92 69.342)
        (xy 122.174 69.342)
      )
    )
  )
)
