(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 23)
    (no_connects 0)
    (area 95.349287 85.700799 178.713201 123.350001)
    (thickness 1.6)
    (drawings 13)
    (tracks 103)
    (zones 0)
    (modules 9)
    (nets 18)
  )
  (page A4)
  (title_block
    (rev 0.2)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6096)
    (via_drill 0.4064)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 /Down)
  (net 6 /Left)
  (net 7 /Right)
  (net 8 "Net-(J1-Pad5)")
  (net 9 /Up)
  (net 10 "Net-(J1-Pad9)")
  (net 11 /Fire)
  (net 12 "Net-(J2-Pad5)")
  (net 13 /aFire)
  (net 14 "Net-(J2-Pad9)")
  (net 15 "Net-(R1-Pad1)")
  (net 16 "Net-(R2-Pad3)")
  (net 17 "Net-(SW1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.3048)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Down)
    (add_net /Fire)
    (add_net /Left)
    (add_net /Right)
    (add_net /Up)
    (add_net /aFire)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad3)")
    (add_net "Net-(SW1-Pad3)")
  )
  (net_class PWR ""
    (clearance 0.2032)
    (trace_width 0.508)
    (via_dia 0.762)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (module Potentiometers:Potentiometer_Alps_RK09K_Horizontal (layer F.Cu) (tedit 58826B09)
    (at 146.05 104.1)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK09K/RK09D1130C1B.html")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single")
    (fp_text reference R2 (at 6.05 -10.15) (layer F.SilkS))
    (fp_text value 100k (at 6.05 5.15) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(R2-Pad3)"))
    (pad 2 thru_hole circle (at 0 -2.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 0 np_thru_hole circle (at 7 -6.9) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 0 np_thru_hole circle (at 7 1.9) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Potentiometers.3dshapes/Potentiometer_Alps_RK09K_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 129.58 92.71)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at -3.85 0) (layer F.SilkS))
    (fp_text value 4.7uF (at 1.25 3.81) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 137.16 92.71 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10nF (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 132.04 110.49 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 5.04 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 1.25 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:DB9M_CI (layer F.Cu) (tedit 5AE8BFB6)
    (at 119.38 101.6 90)
    (descr "Connecteur DB9 male encarte")
    (tags "CONN DB9")
    (fp_text reference J1 (at 8.89 2.54 180) (layer F.SilkS))
    (fp_text value Joy_WE (at 0 6.35 90) (layer F.SilkS))
    (pad 2 connect rect (at 2.794 2.667 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 5 /Down))
    (pad 3 connect rect (at 0 2.667 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 6 /Left))
    (pad 4 connect rect (at -2.794 2.667 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 7 /Right))
    (pad 5 connect rect (at -5.588 2.667 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 1 connect rect (at 5.588 2.667 90) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 9 /Up))
    (pad 9 connect rect (at -4.191 2.667 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 10 "Net-(J1-Pad9)"))
    (pad 8 connect rect (at -1.397 2.667 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 7 connect rect (at 1.397 2.667 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 6 connect rect (at 4.191 2.667 90) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 11 /Fire))
    (model Connect.3dshapes/DB9M_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Connectors:DB9F_CI (layer F.Cu) (tedit 5AE8BFAF)
    (at 166.37 101.6 270)
    (descr "Connecteur DB9 femelle encarte")
    (tags "CONN DB9")
    (fp_text reference J2 (at -8.89 2.54 360) (layer F.SilkS))
    (fp_text value Joy_WY (at 0 6.35 270) (layer F.SilkS))
    (pad 4 connect rect (at 2.794 2.54 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 7 /Right))
    (pad 3 connect rect (at 0 2.54 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 6 /Left))
    (pad 2 connect rect (at -2.794 2.54 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 5 /Down))
    (pad 1 connect rect (at -5.588 2.54 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 9 /Up))
    (pad 5 connect rect (at 5.588 2.54 270) (size 1.778 5.08) (layers F.Cu F.Mask)
      (net 12 "Net-(J2-Pad5)"))
    (pad 6 connect rect (at -4.191 2.54 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 13 /aFire))
    (pad 7 connect rect (at -1.397 2.54 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 1 +5V))
    (pad 8 connect rect (at 1.397 2.54 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 9 connect rect (at 4.191 2.54 270) (size 1.778 5.08) (layers B.Cu B.Mask)
      (net 14 "Net-(J2-Pad9)"))
    (model Connect.3dshapes/DB9F_CI.wrl
      (at (xyz 0 0 -0.033))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 146.05 110.49)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1k0 (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_Micro_SPST (layer F.Cu) (tedit 54BFC180)
    (at 142.24 101.6 270)
    (tags "Switch Micro SPST")
    (fp_text reference SW1 (at -5.08 0 360) (layer F.SilkS))
    (fp_text value "AutoFire ON/OFF" (at 0.025 2.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 /Fire))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 /aFire))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 "Net-(SW1-Pad3)"))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_Micro_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.33 0.33 0.33))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5AE8C11C)
    (at 129.54 105.41 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at -1.27 -2.54 180) (layer F.SilkS))
    (fp_text value NE555 (at 3.81 3.81 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(SW1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 100.885 101.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 119.38 88.9) (xy 99.535 88.9)))
    (feature2 (pts (xy 119.38 114.3) (xy 99.535 114.3)))
    (crossbar (pts (xy 102.235 114.3) (xy 102.235 88.9)))
    (arrow1a (pts (xy 102.235 88.9) (xy 102.821421 90.026504)))
    (arrow1b (pts (xy 102.235 88.9) (xy 101.648579 90.026504)))
    (arrow2a (pts (xy 102.235 114.3) (xy 102.821421 113.173496)))
    (arrow2b (pts (xy 102.235 114.3) (xy 101.648579 113.173496)))
  )
  (dimension 46.99 (width 0.3) (layer Dwgs.User)
    (gr_text "1.8500 in" (at 142.875 122) (layer Dwgs.User))
    (feature1 (pts (xy 166.37 114.3) (xy 166.37 123.35)))
    (feature2 (pts (xy 119.38 114.3) (xy 119.38 123.35)))
    (crossbar (pts (xy 119.38 120.65) (xy 166.37 120.65)))
    (arrow1a (pts (xy 166.37 120.65) (xy 165.243496 121.236421)))
    (arrow1b (pts (xy 166.37 120.65) (xy 165.243496 120.063579)))
    (arrow2a (pts (xy 119.38 120.65) (xy 120.506504 121.236421)))
    (arrow2b (pts (xy 119.38 120.65) (xy 120.506504 120.063579)))
  )
  (gr_text "Adapter \nAuto Fire" (at 146.05 92.71) (layer F.SilkS))
  (gr_line (start 166.37 114.3) (end 119.38 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 88.9) (end 166.37 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.38 88.9) (end 166.37 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.38 114.3) (end 119.38 88.9) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.38 88.9) (xy 166.37 88.9) (xy 166.37 114.3) (xy 119.38 114.3)
      )
    )
  )
)
