(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 51)
    (no_connects 1)
    (area 164.389999 93.904999 221.690001 146.760001)
    (thickness 1.6)
    (drawings 16)
    (tracks 108)
    (zones 0)
    (modules 18)
    (nets 38)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J3-Pad1)")
  (net 2 "Net-(U4-Pad2)")
  (net 3 "Net-(U4-Pad3)")
  (net 4 "Net-(U4-Pad4)")
  (net 5 "Net-(U4-Pad5)")
  (net 6 "Net-(U4-Pad7)")
  (net 7 "Net-(U4-Pad8)")
  (net 8 "Net-(J3-Pad4)")
  (net 9 "Net-(U4-Pad10)")
  (net 10 "Net-(U4-Pad11)")
  (net 11 "Net-(U4-Pad12)")
  (net 12 "Net-(U4-Pad13)")
  (net 13 "Net-(J3-Pad5)")
  (net 14 "Net-(J3-Pad7)")
  (net 15 "Net-(U4-Pad16)")
  (net 16 "Net-(J3-Pad3)")
  (net 17 "Net-(U4-Pad18)")
  (net 18 "Net-(U4-Pad19)")
  (net 19 "Net-(U4-Pad20)")
  (net 20 "Net-(U4-Pad21)")
  (net 21 "Net-(U4-Pad22)")
  (net 22 "Net-(U4-Pad23)")
  (net 23 "Net-(U4-Pad24)")
  (net 24 "Net-(U4-Pad25)")
  (net 25 "Net-(U4-Pad26)")
  (net 26 "Net-(U4-Pad27)")
  (net 27 "Net-(U4-Pad28)")
  (net 28 "Net-(U4-Pad29)")
  (net 29 "Net-(U4-Pad30)")
  (net 30 GND)
  (net 31 "Net-(C5-Pad1)")
  (net 32 "Net-(U4-Pad33)")
  (net 33 "Net-(J3-Pad6)")
  (net 34 "Net-(C1-Pad1)")
  (net 35 /+15V)
  (net 36 /+3.3V)
  (net 37 /+1.8V)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.381)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+1.8V)
    (add_net /+15V)
    (add_net /+3.3V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad19)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad20)")
    (add_net "Net-(U4-Pad21)")
    (add_net "Net-(U4-Pad22)")
    (add_net "Net-(U4-Pad23)")
    (add_net "Net-(U4-Pad24)")
    (add_net "Net-(U4-Pad25)")
    (add_net "Net-(U4-Pad26)")
    (add_net "Net-(U4-Pad27)")
    (add_net "Net-(U4-Pad28)")
    (add_net "Net-(U4-Pad29)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad30)")
    (add_net "Net-(U4-Pad33)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 174.244 118.09 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -1.25 -2.032 360) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 171.079594 111.020838 180)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 4.709594 2.435838 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.35 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.125 0 180) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 3.125 0 180) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 171.079594 98.320838 180)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C3 (at 4.709594 3.070838 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.35 180) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -3.125 0 180) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (pad 2 smd rect (at 3.125 0 180) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 183.565 98.320838)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C4 (at -5.765 -3.070838) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.125 0) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (pad 2 smd rect (at 3.125 0) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 184.15 118.11)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C5 (at 5.08 2.54) (layer F.SilkS))
    (fp_text value 22uF (at 0 3.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.125 0) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 3.125 0) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 195.58 116.255 270)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C6 (at 5.03 -3.175 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.35 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.125 0 270) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /+3.3V))
    (pad 2 smd rect (at 3.125 0 270) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 190.5 113.01 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.56 -1.75 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 208.28 114.885 270)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C8 (at 4.495 2.54 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.35 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.125 0 270) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 37 /+1.8V))
    (pad 2 smd rect (at 3.125 0 270) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 200.66 107.95 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 1.905 -2.54 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 167.386 116.84 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 2.032 -1.016 180) (layer F.SilkS))
    (fp_text value "POWER IN" (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 219.075 116.205)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value DDSPower (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /+3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /+1.8V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 219.075 127.635)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value SIGOUT (at 0 17.57) (layer F.Fab))
    (fp_text user %R (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad7)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 58C301F2)
    (at 217.17 104.775)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference J4 (at 2.286 5.207) (layer F.SilkS))
    (fp_text value CLK_VDD (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 37 /+1.8V))
  )
  (module Inductors_SMD:L_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 173.99 104.590838 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at 1.720838 1.905 180) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 2.6875 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58CE4E7E)
    (at 183.49 106.92)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value LM2940 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 590079C0)
    (at 193.3 102.48 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U2 (at 4.69 4.82 180) (layer F.SilkS))
    (fp_text value LF33_TO252 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (pad 3 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 /+3.3V))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (pad 2 smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (pad 2 smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (pad 2 smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2 (layer F.Cu) (tedit 590079C0)
    (at 206 102.48 90)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference U3 (at 4.69 4.185 180) (layer F.SilkS))
    (fp_text value LF18_TO252 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /+15V))
    (pad 3 smd rect (at -4.2 2.28 90) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 /+1.8V))
    (pad 2 smd rect (at 2.1 0 90) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 30 GND))
    (pad 2 smd rect (at 3.775 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (pad 2 smd rect (at 0.425 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (pad 2 smd rect (at 3.775 -1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (pad 2 smd rect (at 0.425 1.525 90) (size 3.05 2.75) (layers F.Cu F.Paste)
      (net 30 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/TO-252-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:ArduinoMicro (layer F.Cu) (tedit 5B523A25)
    (at 188.595 135.255 270)
    (fp_text reference U4 (at 4.699 21.209 360) (layer F.SilkS))
    (fp_text value ArduinoMicro (at -11.43 -17.78 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 -20.32 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 -17.78 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(U4-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -15.24 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(U4-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 -12.7 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(U4-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 -10.16 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(U4-Pad5)"))
    (pad 6 thru_hole circle (at -7.62 -7.62 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 7 thru_hole circle (at -7.62 -5.08 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(U4-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 -2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(U4-Pad8)"))
    (pad 9 thru_hole circle (at -7.62 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad4)"))
    (pad 10 thru_hole circle (at -7.62 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(U4-Pad10)"))
    (pad 11 thru_hole circle (at -7.62 5.08 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(U4-Pad11)"))
    (pad 12 thru_hole circle (at -7.62 7.62 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(U4-Pad12)"))
    (pad 13 thru_hole circle (at -7.62 10.16 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(U4-Pad13)"))
    (pad 14 thru_hole circle (at -7.62 12.7 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad5)"))
    (pad 15 thru_hole circle (at -7.62 15.24 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad7)"))
    (pad 16 thru_hole circle (at -7.62 17.78 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(U4-Pad16)"))
    (pad 17 thru_hole circle (at -7.62 20.32 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(J3-Pad3)"))
    (pad 18 thru_hole circle (at 7.62 20.32 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(U4-Pad18)"))
    (pad 19 thru_hole circle (at 7.62 17.78 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(U4-Pad19)"))
    (pad 20 thru_hole circle (at 7.62 15.24 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(U4-Pad20)"))
    (pad 21 thru_hole circle (at 7.62 12.7 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(U4-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 10.16 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(U4-Pad22)"))
    (pad 23 thru_hole circle (at 7.62 7.62 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(U4-Pad23)"))
    (pad 24 thru_hole circle (at 7.62 5.08 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(U4-Pad24)"))
    (pad 25 thru_hole circle (at 7.62 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(U4-Pad25)"))
    (pad 26 thru_hole circle (at 7.62 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(U4-Pad26)"))
    (pad 27 thru_hole circle (at 7.62 -2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U4-Pad27)"))
    (pad 28 thru_hole circle (at 7.62 -5.08 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(U4-Pad28)"))
    (pad 29 thru_hole circle (at 7.62 -7.62 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U4-Pad29)"))
    (pad 30 thru_hole circle (at 7.62 -10.16 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U4-Pad30)"))
    (pad 31 thru_hole circle (at 7.62 -12.7 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 32 thru_hole circle (at 7.62 -15.24 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(C5-Pad1)"))
    (pad 33 thru_hole circle (at 7.62 -17.78 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(U4-Pad33)"))
    (pad 34 thru_hole circle (at 7.62 -20.32 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad6)"))
  )
  (gr_text "VCC\nGND" (at 168.402 118.872 270) (layer F.SilkS))
  (gr_text CLKVDD (at 216.916 99.568) (layer F.SilkS))
  (gr_text "+3.3V\nGND\n+1.8V" (at 217.17 118.872) (layer F.SilkS))
  (gr_text "SDIO\nGND\nP0\nIOUP\nCSB\nSCLK\nRST" (at 217.424 135.382) (layer F.SilkS))
  (gr_text + (at 180.594 95.25) (layer F.SilkS))
  (gr_text + (at 174.498 95.25) (layer F.SilkS))
  (gr_text + (at 175.514 113.792) (layer F.SilkS))
  (gr_text + (at 180.086 120.904) (layer F.SilkS))
  (gr_text + (at 211.328 111.506) (layer F.SilkS))
  (gr_text + (at 198.628 113.03) (layer F.SilkS))
  (gr_line (start 164.465 93.98) (end 164.465 94.615) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221.615 93.98) (end 221.615 94.615) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.465 146.685) (end 164.465 94.615) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221.615 146.685) (end 164.465 146.685) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 221.615 94.615) (end 221.615 146.685) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.465 93.98) (end 221.615 93.98) (layer Edge.Cuts) (width 0.15))
  (zone (net 30) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 92.71) (xy 163.83 148.59) (xy 223.52 148.59) (xy 223.52 92.71)
      )
    )
  )
)
